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	SECTION:
	
	A 0025 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	25 HOUR / 30 DAY INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 412 MM-2 Chapters 4, 5, Pratt & Whitney PT6T MM 
NOTE: The Appendix F Airworthiness Check shall be used in conjunction with this inspection.

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0025.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 412 MP
	

	
	Chp 4
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 412 MP
	

	
	Chp 5
	

	1.5 Review Special Inspections and carry out applicable Inspections.
	
	

	
	
	

	1.6 Lubricate and service helicopter as required.
	
	

	
	
	

	1.7 Examine all inspection windows and sight glasses for cracking, crazing, and discoloration. If any of these conditions are present, the part must be removed and replaced prior to returning helicopter for service.
	
	

	
	
	

	1.8 Check oil level and replenish if required. If engine has been stationary for more than 12 hours, run affected power section for two minutes, shut down and check oil level.
	Ref. 72-00-00, ENGINE - SERVICING
	

	
	
	

	A 0025.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	

	A 0025.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Medium Helicopter Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0025.4 FUSELAGE - NOSE SECTION

	
	
	

	4.1 Nose doors for damage, corrosion, security of attachment, and for missing or damaged twist fasteners, seal for condition.
	Chp 52
	

	
	
	






	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.2 Electrical equipment for condition, corrosion, and security.
	Chp 96
	

	
	
	

	4.3 Antennas for condition and security.
	Chp 97
	

	
	
	

	A 0025.5 FUSELAGE - CABIN SECTION 

	
	
	

	5.1 Fuselage structure and compartments for condition, corrosion, water entrapment, and damage to protective finish
	Chp 53
	

	
	
	

	5.2 Tail skid for deformation and security of attachment.
	
	

	
	
	

	5.3 If installed, Emergency float reservoir pressure indicator for proper charge indication.
	
	

	
	
	

	5.4 Floats for proper stowage and condition (if installed).
	
	

	
	
	

	5.5 Antennas for damage, cleanliness, and security.
	Chp 97
	

	
	
	

	5.6 Passenger/cargo doors (and surrounding structure) for damage, corrosion, and proper operation. Window seals for condition
	Chp 52
	

	
	
	

	5.7 Instruments;
	Chp 95
	

	
	
	

	5.7.1 Instrument panel for cleanliness.
	
	

	
	
	

	5.7.2 All instrument, placards, decals, and markings for appearance and legibility.
	
	

	
	
	

	5.7.3 Check magnetic compass for condition and security.
	
	

	
	
	

	5.7.4 All compass cards for validity.
	
	

	
	
	

	5.8 Avionics and electrical equipment;
	Chp 96/97
	

	
	
	

	5.8.1 Pedestal mounted avionics/electrical equipment for condition, cleanliness, and security.
	
	

	
	
	

	5.8.2 Overhead console for condition, cleanliness, and security.
	
	

	
	
	

	5.9 Main rotor transmission;
	Chp 63
	

	
	
	

	5.9.1 Cases for damage, corrosion, condition, and evidence of leakage.
	
	

	
	
	

	5.9.2 Accessories for condition, corrosion, damage, and security of attachment.
	
	

	
	
	






	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.10 External oil lines and hoses for condition, damage, chafing and leaks. Pay particular attention to the lines running aft of the thermostatic relief valve.
	
	

	
	
	

	5.11 Transmission mount dust boots for condition.
	
	

	
	
	

	5.12 Flight control tubes for condition, corrosion, and security.
	
	

	
	
	

	A 0025.6  FUSELAGE - AFT OF CABIN LEFT AND RIGHT SIDE

	
	
	

	6.1 Avionics/electrical and heater compartment doors for condition and security of attachment. Latches for proper operation.
	Chp 52
	

	
	
	

	6.2 Fuselage structure;
	Chp 53
	

	
	
	

	6.2.1 Engine decks for condition and evidence of delamination.
	
	

	
	
	

	6.3 Transmission oil cooling system;
	Chp 63
	

	
	
	

	6.3.1 Oil cooler hoses and tubes for leakage, damage, chafing, and fraying.
	
	

	
	
	

	6.4 Engine oil system;
	Chp 79
	

	
	
	

	6.4.1 Oil cooler hoses and tubes for leakage, damage, chafing and fraying.
	
	

	
	
	

	6.5 Baggage compartment door for damage, proper operation, and security.
	Chp 52
	

	
	
	

	6.6 Driveshaft and intermediate gearbox covers for damage and security
	Chp 52
	

	A 0025.7 CABIN ROOF

	
	
	

	7.1 Cabin structure and cowlings/fairings for condition.
	Chp 52/53
	

	
	
	

	7.2 Rotor brake caliper switches and wiring for condition and security of attachment.
	
	

	
	
	

	7.3 Main Rotor Blades;
	Chp 62
	

	
	
	

	7.3.1 Wash main rotor blades.
	
	

	
	
	

	7.4 Main Rotor Hub;
	Chp 62
	

	
	
	

	7.4.1 Functionally check droop restraint system. 
	
	

	
	
	

	7.4.2 Check for engagement of restraint arms in lower detent of cam window. 
	
	

	
	
	

	7.4.3 Relieve load on each blade and verity lower clevis moves freely through cam window envelope. Binding and roughness in inboard clevis is not acceptable.,
	
	

	
	
	





	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0025.8 LUBRICATION

	
	Table 12-3
Lubrication Chart
	

	8.1 Lubricate the following; Do not intermix grease types. Purge until same grease appears.
	
	

	NOTE: Do not intermix grease types. Purge until same grease appears.
	
	

	8.1.1 Drive link (two places per link).
	
	

	
	
	

	8.1.2 Rephasing lever bearing (four places).
	
	

	
	
	

	8.1.3 Swashplate inner ring trunnion rod ends (two) and collective lever trunnion rod end (one)
	
	

	
	
	

	8.1.4 Collective hub and sleeve (two fittings).
	
	

	
	
	

	8.1.5 Swashplate bearings (two).
	
	

	
	
	

	8.1.6 Main rotor hub pendulum absorbers bearing assembly (eight places).
	
	

	
	
	

	8.1.7 Droop restraint arm, inboard clevis race two fittings (four places).
	
	

	
	
	

	A 0025.9 POST INSPECTION

	
	
	

	9.1 Inspect for operation and leaks.
	
	

	
	
	

	9.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	9.3 If required, complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-412-FM-1
	

	
	
	

	9.4 If required, perform Functional Check Flight if required per Bell 407 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	9.5 If required, confirm all required RII have been completed and signed off.
	
	

	
	
	

	9.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	




Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Bell 412 Continuous Airworthiness Maintenance Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – A 0025 – 25 Hour / 30 Day Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




