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	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 412 MM-2 Chapter 5-9

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0100.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.5 Review Special Inspections and carry out applicable Inspections.
	Chp 5
	

	
	
	

	A 0100.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0100.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0100.1 CABIN HEATER

	
	
	

	1.1 Operationally check cabin heater system.
	
	

	
	
	

	1.2 Check bleed air shutoff _____________________
	
	

	
	
	

	1.3 Inspect line check valve.
	
	

	
	
	

	A 0100.4 TAILBOOM

	
	
	

	4.1 Inspect vertical fin caps for cracks and/or corrosion.
	Chp 53
	

	
	
	

	4.2 Inspect interior structure (including joints, splices, longerons, attach fittings, and hardware) for condition, corrosion, damage, and cracks ____________________
	
	

	
	
	

	4.3 Inspect upper and lower tail fairings for visible damage to the exterior skin and cracks at the attachment points. If paint is missing locally or has scratches, inspect the fairing for delamination and voids with a tap hammer. Inspect fairings for loose or missing attaching hardware.
	
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.4 Inspect upper and lower strakes for visible damage, deformation, cracks at the attachment points, and loose or missing rivets.
	
	

	
	
	

	4.5 Inspect upper and lower strakes for visible damage, deformation, cracks at the attachment points, and loose or missing rivets.
	
	

	
	
	

	4.6 Check elevator attachment lugs at each end of elevator horn for cracks, corrosion, and security.
	
	

	
	
	

	4.7 Check elevator horn to elevator spar attaching bolts and surrounding joint for cracks, corrosion, and security.
	
	

	
	
	

	4.8 Check elevator control tube, support, attaching hardware, and surrounding structure, for corrosion, damage, and security.
	
	

	
	
	

	4.9 Torque check tail rotor gearbox mounting nuts by applying torque in tightening direction, do not exceed 200 inch-pounds (22.6 Nm). If any nut rotates under torque, inspect attachment hardware and tail rotor gearbox for serviceability. 
	
	

	
	
	

	4.10 Inspect the tail rotor counterweight bellcrank 212-011-705-001 retention nuts for cracks, corrosion, and security. Reapply corrosion preventive compound (C-101) if nuts are not completely covered.
	
	

	
	
	

	4.11 Torque check intermediate gearbox mounting bolts by applying torque in tightening direction, do not exceed 50 inch-pounds. If any bolt turns under torque, inspect attachment hardware and intermediate gearbox for serviceability.
	
	

	
	
	

	A 0100.5 MAIN ROTOR CONTROLS

	NOTE:  Disconnect pitch link upper rod ends from the pitch horns to determine main rotor control bearing wear.
	

	5.1 Inspect:
	

	
	

	5.1.1 Swashplate and support assembly for condition and security with special attention to gimbal ring attachment lugs.
	
	

	NOTE:  The presence of black oxide powder will require investigation to determine the cause.
	

	5.1.2 Gimble ring bearings, liners, and attaching hardware for excessive looseness and wear. Gimble ring bearing and attaching bolt axial or radial looseness shall not exceed 0.005 inch (0.127 mm) with no binding allowed.
	
	

	
	
	

	5.1.3 Trunnion bearings and attaching hardware for excessive looseness and wear. Bearings shall not exceed 0.020 inch (0.508 mm) axial looseness.
	
	

	
	
	

	5.1.4 Drive hub and rephasing levers for wear and bearing looseness.
	
	

	
	
	






	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.1.5 Drive links’ spherical bearings for axial looseness. They shall not exceed 0.007 inch (0.178 mm) radial or 0.015 inch (0.381 mm).
	
	

	
	
	

	5.1.6 Swashplate link non-elastomeric bearing for looseness. It shall not exceed 0.015 inch (0.381 mm) axial.
	
	

	
	
	

	5.1.7 Collective lever trunnion bearing for axial looseness. It shall not exceed 0.020 inch (0.508 mm).
	
	

	
	
	

	5.1.8 Pitch link’s non-elastomeric bearing for looseness.  It shall not exceed 0.007 inch (0.178 mm) radial or 0.015 inch (0.381 mm) axial.
	
	

	
	
	




Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 412 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – A 0100 – 100 Hour / 120 Day Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




