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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  ASB 412-00-100
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0102.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.5 Review Special Inspections and carry out applicable Inspections.
	Chp 5
	

	
	
	

	A 0102.2 CORROSION CONTROL

	
	
	

	2.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0102.3 TAILBOOM

	
	

	3.1 Attachment;
	

	
	

	3.1.1 Inspect fuselage and tailboom attachment components and hardware for cracks with 10X magnifying glass. Pay particular attention to interface between forward end of tailboom attachment fitting and cap angle, and main beam web area below cap angle.
	Figure 5-6
	

	
	
	

	3.2 Inspect vertical fin caps for cracks and/or corrosion.
	Chp 53
	

	
	
	

	3.3 Inspect interior structure (including joints, splices, longerons, attach fittings, and hardware) for condition, corrosion, damage, and cracks.
	Chp 53
	

	
	
	

	3.4 Inspect the tail rotor counterweight bellcrank 212-011-705-001 retention nuts for cracks, corrosion, and security. Reapply corrosion preventive compound (C-101) if nuts are not completely covered
	
	

	
CAUTION

COUNTERWEIGHT BELLCRANK RETENTION NUT MS14145L6, OR ITS EQUIVALENT MS17826-6, IS DESIGNATED AS ONE TIME USE ONLY. IF MAINTENANCE ACTION REQUIRES THAT IT BE REMOVED, THE COUNTERWEIGHT BELLCRANK NUT IS TO BE DISCARDED AND  REPLACED WITH A NEW NUT. OVERTORQUING OR INCORRECT APPLICATION OF THE NUT COULD CAUSE MECHANICAL FAILURE RESULTING IN EXCESSIVE VIBRATION OR DAMAGE TO THE TAIL ROTOR BLADES.
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 412 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – A 0102 – 100 Hour / 120 Day Tailboom Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




