	MARITIME HELICOPTERS
	BELL 412 CONTINUOUS AIRWORTHINESS MAINTENANCE PROGRAM

	
	

	Page No:
	1

	Revision:
	Reissue

	Issue Date:
	11/15/20

	SECTION:
	
	B 0150 – ENGINE INSPECTION PROGRAM

	TYPE:
	
	150 HOUR INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  BHT 412 MM-9, Pratt & Whitney PT6T MM

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0150.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Pratt & Whitney 
	

	
	PT6T MM
	

	1.4 Overhaul all components that have completed published operating limits.
	Pratt & Whitney 
	

	
	PT6T MM
	

	B 0150.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings in engine area. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	BHT 412 MM
Chapter 11
	

	B 0150.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	B 0150.4 GENERAL

	
	
	

	4.1 Remove all panels, fairings, and cowlings required to satisfactorily carry out the inspection.
	
	

	
	
	

	B 0150.5 COMPONENTS

	
	

	5.1 Fuel Surge Accumulator
	

	EFFECTIVITY: Post-SB5398
	

	5.1.1 Visually inspect. Replace accumulator if pop-out indicator is extended.
	73-10-03
	

	
	
	

	5.2 Fireseals
	

	
	

	5.2.1 Cracks and security of brackets.
	
	

	
	
	

	5.3 Bleed Air Case Assembly
	

	EFFECTIVITY: Post-SB5445
	

	5.3.1 Check the orientation of the bleed air case assembly.
	72-20-00
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	

	5.4 Inlet Screen
	

	
	

	5.4.1 Cleanliness and condition of mesh.
	
	

	
	
	

	5.4.2 Perform visual inspection of the compressor air inlet screen for broken and or missing wire mesh segments and signs of brittleness.
	
	

	
	
	

	5.4.3 Check integrity of the mesh by manipulating and flexing the screen. Any deviation is a cause for replacement.
	
	

	
	
	

	5.4.4 If the inlet screen is removed, do an inspection of first-stage compressor blades.
	72-00-00 Para 9.B
ENGINE 
	

	
	INSP/CHECK
	

	5.4.5 Do a general visual inspection (GVI) of wash-ring assembly and safety wire for security and obvious damage. If any deviation is found during GVI, do an inspection of first-stage compressor blades per Para. 9.B.
	72-00-00
ENGINE
INSP/CHECK
	

	
	
	

	5.5 Oil Filter Element (10 micron)
	

	
	

	5.5.1 Remove, clean, inspect 3 oil filters on the C-Box. 
	79-20-02
	

	
	
	

	5.5.2 Reinstall filter elements.
	
	

	
	
	

	5.6 Chip Detectors
	

	
	

	5.6.1 Accessory Gearbox - 2 detectors;
	

	
	

	5.6.1.1 Clean with lint-free cloth.
	
	

	
	
	

	5.6.1.2 Measure the minimum weight lift capacity.
	
	

	
	
	

	5.6.1.3 Use a suitable ohmmeter to check the continuity of the electrical circuit when the two poles are shorted together.
	
	

	NOTE:  Reject the component if there is no continuity. Loose pins and broken potting compound are also causes for rejection.
	

	5.6.2 Reduction Gearbox - 3 detectors;
	

	
	

	5.6.2.1 Clean with lint-free cloth.
	
	

	
	
	

	5.6.2.2 Measure the minimum weight lift capacity.
	
	

	
	
	

	5.6.2.3 Use a suitable ohmmeter to check the continuity of the electrical circuit when the two poles are shorted together.
	
	

	NOTE:  Reject the component if there is no continuity. Loose pins and broken potting compound are also causes for rejection.
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0150.6 POST INSPECTION

	
	
	

	6.1 Replace or close all applicable trim panels, fairings, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	6.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-412-FM-1
	

	
	
	

	6.3 Perform Functional Check Flight if required per Bell 412 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	6.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	

	6.5 Confirm all required RII have been completed and signed off.
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 412 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – B 0150 – 150 Hour Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




