	MARITIME HELICOPTERS
	BELL 412 CONTINUOUS AIRWORTHINESS MAINTENANCE PROGRAM

	
	

	Page No:
	1

	Revision:
	Reissue

	Issue Date:
	11/15/20

	SECTION:
	
	B 0600 – ENGINE INSPECTION PROGRAM

	TYPE:
	
	600 HOUR INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  BHT 412 MM-9, Pratt & Whitney PT6T MM

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0600.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Pratt & Whitney PT6T MM
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Pratt & Whitney PT6T MM
	

	
	
	

	B 0600.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings in engine area. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	BHT 412 MM
Chapter 11
	

	B 0600.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	B 0600.4 GENERAL

	
	
	

	4.1 Remove all panels, fairings, and cowlings required to satisfactorily carry out the inspection.
	
	

	
	
	

	B 0600.5 FUEL

	
	

	5.1 Fuel Pump
	

	
	

	5.1.1 Check fuel pump coupling insitu for fretting and corrosion.
	73-10-02, 
FUEL PUMP -
MAINTENANCE PRACTICES
	

	
	
	

	5.2 Fuel Pump Filter
	

	
	

	5.2.1 Install new fuel pump filter.
	73-10-02
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	

	5.3 Fuel Nozzle Assemblies
	

	
	

	5.3.1 Functional Check
	73-10-05
	

	NOTE:  See removal/installation procedures.
	73-10-05
	

	5.3.2 For improved hot-section durability, inspect and clean fuel nozzle assemblies.
	
	

	
	
	

	5.3.3 At any fuel nozzle assembly removal, inspect gas generator case for cracks at boss welds.
	72-00-00, 10.C.
ENGIINE-
INSPECTION/
CHECK
	

	NOTE:  If in-situ cleaning is used the fuel nozzles shall be removed for inspection and functional check to coincide with 1200-hour airframe maintenance schedule.
	

	B 0600.6 POST INSPECTION

	
	
	

	6.1 Replace or close all applicable trim panels, fairings, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	6.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-412-FM-1
	

	
	
	

	6.3 Perform Functional Check Flight if required per Bell 412 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	6.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	

	6.5 Confirm all required RII have been completed and signed off.
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 412 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – B 0600 – 600 Hour Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




