



	Interval
	Inspection
	AAP Frequency

	[bookmark: _Hlk520381998]50 HR / 60 Day
	
	50 HR / 60 Day

	100 HR
	Tail Rotor dyn Balance
Eng Controls Setting Check
T/R Hub Bushing (Removal Required)
	Every 100 hours

	200 HR
	AAIP
	Every 100 hours (1/2 of insp)

	400 HR
	AAIP
	Every 100 hours (1/4 of insp)

	600 HR
	AAIP – Chp 4 Eng Ign Plugs Ops Check 
	600 HR NT

	800 HR
	AAIP
	800 HR

	900 HR
	AAIP Chp 4 AW Limitations
P/N 109-0112-05-105
	800 HR NT

	1200 HR
	AAIP Chp 4 AW Limitations
P/N 109-0112-05-107
	1200 HR NT

	1200 HR
	Fuel Pump Brushes
Hyd Pumps shaft seat on Trans
	1200 HR

	1600 HR
	Landing Skid Attach Bolts
Main D/S Inspection
Engine Mounts/Supports/Oil Cooler Fan
	1600 HR

	2000 HR
	Eng Controls Ops check MEC & MOS Chp 4
	2000 HR NT
This periodicity does not apply if the subject check is performed as part of the Engine pre-start
check and starting procedure

	2400 HR
	Xmsn support/Fitting
Swashplate Insps
Main Rotor/Hub/Blade Root/PC Links/Grip droop stop Insp’s
	2400 HR

	2400 HR AFTER 1200 HR
	T/R G/B Insp (gears)
	2400 HR AFTER 1200 HR

	3200 HR
	Fuel Tanks/Xmsn Components Tail Boom
	3200 HR

	12 Mon
	[bookmark: _GoBack]Indicating Recording System
Stdby Controls  & Indicators
	12 Mon

	200 HR / 12 Mon
	Main Trans FWD AFT LWR Fittings
	200 HR / 12 Mon

	400 HR / 24 Mon
	Swashplate duplex bearing
	400 HR / 24 Mon

	300 Landings
	Lng Gear Dampers – Chk travel
	300 Landings

	300 Landings
	Lng Gear Dampers – Chk travel (Removal Required)
	1200 Landings

	
	
	

	
	
	



