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Definitions

1. System Definitions.

System numbers are based on the Air Transport Association (ATA) Specification Number 100 and items are numbered sequentially.

a.
"Item" (Column 1) means the equipment, system, component, or function listed in the "Item" column. Repair interval categories (A, B, C, and D) are listed on right side of column 1. Repair intervals are described in definition 22.

b.
"Number Installed" (Column 2) is the number (quantity) of items normally installed in the aircraft. This number represents the aircraft configuration considered in developing this MMEL. Should the number be a variable (e.g., passenger cabin items) a number is not required.

c.
"Number Required for Dispatch" (Column 3) is the minimum number (quantity) of items required for operation provided the conditions specified in Column 4 are met.

NOTE:    Where the MMEL shows a variable number required for dispatch, the MEL must reflect the actual number required for dispatch or an alternate means of configuration control approved by the Administrator.

d.
"Remarks or Exceptions" (Column 4) in this column includes a statement either prohibiting or permitting operation with a specific number of items inoperative, provisos (conditions and limitations) for such operation, and appropriate notes.

e.
A vertical bar (change bar) in the margin indicates a change, addition or deletion in the adjacent text for the current revision of that page only. The change bar is dropped at the next revision of that page.

2.
"Airplane/Rotorcraft Flight Manual" (AFM/RFM) is the document required for type certification and approved by the responsible FAA Aircraft Certification Office. The FAA approved AFM/RFM for the specific aircraft is listed on the applicable Type Certificate Data Sheet.

3.
"As required by FAR" means that the listed item is subject to certain provisions (restrictive or permissive) expressed in the Federal Aviation Regulations operating rules. The number of items required by the FAR must be operative. When the listed item is not required by FAR it may be inoperative for time specified by repair category. The term “14 CFR” may be substituted for “FAR” in MMELs or operator MELs.

4.
Each inoperative item must be placarded to inform and remind the crewmembers and maintenance personnel of the equipment condition.

NOTE:   To the extent practical, placards should be located adjacent to the control or indicator for the item affected; however, unless otherwise specified, placard wording and location will be determined by the operator.

5.
"-" symbol in Column 2 and/or Column 3 indicates a variable number (quantity) of the item installed.

6.
"Deleted" in the remarks column after a sequence item indicates that the item was previously listed but is now required to be operative if installed in the aircraft.

7. 
As used in MMELs, "ER" refers to Extended Operations (ETOPS) of an airplane with operational approval to conduct ETOPS in accordance with the applicable regulations.

8.
"Federal Aviation Regulations" (FAR) means the applicable portions of the Federal Aviation Act and Federal Aviation Regulations.

9.
"Flight Day" means a 24 hour period (from midnight to midnight) either Universal Coordinated Time (UCT) or local time, as established by the operator, during which at least one flight is initiated for the affected aircraft.
10.
"Icing Conditions" means an atmospheric environment that may cause ice to form on the aircraft (structural) or in the engine(s) (induction).

11.
Alphabetical symbol in Column 4 indicates a proviso (condition or limitation) that must be complied with for operation with the listed item inoperative.

12.
"Inoperative" means a system and/or component malfunction to the extent that it does not accomplish its intended purpose and/or is not consistently functioning normally within its approved operating limit(s) or tolerance(s).

13.
"Notes:" in Column 4 provides additional information for crewmember or maintenance consideration. Notes are used to identify applicable material which is intended to assist with compliance, but do not relieve the operator of the responsibility for compliance with all applicable requirements. Notes are not a part of the provisos.

14.
Inoperative components of an inoperative system: Inoperative items which are components of a system which is inoperative are usually considered components directly associated with and having no other function than to support that system. (Warning/caution systems associated with the inoperative system must be operative unless relief is specifically authorized per the MMEL).

15.
"(M)" symbol indicates a requirement for a specific maintenance procedure which must be accomplished prior to operation with the listed item inoperative. Normally these procedures are accomplished by maintenance personnel; however, other personnel may be qualified and authorized to perform certain functions. Procedures requiring specialized knowledge or skill, or requiring the use of tools or test equipment should be accomplished by maintenance personnel. The satisfactory accomplishment of all maintenance procedures, regardless of who performs them, is the responsibility of the operator. Appropriate procedures are required to be published as part of the operator's manual or MEL.

16.
"(O)" symbol indicates a requirement for a specific operations procedure which must be accomplished in planning for and/or operating with the listed item inoperative. Normally these procedures are accomplished by the flight crew; however, other personnel may be qualified and authorized to perform certain functions. The satisfactory accomplishment of all procedures, regardless of who performs them, is the responsibility of the operator. Appropriate procedures are required to be published as a part of the operator's manual or MEL.

NOTE: The (M) and (O) symbols are required in the operator's MEL unless otherwise authorized by the Administrator.

17.
"Deactivated" and "Secured" means that the specified component must be put into an acceptable condition for safe flight. An acceptable method of securing or deactivating will be established by the operator.

18.
"Visual Flight Rules" (VFR) is as defined in FAR Part 91. This precludes a pilot from filing an Instrument Flight Rules (IFR) flight plan.

19.
"Visual Meteorological Conditions" (VMC) means the atmospheric environment is such that would allow a flight to proceed under the visual flight rules applicable to the flight. This does not preclude operating under Instrument Flight Rules.

20.
"Visible Moisture" means an atmospheric environment containing water in any form that can be seen in natural or artificial light; for example, clouds, fog, rain, sleet, hail, or snow.

21.
"Passenger Convenience Items" Deleted see NEF #30

22.
Repair Intervals: All users of an MEL approved under FAR 121, 125, 129 and 135 must effect repairs of inoperative systems or components, deferred in accordance with the MEL, at or prior to the repair times established by the following letter designators:

Category A.  Items in this category shall be repaired within the time interval specified in the remarks column of the operator's approved MEL.  For time intervals specified in “calendar days” or "flight days," the day the malfunction was recorded in the aircraft maintenance record/logbook is excluded.  For all other time intervals (flights, flight legs, cycles, hours, etc), repair tracking begins at the point when the malfunction is deferred in accordance with the operator's approved MEL.


Category B.  Items in this category shall be repaired within three (3) consecutive calendar days (72 hours), excluding the day the malfunction was recorded in the aircraft maintenance record/logbook. For example, if it were recorded at 10 a.m. on January 26th, the three day interval would begin at midnight the 26th and end at midnight the 29th.


Category C.  Items in this category shall be repaired within ten (10) consecutive calendar days (240 hours), excluding the day the malfunction was recorded in the aircraft maintenance record/logbook. For example, if it were recorded at 10 a.m. on January 26th, the 10 day interval would begin at midnight the 26th and end at midnight February 5th.


Category D.  Items in this category shall be repaired within one hundred and twenty (120) consecutive calendar days (2880 hours), excluding the day the malfunction was recorded in the aircraft maintenance log and/or record. The letter designators are inserted adjacent to Column 2.

An operator who has the authorization to use an MEL also has the authority to approve extensions to the maximum repair interval for category B and C items provided the responsible Flight Standards District Office (FSDO) is notified within 24 hours of the MEL extension.  The operator is not authorized to extend A and D items in the MEL. Misuse of the MEL extension authority may result in the operators OpSpecs/Mspecs being amended by removing the authority for the operator to use the MEL extension authority and/or use an MEL.

23.
Electronic fault alerting system – General

New generation aircraft display system fault indications to the flight crew by use of computerized display systems. Each aircraft manufacturer has incorporated individual design philosophies in determining the data that would be represented.

The following are customized definitions (specific to each manufacturer) to help determine the level of messages affecting the aircraft's dispatch status. When preparing the MEL document, operators are to select the proper Definition No. 23 for their aircraft, if appropriate.

NO CUSTOMIZED DEFINITIONS OF FAULT ALERTING ARE APPLICABLE TO THE BELL HELICOPTER MODEL BH407 SERIES AIRCRAFT.

24.
Not Required
25.
Not Required

26.
"Excess Items" means those items that have been installed that are redundant to the requirements of the FARs.

27.
"Day of Discovery" is the calendar day an equipment/instrument malfunction was recorded in the aircraft maintenance log and or record. This day is excluded from the calendar days or flight days specified in the MMEL for the repair of an inoperative item of equipment. This provision is applicable to all MMEL items, i.e., categories "A, B, C, and D."

28.
"Considered Inoperative", as used in the provisos means that item must be treated for dispatch, taxi and flight purposes as though it were inoperative. The item shall not be used or operated until the original deferred item is repaired. Additional actions include: documenting the item on the dispatch release (if applicable), placarding, and complying with all remarks, exceptions, and related MMEL provisions, including any (M) and (O) procedures and observing the repair category.

29.
"Is not used" in the provisos, remarks or exceptions for an MMEL item may specify that another item relieved in the MMEL “is not used.” In such cases, crewmembers should not activate, actuate, or otherwise utilize that component or system under normal operations. It is not necessary for the operators to accomplish the (M) procedures associated with the item. However, operational requirements must be complied with, and an additional placard must be affixed, to the extent practical, adjacent to the control or indicator for the item that is not used to inform crewmembers that a component or system is not used under normal operations.

30.
Nonessential equipment and furnishings (NEF) are those items installed on the aircraft as part of the original type certification, supplemental type certificate, or other form of alteration that have no effect on the safe operation of flight and would not be required by the applicable certification rules or operational rules. They are those items that if inoperative, damaged or missing have no effect on the airplane’s ability to be operated safely under all operational conditions. These nonessential items may be installed in areas including, but not limited to, the passenger compartment, flight deck area, service areas, cargo areas, crew rest areas, lavatories, and galley areas. NEF items are not items already identified in the MEL or CDL of the applicable airplane. They do not include items that are functionally required to meet the certification rule or for compliance with any operational rule. Operator’s NEF process shall not provide for deferral of items within serviceable limits identified in the manufacture’s maintenance manual or operator’s approved maintenance program such as wear limits, fuel/hydraulic leak rates, oil consumption, etc. Cosmetic items that are fully serviceable but worn or soiled may be deferred under an operator’s NEF process.

31.    As used in MMELs, Heavy Maintenance Visit (HMV) is a scheduled C-check/D-check or airworthiness maintenance program inspection where the aircraft is scheduled to be out of service for 4 or more days.

Preamble

The following is applicable for authorized certificate holders operating under Federal Aviation Regulations (FAR) Parts 121, 125, 129, and 135: The FAR require that all equipment installed on an aircraft in compliance with the Airworthiness Standards and the Operating Rules must be operative. However, the Rules also permit the publication of a Minimum Equipment List (MEL) where compliance with certain equipment requirements is not necessary in the interests of safety under all operating conditions. Experience has shown that with the various levels of redundancy designed into aircraft, operation of every system or installed component may not be necessary when the remaining operative equipment can provide an acceptable level of safety. A Master Minimum Equipment List (MMEL) is developed by the FAA, with participation by the aviation industry, to improve aircraft utilization and thereby provide more convenient and economic air transportation for the public. The FAA approved MMEL includes those items of equipment related to airworthiness and operating regulations and other items of equipment which the Administrator finds may be inoperative and yet maintain an acceptable level of safety by appropriate conditions and limitations; it does not contain obviously required items such as wings, flaps, and rudders. The MMEL is the basis for development of individual operator MELs which take into consideration the operator's particular aircraft equipment configuration and operational conditions. Operator MELs, for administrative control, may include items not contained in the MMEL; however, relief for administrative control items must be approved by the Administrator. An operator's MEL may differ in format from the MMEL, but cannot be less restrictive than the MMEL. The individual operator's MEL, when approved and authorized, permits operation of the aircraft with inoperative equipment.

Equipment not required by the operation being conducted and equipment in excess of FAR requirements are included in the MEL with appropriate conditions and limitations. The MEL must not deviate from the Aircraft Flight Manual Limitations, Emergency Procedures or with Airworthiness Directives. It is important to remember that all equipment related to the airworthiness and the operating regulations of the aircraft not listed on the MMEL must be operative.

Suitable conditions and limitations in the form of placards, maintenance procedures, crew operating procedures and other restrictions as necessary are specified in the MEL to ensure that an acceptable level of safety is maintained.

The MEL is intended to permit operation with inoperative items of equipment for a period of time until repairs can be accomplished. It is important that repairs be accomplished at the earliest opportunity. In order to maintain an acceptable level of safety and reliability the MMEL establishes limitations on the duration of and conditions for operation with inoperative equipment.

The MEL provides for release of the aircraft for flight with inoperative equipment. When an item of equipment is discovered to be inoperative, it is reported by making an entry in the Aircraft Maintenance Record/Logbook as prescribed by FAR. The item is then either repaired or may be deferred per the MEL or other approved means acceptable to the Administrator prior to further operation. MEL conditions and limitations do not relieve the operator from determining that the aircraft is in condition for safe operation with items of equipment inoperative.

When these requirements are met, an Airworthiness Release, Aircraft Maintenance Record/Logbook entry, or other approved documentation is issued as prescribed by FAR. Such documentation is required prior to operation with any item of equipment inoperative. 

Operators are responsible for exercising the necessary operational control to ensure that an acceptable level of safety is maintained. When operating with multiple inoperative items, the interrelationships between those items and the effect on aircraft operation and crew workload will be considered.

Operators are to establish a controlled and sound repair program including the parts, personnel, facilities, procedures, and schedules to ensure timely repair.

WHEN USING THE MEL, COMPLIANCE WITH THE STATED INTENT OF THE PREAMBLE, DEFINITIONS, AND THE CONDITIONS AND LIMITATIONS SPECIFIED IN THE MEL IS REQUIRED.

Guidelines for (O) & (M) Procedures

The FOEB has identified a need for certain procedures to provide an adequate level of safety while providing relief for some items. Those procedures must be established by the operator. The following guidelines specify the objectives of the required procedures:

21-1
a)
(M)
Procedure to inspect heater, isolate its fuel supply and




deactivate/secure heater electrical system.


b)
(M)
Procedure to inspect shroud, ensure no leaks exist and




deactivate/secure system.


c) 
(M)
Procedure to inspect shroud, ensure no leaks exist and




deactivate/secure system.

21-2
a)
(M)
Procedure to inspect bleed air defog system, ensure no leaks




exist, and deactivate/secure system.


b)
(O)
Procedure to insure that the system has been deactivated.

21-3

(M)
Procedure to inspect air conditioner, ensure drive system is




not restricted, and deactivate/secure system.

21-4

(M)
Procedure to inspect bleed air ECU system, ensure no leaks


 

exist, and deactivate/secure the system.

23-5

(O)
Procedure for alternate communications procedures.

24-2

(M)
Procedure to inspect, disconnect auxiliary battery and secure cables.

24-3

(M)
Procedure to inspect, deactivate or remove generator/




alternator, secure cables and ensure drive system is not restricted.

24-4

(M)
Procedure to deactivate the inoperative system and drive




system is not restricted.

28-4

(O)
Procedure to verify Solenoid Drain Valve is closed.

30-1

(M)
Procedure to inspect, deactivate and secure the anti-ice System.

31-1

(O)
Alternate procedure for determining time in service.

65-1

(M)
Procedure to inspect rotor brake assembly to determine that




rotor is free and no hydraulic leaks exist.
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	21  AIR CONDITIONING
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Cabin Heating System
	
	
	
	

	
	
	
	
	
	
	

	
	a) Combustion
	C
	0
	0
	Not installed

	
	
	
	
	
	
	

	
	b) Shroud
	C
	0
	0
	Not installed

	
	
	
	
	
	
	

	
	c) Bleed Air
	C
	1
	0
	(M)
	May be inoperative provided system is deactivated / secured. Maintenance will pull and collar the Heater CB and disconnect the bleed air heater line at the engine scroll and cap the outlet with a stainless steel cap.  A leak check will be performed before return to service.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2.  Defogging System
	
	
	
	
	

	
	
	
	
	
	
	

	
	a) Bleed Air
	C
	1
	0
	(M)
	May be inoperative provided system is deactivated / secured. Maintenance will pull and collar the Heater CB and disconnect the bleed air heater line at the engine scroll and cap the outlet with a stainless steel cap.  A leak check will be performed before return to service.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	b) Other defogging systems
	C
	1
	0
	(O)
	May be inoperative provided pilot, turns DEFOG blower off and opens both front sliding windows and does not attempt a takeoff until the windshield is clear of fog / condensation.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Air Conditioner (Freon)
	D
	–
	0
	(M) May be inoperative provided:

	
	
	
	
	
	

	
	
	
	
	
	1)
	Maintenance will inspect air conditioner in accordance with manufacture’s recommendations and determine failure cause to assure no further damage will occur,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Maintenance will ensure drive system is not restricted by rotating compressor or removing belt,

	
	
	
	
	
	
	and

	
	
	
	
	
	3)
	Maintenance will deactivate system by pulling circuit breaker and securing with collar.

	
	
	
	
	
	
	

	4
	Bleed Air System - ECU
	D
	0
	0
	Not installed.
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	22  AUTO FLIGHT
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Autopilot
	C
	– 
	0
	May be inoperative provided operations do not require its 

	
	
	
	
	
	use.  Restricted to VFR only.

	
	
	
	
	
	
	

	2
	SAS
	C
	0
	0
	Not installed.

	
	
	
	
	
	
	

	3
	Force Trim System
	D
	–
	0
	May be inoperative for VFR only.
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	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	23  COMMUNICATIONS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Communications Systems: 
	
	
	
	Any in excess of those required by FAR may be inoperative provided it is not powered by the, Emergency DC Bus, Battery Bus, or the DC Transfer Bus and not required for emergency procedures.

	
	(VHF and UHF)
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	a)VHF Communications
	D
	–
	1
	One VHF Comm may be inoperative for VFR operations (except extended over water operations), provided operations are not predicated on the affected radio.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on control head.

	
	
	
	
	
	
	

	     
	b) UHF/FM Transceiver
	D
	–
	0
	May be inoperative. Place INOP placard on control head.

	
	
	
	
	
	
	

	     
	c) HF FM Transceiver
	D
	–
	0
	May be inoperative. Place INOP placard on control head.

	
	
	
	
	
	
	

	     
	d) FM Encoder
	D
	–
	0
	May be inoperative. Place INOP placard on control head.

	
	
	
	
	
	
	

	     
	e) 800 MHz Transceiver
	D
	–
	0
	May be inoperative. Place INOP placard on control head.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Cockpit/Cabin Speaker
	D
	0
	0
	Not installed.

	
	
	
	
	
	
	

	3
	Cabin ICS System
	D
	–
	0
	Any in access of those required or for non passenger carrying operations may be inoperative, provided alternate procedures are established and used.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	(O)
	Pilot shall brief the passenger(s) regarding alternate normal and emergency procedures to be used. The Pilot briefing must include any appropriate operating restrictions.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on inoperative system control head.

	
	
	
	
	
	
	

	4
	External Loud Speaker
	D
	–
	0
	May be inoperative. Place INOP placard on control head.

	
	
	
	
	
	
	

	5
	High Frequency (HF) 
	D
	0
	0
	Not installed.

	
	Communication System
	
	
	
	
	

	
	
	
	
	
	
	

	6
	Satellite Tracking System(s), 
	D
	–
	0
	May be inoperative. Place INOP placard on control head.

	
	(i.e. Blue Sky, SkyConnect
	
	
	
	
	

	
	Outerlink, etc.)
	
	
	
	
	

	
	
	
	
	
	
	

	7
	Satellite Phone (i.e. 
	D
	–
	0
	May be inoperative. Place INOP placard on control head.

	
	SkyConnect Satellite 
	
	
	
	
	

	
	Phone,etc.)
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	1
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	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	24  ELECTRICAL POWER
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Generator Caution System 
	B
	–
	0
	May be inoperative provided loadmeter is operative.

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on indicator.

	
	
	
	
	
	
	

	2
	Auxiliary Battery
	D
	–
	0
	(M) May be inoperative provided:

	
	
	
	
	
	

	
	
	
	
	
	1)
	Battery is inspected, disconnected and cables 

	
	
	
	
	
	
	secured,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Battery remains installed.

	
	
	
	
	
	
	

	
	
	D
	–
	0
	(M) May be inoperative provided

	
	
	
	
	
	

	
	
	
	
	
	1)
	Battery is inspected, then removed and cables 

	
	
	
	
	
	
	secured,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Appropriated ballast is installed.

	
	
	
	
	
	
	

	
	
	D
	–
	0
	(M) May be inoperative provided

	
	
	
	
	
	

	
	
	
	
	
	1)
	Battery is inspected, then removed and cables 

	
	
	
	
	
	
	secured,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Weight and balance is revised.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Standby Generator/Alternator
	C
	–
	0
	May be inoperative for VFR.

	
	
	
	
	
	

	
	
	
	
	
	(M) Maintenance shall:

	
	
	
	
	
	

	
	
	
	
	
	1)
	Inspect for burned or arched wires and ensure drive 

	
	
	
	
	
	
	system is not restricted by rotating compressor,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Deactivate system by pulling and collaring the circuit 

	
	
	
	
	
	
	breaker.

	
	
	
	
	
	
	or

	
	
	
	
	
	3)
	Remove starter/generator, remove mount plate, 

	
	
	
	
	
	
	install blank, cap and stow cables.

	
	
	
	
	
	
	

	4
	Starter/Generator (Twin 
	C
	0
	0
	Not applicable.

	
	engine models only)
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	25  EQUIPMENT/FURNISHINGS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Crew Member Shoulder 
	B
	–
	1
	Pilots must be operative.

	
	Harness
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Passenger Seat Belts
	C
	–
	0
	One required for each occupied seat. If belt is inoperative 

or missing, seat must be blocked and placarded.

	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Passenger Shoulder Harness
	C
	–
	0
	May be inoperative. If Shoulder Harness is inoperative or 

	
	
	
	
	
	missing, seat must be blocked and placarded.

	
	
	
	
	
	
	

	4
	Passenger Convenience 
	
	0
	0
	Relocated to Item # 25-15 Non-essential Furnishings (NEF)

	
	Item(s)
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Cargo Suspension System
	D
	0
	0
	Not installed.

	
	
	
	
	
	
	

	6
	Hoist System
	D
	0
	0
	Not installed.

	
	
	
	
	
	
	

	7
	Litter Kit
	D
	1
	0
	May be inoperative.

	
	
	
	
	
	
	

	8
	EMS Equipment
	
	
	
	
	

	
	
	
	
	
	
	

	
	a) Suction pump
	D
	1
	0
	(M)
	May be inoperative provided system is deactivated and secured. Maintenance will collar Suction Pump Circuit Breaker in the off position

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	b) 110 VAC Inverter
	D
	1
	0
	(M)
	May be inoperative provided system is deactivated and secured. Maintenance will collar the Inverter Circuit Breaker in the off position

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	c) Medical Oxygen System
	D
	1
	0
	(O)
	or (M) May be inoperative provided:        

	
	
	
	
	
	
	Pilot or Mechanic ensures the system is turned off

	
	
	
	
	
	
	and verifies no pressure at outlet.

	
	
	
	
	
	

	
	d) Medical Oxygen Quantity
	D
	1
	0
	(M)
	May be inoperative provided:     

	
	Indicator
	
	
	
	
	Mechanic weighs oxygen container to determine

	
	
	
	
	
	
	content quantity.      

	
	
	
	
	
	
	

	
	e) Medical Air Pressure System     
	D
	1
	0
	(M)
	May be inoperative provided:     

	
	
	
	
	
	
	Mechanic pulls and collars circuit breaker.           

	
	
	
	
	
	
	Place INOP placard on outlet.                          

	
	
	
	
	
	
	

	
	f) Monitor Mount(s)
	D
	–
	0
	May be inoperative. Place INOP placard on Mount(s).

	
	
	
	
	
	
	

	
	g) Attendants Audio Amplifier /
	D
	–
	0
	May be inoperative provided oral communications are 

	
	  Audio Panel
	
	
	
	utilized.  Place INOP placard on affected control head.
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	25  EQUIPMENT/FURNISHINGS
	
	
	
	
	

	
	
	
	
	
	
	

	9
	Emergency Locator 
	
	
	
	

	
	Transmitter (ELT)
	
	
	
	

	
	
	
	
	
	

	
	a) Survival Type ELTs
	D
	–
	​–
	Not installed.

	
	
	
	
	
	

	
	b) Fixed ELTs
	A
	​–
	0
	May be inoperative provided

	
	
	
	
	
	1)
	System is deactivated,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Repairs are made within 90 days.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Remove ELT and placard “ELT not installed” in 

	
	
	
	
	
	
	plain view of flight crew.

	
	
	
	
	
	
	

	
	
	A
	​–
	0
	May be missing provided repairs are made within 90 days.

	
	
	
	
	
	

	
	
	D
	–
	1
	Any in excess of one (1) ELT may be inoperative or missing.

	
	
	
	
	
	Placard “INOP” next to remote switch.

	
	
	
	
	
	
	

	10
	Flotation Inflation System
	D
	0
	0
	Not installed.

	
	
	
	
	
	
	

	11
	Sonic Locator
	D
	0
	0
	Not installed.

	
	
	
	
	
	
	

	12
	Forward Looking Infra Red 
	D
	0
	0
	Not installed.

	
	(FLIR)
	
	
	
	

	
	
	
	
	
	
	

	13
	Auxiliary Fuel and/or lubricant 
	D
	0
	0
	Not installed.

	
	heating system
	
	
	
	

	
	
	
	
	
	
	

	14
	Electronic News Gathering 
	D
	0
	0
	Not installed.

	
	(ENG) Equipment
	
	
	
	

	
	
	
	
	
	
	

	15
	Non-essential Furnishings (NEF)
	
	–
	0
	May be inoperative, damaged, or missing provided that the item(s) is deferred in accordance with the operator's NEF deferral program. The NEF program, procedures, and processes are outlined in the Air Methods Operations Manual. 

(M) and/or (O) procedures, if required, must be available to the flight crew and included in the operator's appropriate document.

NOTE: EXTERIOR LAVATORY DOOR ASH TRAYS ARE NOT CONSIDERED NEF ITEMS.
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	26  FIRE PROTECTION
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Engine Fire Warning System 
	B
	0
	0
	Not applicable.

	
	(Twin engine models only)
	
	
	
	

	
	
	
	
	
	
	

	2
	Portable Fire Extinguisher
	D
	–
	1
	Any in excess of those required by FAR may be inoperative 

	
	
	
	
	
	or missing provided:

	
	
	
	
	
	1)
	The inoperative fire extinguisher is tagged inoperative, removed from the installed location, and placed out of sight so it cannot be mistaken for a functional unit,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Required distribution is maintained.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Engine Fire Extinguishing 
	B
	0
	0
	Not Installed

	
	System
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	 2. NUMBER INSTALLED
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	28  FUEL
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Fuel Quantity Gauge
	
	
	
	Deleted

	
	
	
	
	
	
	

	2
	Auxiliary Fuel Tank
	D
	0
	0
	Not installed.

	
	
	
	
	
	
	

	3
	Fuel Low Warning Caution Light 
System
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	(206A and 206B only)
	
	
	
	Deleted

	
	
	
	
	
	
	

	
	(206L series only)
	
	
	
	Deleted

	
	
	
	
	
	
	

	4
	Solenoid Drain Valve System
	D
	2
	0
	May be inoperative.

	
	
	
	
	
	

	
	
	
	
	
	(O)
	Prior to flight, crew shall perform a visual check to verify the manual drain valve is closed. 

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Fuel Boost Pump

(Twin engine models only)
	B
	0
	0
	Not applicable.

	
	
	
	
	
	

	
	
	
	
	
	
	

	6
	Fuel Flow Indicator (Twin engine 
	B
	0
	0
	Not applicable.

	
	models only)
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	30  ICE AND RAIN PROTECTION
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Engine Anti-ice System
	B
	1
	0
	May be inoperative provided:

	
	
	
	
	
	

	
	
	
	
	
	1)
	Known and forecast conditions for flight are at ambient temperatures above +4° C with no visible moisture,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Operations are conducted in accordance with RFM.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Maintenance will inspect, then install a stainless steel plug in the solenoid valve and collar the engine anti-ice circuit breaker.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard next to switch.                          

	
	
	
	
	
	

	
	
	
	
	
	

	2
	Pitot Heater
	C
	1
	0
	May be inoperative provided OAT is above 0° C.

	
	
	
	
	
	
	

	
	
	C
	1
	0
	May be inoperative provided Operations are not conducted 

	
	
	
	
	
	in visible moisture.

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on next to switch                        

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Automatic Engine Reignition 
	C
	0
	0
	Not installed.

	
	kit (A, B, and L models only)
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	4
	Engine Continuous Ignition 
	B
	2
	0
	May be inoperative provided:

	
	System
	
	
	
	

	
	
	
	
	
	1)
	Known and forecast conditions for flight is at ambient temperatures above 4.4o C (40o F) with no visible Moisture,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Operations are conducted in accordance with RFM.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Engine Anti-Ice Lights
	B
	2
	0
	May be inoperative provided:

	
	
	
	
	
	

	
	
	
	
	
	1)
	Known and forecast conditions for flight is at ambient temperatures above 4.4o C (40o F) with no visible Moisture,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Operations are conducted in accordance with RFM.
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	31  INDICATING/RECORDING SYSTEMS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Clock, Displaying Hours, Minutes 
and Seconds, with Sweep

Second Pointer or Electric Digital
Clock.
	C
	1 
	0
	May be inoperative for VFR.  For IFR, one (1) operative clock displaying hours, minutes and seconds with sweep second pointer or an electric digital clock must be located on the instrument panel in a position that makes it plainly visible to, and usable by any pilot at the pilot's station.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Hour Meter
	C
	–
	0
	May be inoperative provided 

	
	
	
	
	
	

	
	
	
	
	
	(O)
	An alternate means is utilized for recording time in service,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	(O)
	All flight time with hour meter inoperative will be

recorded and entered in the aircraft logbook,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	(M)
	Adjustments to maintenance time will be recorded in the logbook when the hour meter is repaired.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on meter.                          

	
	
	
	
	
	
	

	3
	Elapsed Timer
	D
	–
	0
	May be inoperative.

	
	
	
	
	
	
	

	4
	Aircraft/Engine Monitoring 
	D
	0
	0
	Not installed.

	
	System.
	
	
	
	

	
	
	
	
	
	
	

	5
	Voice Warning System
	D
	0
	0
	Not installed.

	
	
	
	
	
	
	

	6
	Warning Horn Mute System
	
	
	
	
	

	
	
	
	
	
	
	

	
	a) 206B and 206L models only
	D
	0
	0
	Not applicable.

	
	
	
	
	
	
	

	
	b) All other models
	D
	–
	0
	May be inoperative.

	
	
	
	
	
	
	

	7
	Vibration Monitoring System
	D
	0
	0
	Not installed.

	
	
	
	
	
	
	

	8
	Flight Event Recorder (Alerts)
	A
	–
	0
	May be inoperative for 10 (ten) flight days.
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	33  LIGHTS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Position Light System
	C
	1
	0
	May be inoperative for day. Place INOP placard on switch.                          

	
	
	
	
	
	
	

	2
	Anti-Collision Light System
	C
	1
	0
	May be inoperative for day. Place INOP placard on switch.                          

	
	
	
	
	
	
	

	3
	Landing Light(s)
	C
	2
	0
	One or both may be inoperative for day.  One may be inoperative for night.  Both may be inoperative for night provided that a searchlight is installed and operating.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch(s).                          

	
	
	
	
	
	
	

	4
	System Cockpit Instrument 

Lighting
	B
	–
	0
	May be inoperative provided:

	
	
	
	
	
	

	
	
	
	
	
	1)
	Sufficient lighting is available to make each required instrument, control and other device for which it is provided easily readable,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Direct rays and reflections do not impair visibility

either inside or outside the aircraft,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	3)
	Lighting intensity can be controlled or preset to a 

satisfactory level for the expected flight condition,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	4)
	Lighting configuration at dispatch is acceptable to 

the pilot.

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch.                          

	
	
	
	
	
	

	5
	Cabin Lighting System
	C
	1
	0
	May be inoperative. Place INOP placard on switch.                          

	
	
	
	
	
	
	

	6
	Cockpit Utility Light
	C
	1
	0
	May be inoperative. Place INOP placard on switch.                          

	
	
	
	
	
	
	

	7
	Strobe Light System
	C
	–
	0
	May be inoperative. Place INOP placard on switch.                          

	
	
	
	
	
	
	

	8
	Taxi Light
	C
	0
	0
	Not installed.

	
	
	
	
	
	
	

	9
	Search Light
	C
	–
	0
	May be inoperative. Place INOP placard on switch.                          

	
	
	
	
	
	
	

	10
	External Utility Lights
	C
	–
	0
	May be inoperative. Place INOP placard on switch.                          
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	33  LIGHTS
	
	
	
	
	

	
	
	
	
	
	
	

	11
	NVG compatible Lighting 
	C
	–
	0
	Unaided operation (without NVG’s) may be permitted with 

inoperative NVG supplemental lights; cracked or missing

filters, provided the remaining lights are:

	
	System
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	1)
	Sufficient to clearly illuminate all required instruments, controls, and other devices for which they are provided,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Positioned so that direct rays are shielded from flight 

crew-members eyes,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	3)
	Lighting configuration and intensity is acceptable to 

the flight crew.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	




	MARITIME HELICOPTERS
	
	
	
	
	

	
	
	
	
	
	
	MINIMUM EQUIPMENT LIST

	
	
	
	
	
	
	

	AIRCRAFT:
	
	
	
	
	
	REVISION NO: 17
	PAGE:

	407 SERIES
	
	
	
	
	

	
	
	
	
	
	
	DATE: 08/05/10
	34-1

	
	
	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	34  NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Gyroscopic Rate of Turn with 
	C
	–
	0
	May be inoperative. Place INOP placard on instrument.                          

	
	Slip Indicator
	
	
	
	

	
	
	
	
	
	
	

	2
	Gyroscopic Bank and Pitch 
	C
	–
	0
	Required for NVG operations. May be inoperative for Day, 

Night VFR use. Place INOP placard on indicator.                          

	
	Indicator
	
	
	
	

	
	
	
	
	
	
	

	3
	Directional Gyro
	C
	1
	0
	 May be inoperative for Day, Night VFR use, except for:

	
	
	
	
	
	

	
	
	
	
	
	1)
	VFR over-the-top conditions.

	
	
	
	
	
	
	or

	
	
	
	
	
	2)
	May be inoperative provided the Free mode is functioning.

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	(O)
	The pilot MUST align the DG and wet compass at intervals not to exceed 10 Minutes.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on instrument.                          

	
	
	
	
	
	
	

	4
	Vertical Speed Indicator
	C
	1
	0
	May be inoperative for VFR operations.

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on instrument.                          

	
	
	
	
	
	
	

	5
	ATC Transponder 
	C
	–
	0
	May be inoperative provided;

	
	
	
	
	
	
	

	
	
	
	
	
	1)
	Enroute operations do not require its use,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Prior to flight, approval is obtained from ATC facilities

	
	
	
	
	
	
	having jurisdiction over the planned route of flight.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	D
	–
	1
	Any in excess of one (1) may be inoperative.

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on control head.                          
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	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	34  NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	6
	Navigation Equipment
	
	
	
	
	

	
	
	
	
	
	
	

	
	a) VOR Navigation System.
	C
	–
	0
	One navigation system must be operative for VFR over the top or night VFR in which case the VOR system(s) may be inoperative provided at least one navigation system (ADF, GPS, and RNAV) is operative.  Two navigation systems must be operative when conducting extended over water operations in which case the VOR(s) may be inoperative provided two of the following navigation systems are operative: (ADF, GPS, RNAV)

	
	
	
	
	
	
	

	
	b) RNAV Navigation System.
	C
	–
	0
	One navigation system must be operative for VFR over the top or night VFR in which case the RNAV system(s) may be inoperative provided at least one navigation system (ADF, GPS, and VOR) is operative. Two navigation systems must be operative when conducting extended over water operations in which case the RNAV(s) may be inoperative provided two of the following navigation systems are operative: (ADF, GPS, VOR)

	
	
	
	
	
	
	

	
	c) ADF Navigation System.
	C
	–
	0
	One navigation system must be operative for VFR over the top or night VFR in which case the ADF system(s) may be inoperative provided at least one navigation system (VOR, GPS, and RNAV) is operative.  Two navigation systems must be operative when conducting extended over water operations in which case the ADF(s) may be inoperative provided two of the following navigation systems are operative: (VOR, GPS, RNAV)

	
	
	
	
	
	
	

	
	d) GPS System.
	C
	–
	0
	One navigation system must be operative for VFR over the top or night VFR in which case the GPS system(s) may be inoperative provided at least one navigation system (ADF, VOR, and RNAV) is operative.  Two navigation systems must be operative when conducting extended over water operations in which case the GPS(s) may be inoperative provided two of the Following navigation systems are operative (ADF, VOR, RNAV)

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on affected system control head.                          

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


	MARITIME HELICOPTERS
	
	
	
	
	

	
	
	
	
	
	
	MINIMUM EQUIPMENT LIST

	
	
	
	
	
	
	

	AIRCRAFT:
	
	
	
	
	
	REVISION NO: 17
	PAGE:

	407 SERIES
	
	
	
	
	

	
	
	
	
	
	
	DATE: 08/05/10
	34-3

	
	
	1
	 2. NUMBER INSTALLED
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	34  NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	7
	Weather Radar/Thunderstorm 
	
	
	
	
	

	
	Detection Equipment
	
	
	
	
	

	
	
	
	
	
	
	

	
	a) Stormscope
	C
	–
	0
	May be inoperative. Place INOP placard on display.

	
	
	
	
	
	
	

	
	b) Cockpit Weather Displays
	C
	–
	0
	May be inoperative. Place INOP placard on display.

	
	
	
	
	
	
	

	8
	Marker Beacon
	C
	–
	0
	May be inoperative provided an instrument approach is not 

predicated on its use.

	
	
	
	
	
	

	
	
	
	
	
	
	

	9
	Flight Director
	C
	0
	0
	Not installed.

	
	
	
	
	
	
	

	10
	Radar Altimeter
	C
	1
	0
	May be inoperative for day VFR use.

	
	
	
	
	
	

	
	
	
	
	
	(O)
	Required for NVG Operations or night VFR

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on instrument.

	
	
	
	
	
	

	11
	Altitude Encoding System
	C
	–
	0
	May be inoperative, except for operations in the following:

	
	
	
	
	
	
	

	
	
	
	
	
	1)
	Enroute operations do not require its use,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Prior to flight, approval is obtained from ATC facilities
having jurisdiction over the planned route of flight.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	D
	–
	1
	Any in excess of one (1) may be inoperative.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	12
	DME
	D
	–
	0
	Not required for flights conducted below FL240 

	
	
	
	
	
	

	
	
	
	
	
	
	

	13
	RMI
	C
	–
	0
	Not installed. 

	
	
	
	
	
	
	

	14
	Standby Attitude Indicator
	C
	–
	0
	May be inoperative. Place INOP placard on instrument.

	
	
	
	
	
	
	

	15
	OAT/Free Air
	C
	–
	1
	May be inoperative provided approved alternate onboard 

OAT source is installed and operative.

	
	
	
	
	
	

	
	
	
	
	
	
	

	16
	Airspeed Indicator
	C
	–
	1
	One required at pilot’s station.

	
	
	
	
	
	
	

	17
	Altimeter
	C
	–
	1
	One required at pilot’s station.

	
	
	
	
	
	
	

	18
	Deleted
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	34  NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	19
	Traffic Alert / Advisory Systems 
	B
	–
	0
	May be inoperative provided:

	
	(TAS, TCAS I)
	
	
	
	

	
	
	
	
	
	1)
	System is deactivated and secured,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Enroute or approach procedures do not require its use.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Secure system by pulling and collaring circuit breaker.

	
	
	
	
	
	
	

	
	
	C
	–
	0
	May be inoperative provided:

	
	
	
	
	
	

	
	
	
	
	
	1)
	Aircraft is not operated with a passenger configuration     
of 10 or more seats, excluding any pilot,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	System is deactivated and secured,

	
	
	
	
	
	
	and

	
	
	
	
	
	3)
	Enroute or approach procedures do not require its use.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Secure system by pulling and collaring circuit breaker.

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on Unit.

	
	
	
	
	
	

	
	a) Traffic Alert Display System(s)
	C
	–
	–
	Display(s) may be inoperable provided: 

	
	  (TAS, TCAS I)
	
	
	
	

	
	               
	
	
	
	1)
	Other Traffic Alert Display(s) are functioning properly
and displaying correct information. 

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	2)
	TA audio functions are operative. (TCAS I Only)

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on display.

	
	
	
	
	
	
	

	
	b) Audio Functions (TCAS I)
	B
	–
	–
	May be inoperative provided enroute or approach procedures do not require the use of TCAS I.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	(M)
	Secure system by pulling and collaring circuit breaker.

	
	
	
	
	
	

	
	
	
	
	
	

	20
	Helicopter Ground Proximity
	C
	–
	0
	May be inoperative for Day. May be inoperative at night 

	
	Warning System/Terrain
	
	
	
	provided:

	
	Awareness and Warning
	
	
	
	
	

	
	System. TAWS/GPWS
	
	
	
	(O)
	At night, flight crew shall conduct enroute segment of the flight at 500 feet or above any obstacle on the route of flight or circumnavigate obstacle at a safe distance.
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	35  OXYGEN
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Oxygen System and Masks 

(Crew and Passengers)
	D
	–
	0
	May be operative for all flights below 10,000 feet MSL
provided;

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	1)
	Oxygen is not required for medical use by passengers or an alternate source of Medical Oxygen is available.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	Secure the onboard Medical Oxygen Secured by closing the Bottle Valve.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	For flights conducted above 10,000 feet MSL;

	
	
	
	
	
	

	
	
	
	
	
	1)
	Corresponding passenger seat is blocked and placarded "DO NOT OCCUPY" on seat belt in plain view,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Ensure affected mask does not permit flow when

	
	
	
	
	
	
	cabin oxygen system is activated.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Ensure that the mask safety flow pin will NOT be removed from the manifold by securing the flow pin with Safety wire (do not wrap safety wire around any O2 lines), or remove lanyard from safety flow pin. This will ensure that oxygen flow is blocked, and is not permitted.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	(O)
	If the flight is conducted between 10,000 feet through 12,000 feet MSL for more than 30 minutes or any time above 12,000, the pilot must use supplemental oxygen. If the flight is conducted between 10,000 feet through 15,000 feet MSL for more than 30 minutes or any time above 15,000 feet MSL, all occupants other than pilot must have oxygen available.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Placard INOP placard on mask.
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	52  DOORS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Litter Door Caution System
	C
	1
	0
	May be inoperative provided litter is secured, and a visual check verifies that the door is closed, and latched, prior to flight.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on caution light.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Baggage Door Caution Light
	C
	1
	0
	May be inoperative provided all baggage is secured, and a visual check verifies that the door is closed, and latched, prior to flight.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on caution light.
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	1
	 2. NUMBER INSTALLED

	SYSTEM &
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	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	65  ROTORS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Rotor Brake System
	C
	1
	0
	May be inoperative;

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Maintenance shall;

1) Safety the handle in the off position to prevent inadvertent use of the rotor brake, 

                                    and

2) Ensure the brake pads are not contacting the rotor brake disk, 
                                    and

3) Perform a visual inspection to ensure that no hydraulic leaks exist,

                                    and

4) Ensure that the rotor is free.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard next to Rotor Brake.
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	71  POWERPLANT
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	1
	Engine Air Particle Separator/Particle 
	
	
	
	

	
	Purge System
	
	
	
	

	
	
	
	
	
	
	

	
	a) 206L-1 and twin engine 
	C
	0
	0
	Not Applicable

	
	    models
	
	
	
	

	
	
	
	
	
	
	

	
	b) 206L-3, and L-4 models only
	C
	1
	0
	May be inoperative provided operations are conducted in 

	
	
	
	
	
	accordance with the RFM.

	
	
	
	
	
	
	

	2
	Water Alcohol Injection System
	D
	0
	0
	Not installed.

	
	
	
	
	
	
	

	3
	Engine Fire Detection System
	C
	0
	0
	Not installed.
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	73  ENGINE FUEL & CONTROL
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Engine Trim System (Twin 

Engine models only)
	C
	0
	0
	Not applicable.
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	77  ENGINE INDICATING
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Tachometer, Dual Indicating  
	
	
	
	Deleted

	
	(N2/Nr) (Single engine models)
	
	
	
	

	
	
	
	
	
	

	2
	Deleted.
	
	
	
	
	

	
	
	
	
	
	
	

	3
	TOT Light System
	
	
	
	
	

	
	
	
	
	
	
	

	
	a) Single Engine Models
	C
	1
	0
	May be inoperative. Place inop placard near indicator.

	
	
	
	
	
	
	

	
	b) Twin Engine Models
	B
	0
	0
	Not applicable.

	
	
	
	
	
	
	

	4
	Engine N1 Tach (Twin Engine 
	B
	0
	0
	Not applicable.

	
	models only)
	
	
	
	

	
	
	
	
	
	
	

	5
	Engine Low RPM Warning 
	B
	0
	0
	Not applicable.

	
	System (Twin Engine models
	
	
	
	

	
	only)
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	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	79  ENGINE OIL
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Engine Scavenge Filter By-pass Indicator
	D
	1
	0
	May be inoperative provided by-pass indicator did not extend in conjunction with engine chip light.

	
	
	
	
	
	
	

	
	
	
	
	
	Place inop placard near indicator.

	
	
	
	
	
	
	

	ITEMS 2 THROUGH 6 
APPLY ONLY TO TWIN ENGINE
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Oil Temperature Indicator
	B
	0
	0
	Not applicable.

	
	
	
	
	
	
	

	3
	Oil Pressure Indicator
	B
	0
	0
	Not applicable.

	
	
	
	
	
	
	

	4
	Engine Chip Detector
	B
	0
	0
	Not applicable.

	
	
	
	
	
	
	

	5
	High Oil Temperature Caution 
	B
	0
	0
	Not applicable.

	
	System
	
	
	
	

	
	
	
	
	
	
	

	6
	Low Oil Pressure Caution 
	B
	0
	0
	Not applicable.

	
	System
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	7
	Benz Airborne System
	C
	0
	0
	Not installed.

	
	Monitoring System (Auto-Fault)
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	


