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Definitions

1. 	System Definitions.


2.	Not Required


3. 	ATA System Page. The ATA system page is divided into four (4) columns and contains: item and repair category; number installed; number required for dispatch; and remarks or exceptions.  Standard ATA categories are used.  Items are numbered sequentially.

A.  Item.  This column depicts the equipment, system, component, or function listed in the “Item” column.

B.  Repair Category.  See definition #24.

C.  Number Installed.  This column depicts the number (quantity) of instrument and equipment items normally installed in the aircraft.  This number represents the aircraft configuration considered in developing this MEL.  Should the number be a variable (e.g., fleet configuration differences, cockpit lighting items, cabin lighting items, cargo restraint components) a number is not required and the “-” symbol is used.

D.  Number Required for Dispatch.  This column depicts the minimum number (quantity) of instrument and equipment items required for operation provided the conditions specified in the “Remarks or Exceptions” column are met.  Where the MEL shows a variable number required for dispatch, the MEL must reflect the actual number required for dispatch or an alternate means of configuration control approved by the Administrator.

E.  Remarks or Exceptions.  This column may include a statement(s) either prohibiting or permitting operation with a specific number of instrument and equipment items inoperative, provisos (conditions and limitations) for such operation, and appropriate notes.

F.  Provisos.  Provisos are indicated by a number or a lower case letter in “Remarks or Exceptions”.  Provisos are conditions or limitations that must be complied with for operation with the listed instrument or equipment item inoperative.

G.  Notes.  Notes provide additional information for crewmember or maintenance consideration.  Notes are used to identify applicable material, which is intended to assist with compliance, but do not relieve the aircraft operator of the responsibility for compliance with all applicable requirements.  Additional notes may be amended, deleted, or added to the MEL by the aircraft operator, as appropriate.  Notes are not a part of the provisos.

H.  Vertical Bar (change bar).  A vertical bar indicates a change, addition, or deletion in the adjacent text for the current revision of that page only.  All change bars applicable to the previous revision of the MEL are removed prior to the release of the next revision.

4.    	Rotorcraft Flight Manual (RFM).  The FAA-approved RFM is the document approved by the responsible FAA Aircraft Certification Office (ACO) during type certification.  The approved flight manual for the specific aircraft is listed on the applicable Type Certificate Data Sheet (TCDS).  The approved flight manual is the source document for operational limitations and performance parameters for an aircraft.  The term “approved flight manual” can apply to either an AFM or an RFM.  The FAA requires an approved flight manual for aircraft type certification.

5.    	Not Used.

6.    	Code of Federal Regulations (CFR) and Federal Aviation Regulations (FAR).  CFR, the current term, and FAR both refer to the applicable portions of the Federal Aviation Act and Code of Federal Regulations.



7.   Considered Inoperative.  The phrase, “Considered Inoperative”, as used in the provisos, means that an instrument and equipment item must be treated for dispatch, taxi and flight purposes as though it were inoperative.  The item will not be used or operated until the original deferred item is repaired.  Additional actions include: documenting the item on the dispatch release (if applicable), placarding, and complying with all remarks, exceptions, and related MEL provisions, including any (M) and (O) procedures and observing the repair category.

8.   	Continuing Authorization – Single Extension.  An aircraft operator who has the authorization to use an FAA approved MEL may also have the authority to use a continuing authorization to approve a single (one-time) extension to the repair interval for category B or C items in accordance with Operations Specification D095.  Continuing Authorization – Single Extension is not authorized for repair category A and D items.

9.    Dash (-).  Indicates a variable number (quantity) of the instrument and equipment items may be installed or required for dispatch.  This is common when a fleet MEL is used since aircraft of the same make and model may have differing numbers of specific instrument and/or equipment items installed.

10.   Day of Discovery.  This is the calendar-day an equipment/instrument malfunction was recorded in the aircraft maintenance record/logbook.  This day is excluded from the calendar-days or flight-days specified in the MEL for the repair interval of an inoperative instrument and/or equipment item. This provision is applicable to all MEL items; i.e., categories A, B, C, and D.

11.  	Deactivated and/or Secured.  When the MEL refers to an instrument and/or equipment item as deactivated and/or secured, the specified component must be put into an acceptable condition for safe flight.  An acceptable method of deactivating and/or securing will be established by the aircraft operator.

12.  	Deleted.  "Deleted" in the remarks column after a sequence item indicates that the item was previously listed but is now required to be operative if installed in the aircraft.

13.  	Not required.

14.  	Excess Items.  Excess items are those instrument and equipment items that have been installed that are redundant to the requirements of the 14 CFR.

15.  	Flight Day.  A flight-day is a 24-hour period (from midnight to midnight) either universal coordinated time (UTC) or local time, as established by Maritime Helicopters, during which at least one flight is initiated for the affected aircraft.

16.  	Not required.

17.  	Icing Conditions.  An atmospheric environment that may cause ice to form on the aircraft (structural) or in the engine(s) (induction).

18.  	Inoperative.  A system and/or component malfunction to the extent that it does not accomplish its intended purpose and/or is not consistently functioning normally within its approved operating limit(s) and/or tolerance(s).

19.  	Inoperative Components of an Inoperative System.  Inoperative instrument and equipment items, which are components of a system that is inoperative, are usually considered components directly associated with and having no other function than to support that system (warning/caution systems associated with the inoperative system must be operative unless relief is specifically authorized per the MEL).

20.  Is Not Used.  The phrase “Is Not Used” in the provisos, remarks or exceptions for an MEL instrument or equipment item may specify that another item in the MEL “is not used”.  In such cases, crewmembers must not activate, actuate, or otherwise utilize that item under normal operations.  It is not necessary for aircraft operators to accomplish the (M) procedure(s) associated with the item.  However, (O) operational requirements must be complied with, and an additional placard must be affixed, to the extent practical, adjacent to the control or indicator for the item that is not used. This informs crewmembers that an instrument or equipment item is not to be used under normal operations.



21.  	Nonessential Equipment and Furnishings (NEF).  NEFs are those items installed on the aircraft as part of the original type certification (TC), STC, engineering order, or other form of alteration that have no effect on the safe operation of flight and would not be required by the applicable certification rules or operational rules.  They are those items that, if inoperative, damaged, or missing, have no effect on the aircraft’s ability to be operated safely under all operational conditions.  NEF items are not instrument and equipment items already identified in the MEL or CDL of the applicable aircraft.  They do not include instrument and equipment items that are functionally required to meet the certification rule or for compliance with any operational rule.

22.  	Operative.  An operative system and/or component will accomplish its intended purpose and is consistently functioning normally within its design operating limit(s) and tolerance(s).  When an MEL item specifies that an item of equipment must be operative, it does not mean that it’s operational status must be verified; it’s to be considered operative unless reported or known to be malfunctioning. When an MEL item specifies that an item of equipment must be verified operative, it means that it must be checked and confirmed operative at the interval(s) specified for that MMEL item.  When an MEL item specifies that an item of equipment must be verified but no interval is specified, verification is required only at the time of deferral.

Other terminology sometimes used interchangeably with “operative” within the MMEL is “operates normally”, "fully operative", and "considered operative”.  The aircraft operator's MEL may incorporate standardized terminology of the aircraft operator’s choice to specify that an item of equipment must be operative, provided the aircraft operator's MEL definitions indicate that the selected "operative" terminology means that the required item of equipment will accomplish its intended purpose and is consistently functioning normally within its design operating limit(s) and tolerance(s).

23.  	Placarding.  Each inoperative instrument or equipment item must be placarded to inform and remind the crewmembers and maintenance personnel of the item condition.  To the extent practical, placards should be located adjacent to the control or indicator for the item affected; however, unless otherwise specified (i.e. AFM), placard wording and location will be determined by the aircraft operator.

24.  	Repair Category.  All users of an MEL approved under parts 91K, 121, 125, 129, 135, and 142 must effect repairs of inoperative instrument and equipment items, deferred in accordance with the MEL, at or prior to the repair times established by the following letter designators.  Part 91 MEL users (D095/D195 LOAs) are not required to comply with the repair categories, but will comply with any provisos defining a repair interval (flights, flight legs, cycles, hours, etc):

A.  Repair Category A.  This category item must be repaired within the time interval specified in the “Remarks or Exceptions” column of the aircraft operator’s approved MEL.  For time intervals specified in “calendar days” or “flight days”, the day the malfunction was recorded in the aircraft maintenance record/logbook is excluded.  For all other time intervals (i.e., flights, flight legs, cycles, hors, etc.), repair tracking begins at the point when the malfunction is deferred in accordance with the operator’s approved MEL.

B.  Repair Category B.  This category item must be repaired within 3 consecutive calendar-days (72 hours) excluding the day the malfunction was recorded in the aircraft maintenance record/logbook.  For example, if it were recorded at 10 a.m. on January 26th, the 3-day interval would begin at midnight the 26th and end at midnight the 29th.

C.  Repair Category C.  This category item must be repaired within 10 consecutive calendar-days (240 hours) excluding the day the malfunction was recorded in the aircraft maintenance record/logbook.  For example, if it were recorded at 10 a.m. on January 26th, the 10-day interval would begin at midnight the 26th and end at midnight February 5th.

D.	Repair Category D.  This category item must be repaired within 120 consecutive calendar-days (2880 hours) excluding the day the malfunction was recorded in the aircraft maintenance record/logbook.

25.  	Takeoff.  Takeoff is the act of beginning a flight in which an aircraft is accelerated from a state of rest to that of flight.  For the purposes of MEL relief, this translates to the point at which the pilot physically begins to apply power to initiate the takeoff from the runway or takeoff surface.

26.  	Not Used.

27.  	Visible Moisture.  An atmospheric environment containing water, in any form, that can be seen in natural or artificial light; for example, clouds, fog, rain, sleet, hail, or snow.

28.  	Visual Flight Rules (VFR).  VFR is as defined in 14 CFR Part 91.  This precludes a pilot from filing an Instrument Flight Rules (IFR) flight plan.

29.  	Visual Meteorological Conditions (VMC).  VMC means the atmospheric environment is such that would allow a flight to proceed under the visual flight rules applicable to the flight.  This does not preclude operating under Instrument Flight Rules.

30.  	(M).  This symbol indicates a requirement for a specific maintenance procedure which must be accomplished prior to operation with the listed item inoperative.  Normally, these procedures are accomplished by maintenance personnel; however, other personnel may be qualified and authorized to perform certain functions.  Procedures requiring specialized knowledge or skill, or requiring the use of tools or test equipment, should be accomplished by maintenance personnel.  The satisfactory accomplishment of all maintenance procedures, regardless of who performs them, is the responsibility of the aircraft operator.  Appropriate procedures are required to be produced as part of the aircraft operator’s manual or MEL.

31.  	(O).  This symbol indicates a requirement for a specific operations procedure which must be accomplished in planning for and/or operating with the listed item inoperative.  Normally, these procedures are accomplished by the flightcrew; however, other personnel may be qualified and authorized to perform certain functions.  The satisfactory accomplishment of all procedures, regardless of who performs them, is the responsibility of the aircraft operator.  Appropriate procedures are required to be produced as a part of the aircraft operator’s manual or MEL.

32.  	Electronic Fault Alerting System.  New generation aircraft display system fault indications to the flight crew by use of computerized display systems.  Aircraft manufacturers incorporate individual design philosophies when determining the data that is represented.  The following are customized definitions (specific to each manufacturer) to help determine the level of messages affecting the aircraft's dispatch status.

	A.  NO CUSTOMIZED DEFINITIONS OF FAULT ALERTING ARE APPLICABLE TO THE MESSERSCHMITT-BOLKOW-BLOHM MODEL BO-105 SERIES AIRCRAFT.
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Preamble
(Effective 6/14/89)

The following is applicable for authorized certificate holders operating under  Title 14 Code of Federal Regulations (14 CFR) Parts 121, 125, 129, 135:  14 CFR  require that all equipment installed on an aircraft in compliance with the Airworthiness Standards and the Operating Rules must be operative.  However, the Rules also permit the publication of a Minimum Equipment List (MEL) where compliance with certain equipment requirements is not necessary in the interests of safety under all operating conditions.  Experience has shown that with the various levels of redundancy designed into aircraft, operation of every system or installed component may not be necessary when the remaining operative equipment can provide an acceptable level of safety. 

A Master Minimum Equipment List (MMEL) is developed by the FAA, with participation by the aviation industry, to improve aircraft utilization and thereby provide more convenient and economic air transportation for the public.  The FAA approved MMEL includes those items of equipment related to airworthiness and operating regulations and other items of equipment which the Administrator finds may be inoperative and yet maintain an acceptable level of safety by appropriate conditions and limitations;  it does not contain obviously required items such as wings, flaps, and rudders.  The MMEL is the basis for development of individual operator MELs which take into consideration the operator's particular aircraft equipment configuration and operational conditions. Operator MELs, for administrative control, may include items not contained in the MMEL; however, relief for administrative control items must be approved by the Administrator.  An operator's MEL may differ in format from the MMEL, but cannot be less restrictive than the MMEL. The individual operator's MEL, when approved and authorized, permits operation of the aircraft with inoperative equipment. Equipment not required by the operation being conducted and equipment in excess of  14 CFR requirements are included in the MEL with appropriate conditions and limitations.  The MEL must not deviate from the Aircraft Flight Manual Limitations, Emergency Procedures or with Airworthiness Directives.  It is important to remember that all equipment related to the airworthiness and the operating regulations of the aircraft not listed on the MMEL must be operative. 

Suitable conditions and limitations in the form of placards, maintenance procedures, crew operating procedures and other restrictions as necessary are specified in the MEL to ensure that an acceptable level of safety is maintained. 

The MEL is intended to permit operation with inoperative items of equipment for a period of time until repairs can be accomplished.  It is important that repairs be accomplished at the earliest opportunity. In order to maintain an acceptable level of safety and reliability the MMEL establishes limitations on the duration of and conditions for operation with inoperative equipment.  

The MEL provides for release of the aircraft for flight with inoperative equipment.  When an item of equipment is discovered to be inoperative, it is reported by making an entry in the Aircraft Maintenance Record/Logbook as prescribed by 14 CFR. The item is then either repaired or may be deferred per the MEL or other approved means acceptable to the Administrator prior to further operation. MEL conditions and limitations, do not relieve the operator from determining that the aircraft is in condition for safe operation with items of equipment inoperative. When these requirements are met, an Airworthiness Release, Aircraft Maintenance Record/Logbook entry, or other approved documentation is issued as prescribed by 14 CFR. Such documentation is required prior to operation with any item of equipment inoperative. 

Operators are responsible for exercising the necessary operational control to ensure that an acceptable level of safety is maintained. When operating with multiple inoperative items, the interrelationships  between those items and the effect on aircraft operation and crew workload will be considered.  Operators are to establish a controlled and sound repair program including the parts, personnel, facilities, procedures and schedules to ensure timely repair. 

WHEN USING THE MEL, COMPLIANCE WITH THE STATED INTENT OF THE PREAMBLE, DEFINITIONS, AND THE CONDITIONS AND LIMITATIONS SPECIFIED IN THE MEL IS REQUIRED. 
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Deferral Procedures

The following policy and procedures will be adhered to by the Maritime Helicopters Inc. company in the use of this FAR Part 135 Minimum Equipment List (MEL).

It is the pilot in command's responsibility to become thoroughly familiar with the policy and procedures concerning the use of MEL. All items related to the airworthiness of the aircraft and not included on the MEL are required to be fully and properly operative. Any discrepancies discovered after engine start and prior to flight, the pilot shall abort and item must be addressed I/AW this approved MEL. If the pilot is able to MEL the item(s), he shall follow the instructions in column 4. REMARKS & EXCEPTIONS (O) instructions and label as appropriate.  If an item must be addresses by a mechanic indicated by the an (M), they must contact a mechanic and ensure (M) remarks compliance before further flight. 

If any item failure occurs after engine start, but prior to take-off the pilot shall review the MEL procedure to determine if the item can be MEL’d and if not shall contact maintenance to have the item repaired.

If an inoperative item requires a Maintenance procedure, that procedure must be accomplished and recorded in accordance with FAR Sections 43.11, 91.405(c)(d) and 135.179 prior to flight.

When the discrepancy is corrected, the person performing the maintenance will record it in accordance with FAR Section 43.11.  Inoperative items allowed by the MEL must be corrected no later than the period specified by the letters (A, B, C, D). As soon as practical after discovering the failure, Maritime Helicopters shall make arrangements at the aircraft base or at a suitably equipped repair facility to accommodate the repairs within the limitations if the aircraft is to be kept in service.

An item which is inoperative, but required by special flight conditions, will be repaired before operating in those conditions. The Maritime Helicopters Inc. company will ensure that all discrepancies are recorded in the aircraft maintenance logbook and the Discrepancy Report and Deferral Report so the pilot in command may be aware of any inoperative instruments or equipment. 

Maintenance personnel shall be informed and trained (when applicable) that an MEL is being utilized. The PIC shall ensure that the proper MEL logbook entries are made by maintenance personnel when appropriate. The PIC or Maintenance personnel shall ensure the proper placards are affixed per the MEL as applicable.

General
The pilot in command (PIC) shall make the final decision to defer based on:
a. This Minimum Equipment List (MEL).
b. All applicable Federal Aviation Regulations.
c. All applicable Airworthiness Directives.
d. Good judgment.
e. Input from maintenance personnel, when applicable.

Placards
The crewmember (For an (O) procedure) or the maintenance personnel or PIC, when authorized, (For an (M) procedure) shall affix the required placard. If the (M) procedure states PIC or Flight Crewmember, pilot placarding is authorized.

Placard Procedure
The pilot or mechanic will enter the discrepancies in the Aircraft Log Book. Then in the “Corrective Action” column make a statement that the defective unit is being deferred I/A/W Maritime Helicopters MEL, item number _________. (ie. 2841-01 for Fuel quantity gauge), see MEL Discrepancy and Deferral Report. 

On the MEL Discrepancy and Deferral Report, which is located on the back side of the logbook cover, write the discrepancy up exactly how is was written up in the log book.
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Remove a red sticker from the envelope inside the RFM and attach to or near the affected control of the inoperative item. Date the sticker with the current day's date and MEL Item and System number.
Method of Tracking
MEL discrepancies shall be tracked by the Chief Inspector for all aircraft reporting to the Homer Base and tracked by the Fairbanks Maintenance Lead for aircraft reporting to Fairbanks.  This will include number of items per aircraft, reason for any delay in repair, length of delay and an estimated date item will be repaired.

Plan for Repair
MEL deferrals that cannot be corrected by simple part(s) replacement shall be discussed with either the Fairbanks Maintenance Manager or Chief Inspector to determine a plan of action.  Arrangement will be made for any specialized tooling and/or facilities to correct the discrepancy as required.

Unavailability of Parts
If parts are not available, they must be ordered by the quickest possible shipping method to receive and installed the part prior to the end of the allowed deferral timeframe. If a vendor indicates there will be any delay, an expected delivery date shall be requested. 

Procedure for Controlling Extensions
MEL items may not be rectified prior to the allotted Category time due to possible parts delays or access to suitable repair facilities. In these instances, a MEL extension request shall be sent to the Flight Standards District Office certificated team responsible for Maritime Helicopters.  Included in the request shall be the reason for the delay and a plan of action to correct the discrepancy. Extensions may only be initiated by the Fairbanks Lead or Chief Inspector after coordination with the Director of Maintenance.

Duties and Responsibilities
· The pilot or mechanic is responsible for the discovery and initiation of all MEL requests and notification to either the Fairbanks Maintenance Lead or the Chief Inspector.
· An A&P rated mechanic is responsible for rectification of the deferred item and will transcribe the entry from the Discrepancy and Deferral Report back to the current aircraft logbook page as a Discrepancy, then enter the corrective action. The same corrective action will be entered below the original discrepancy in the Discrepancy and Deferral Report, which closes out the MEL.  
· The Chief Inspector will be responsible to track all MEL items, status of parts and repair processes.
· The Director of Maintenance shall retain overall responsibility for MEL management but may delegate duties.

[bookmark: _Hlk62553465]Manual Revision and Control
The Director of Maintenance is responsible for the content of this manual and any revisions. This manual requires FAA approval prior to release. Revisions to this manual must be routed MHI internal and FAA acceptance prior to distribution. This manual cannot be published or distributed to end users prior to formal submission to and approval by the FAA indicated by signature(s) on the Control Page(s).

Changes made to this manual will be indicated throughout by change bars. A vertical bar (change bar) in the right margin indicates a change, addition, or deletion in the adjacent text for the current revision of that page only.  The change bar is dropped at the next revision of that page. The effected paged will also be annotated by updating the revision level and date in the top right-hand corner. The Control Page(s) and Log of Revisions will also be updated as required. 

The Director of Maintenance shall submit the proposed revision in electronic PDF format to the Federal Aviation Administration (FAA) for review and approval. Should a proposed revision be found unacceptable by the FAA, the Director of Maintenance will immediately withdraw the proposed revision and decide whether to further revise and resubmit to the FAA.
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	JASC SYSTEM & TITLE
	1. REPAIR CATEGORY

	SYSTEM & SEQUENCE
NO.
	
COMPONENT DESCRIPTION
	
	2. NUMBER INSTALLED

	
	
	
	
	3. NUMBER REQUIRED FOR DISPATCH

	
	
	
	
	
	4. REMARKS & EXCEPTIONS



	21. AIR CONDITIONING

	2100-01
	Air Conditioning System
	D
	0
	0
	Not Installed.
	

	2100-02
	Freon Air Conditioner
	C
	0
	0
	DELETED (see item 2100-01)
	

	2100-03
	Fresh Air Vent
	C
	2
	1
	Co-pilots fresh air vent may be inoperative.
	

	2100-04
	Cold Weather Kit
Heater Fan
	C
	1
	0
	May be inoperative above -35°C (-31°F) OAT.
	

	2120-01
	Windshield Defog/
Ventilation Blower
(Pilots/Co-pilot)
	C
	1
	1
	May be inoperative provided Bleed Air
Heater or Bleed Air ECU is operative.
	

	2140-01
	Bleed Air Heating
System
	C
	1
	0
	May be inoperative, provided:

 a)  Bleed air heating system is not required for  defrosting/defogging.
b)  Flight is not conducted in visible moisture, and,
c)  Pilot's air vent blower is operative
     
(M) A Maintenance technician will disconnect and secure the line to ensure it doesn’t chaff, IAW CH 850 of the BO105 Maintenance Manual.

  (O)  Pilot shall avoid all flight operations in visible moister and ensure air vent blower is operative.

	

	2140-02
	Electrical Heating and Ventilating System
	C
	1
	0
	May be inoperative above +5°C (41°F) outside air temperature provided;

 a) Pilot's Vent Blower operative, and
 b) System is deactivated and secured.

(M) A Maintenance technician will ensure no evidence of damage, electrical short, exist, and: Pull and tie wrap the circuit breaker on the circuit breaker panel.
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	21. AIR CONDITIONING

	2140-03
	Bleed Air ECU Systems (STC SH1031EA)
	C
	0
	0
	Not Installed
	

	2140-04
	Windshield Defog Vent Blowers
	C
	0
	0
	DELETED
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	22. AUTO FLIGHT

	2200-01
	(CSAS) Control Stabilization Augmentation System) (LS Models Only)
	 C
	0
	0
	Not Installed.
	

	2200-02
	(SAS) Stability Augmentation System (Except LS Models)
	 C
	0
	0
	Not Installed.
	

	2210-01
	4-way Beep Trim System
	B
	1
	0
	Not Installed.
	

	2210-02
	Force Trim Release
(FTR) System
	B
	0
	0
	Not Installed.
	

	2210-03
	Flight Director System
	C
	0
	0
	Not Installed.
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	23. COMMUNICATIONS

	2300-01

	Communications
Systems (FM)
	D
	1
	0
	May be inoperative if operations do not require its use.
	

	2300-02
	Cockpit Intercom System ICS 
	D
	2
	1
	Co-pilots side ICS may be inoperative.
	

	2300-03
	Cabin ICS 
	D
	3
	1
	One or more may be inoperative, provided;

(O) Pilot shall brief the passenger(s) regarding alternate normal and emergency procedures to be used. The Pilot briefing must include any appropriate operating restrictions.
	

	2300-04
	Flight Deck Headset
Earphones/Headphone
	C
	-
	1
	Any in excess of one headset for each required cockpit crew member or hoist/cargo hook operator on duty may be inoperative or missing.
NOTE:  Spare headset must be available and operative.
	

	2300-05
	Headset (passengers) 
	D
	-
	0
	May be inoperative or missing, provided;

(O) Pilot shall brief the passenger(s) regarding alternate normal and emergency procedures to be used. The Pilot briefing must include any appropriate operating restrictions.
	

	2310-01
(PL-106) 
	Communications
Systems (HF)
	D

C
	0

0
	0

0
	Not installed.
	

	2310-02
	Satellite Tracking or Satellite Phone Systems(s)
	D
	1
	0
	NOTE: SATCOM is to be used only as a backup to normal HF communications unless otherwise authorized by the appropriate ATC facilities.
	

	2311-01
(PL-95)
	Communications
Systems (UHF)
	D
	0
	0
	Not Installed.
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	23. COMMUNICATIONS

	 2312-01
 (PL-95)
	Communications
Systems (VHF)




a) VHF Communications
    Control Panels

1. Frequency Transfers Light
2. Frequency Transfer Switch
3. Frequency Selector Knob
4. Frequency Indication






	D







C

C

C

C
	2







-

-

-

-
	1







0

0

2

2
	Any in excess of those required by FAR may be inoperative provided it is not powered by the, Emergency DC Bus, Battery Bus, or the DC Transfer Bus and not required for emergency procedures.
	 

	2312-02

	Communications
Systems (FM)






	D






	1






	0






	May be inoperative provided operations are not predicated on the affected radio.
	

	2340-01
	External Loud Speaker
	C
	0
	0
	Not Installed.
	

	2340-02
	Telephone
	C
	0
	0
	DELETED.
	

	2350-01
	Aural Warning Generator
	C
	0
	0
	Not Installed.
	

	2350-01
	Automatic Voice Alert Device
	C
	0
	0
	Not Installed.
	

	2370-01/02
(PL-29)
	Cockpit Voice Recorder (CVR)
	A
	0
	0
	Not Installed.
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	24. ELECTRICAL POWER

	2400-03
	EPU (External Power Unit) Door Caution Light
(LS models only)
	B
	1
	0
	May by inoperative provided EPU door is verified closed prior to flight.
	

	2400-04
	EPU (External Power Unit) Door Caution Light
(LS models only)
	C
	0
	0
	May by inoperative, provided EPU is disconnected and EPU door is closed prior to flight.

(O) Pilot will physically ensure the EPU is disconnected and door is closed prior to flight.
	

	2400-05
	Emergency Power
Supply (for Standby Attitude Indicator)
	C
	0
	0 
	Not installed. (Not Required for day VFR)
	

	2422-02
	Utility Inverter
	C
	0
	0
	Not installed.
	

	2432-01
	Battery(s)
	C
	1
	1
	Must be operative.
	

	2432-02
	Battery Discharge Warning Light
	C
	1
	0
	May be inoperative provided both generators (Item 2435-01) and respective ammeter and voltmeter indications are operative.
	

	2432-03

	Flight Inverter
	C
	0
	0
	Not installed. (Not Required for VFR)
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	24. ELECTRICAL POWER

	2435-01
	Generator
	A
	2
	1
	One may be inoperative for three consecutive days for other than Night VFR provided:

a)  Electrical load is reduced to single generator capacity,
b)  Ammeter and Voltmeter indication of the operative generator ore both working, and,
c)  Inoperative Generator is deactivated and secured.

NOTE: Total electrical failure will limit fuel  available to quantity contained in supply tank at time of failure.

(M) A maintenance technician  will ensure no evidence of damage, electrical short, or hazards exist, and: Pull and tie wrap the field circuit breaker on the right hand side baggage compartment and ensure starter mode is operational by temporarily activating starter button.
	

	2435-02
	Generator I / Generator II Warning Light
	C
	2
	0
	May be inoperative provided respective Ammeter
 and Voltmeter are both operative.
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	25. EQUIPMENT/FURNISHINGS

	2500-01 (PL-116)
	NEF Items
	-
	-
	0
	May be inoperative, damaged or missing provided that the item(s) is deferred in accordance with the NEF deferral program. The NEF program, procedures and processes are outlined in the Maritimes NEF manual. 

(M)(O) Procedures, if required, must be available to the flight crew and included in the operator’s appropriate document.


	




	2500-02
	Electro-optical System Enhanced Vision (i.e. FLIR)
	D
	1
	0
	May be inoperative provided the system is deactivated, secured & placarded.

(M) Maintenance shall deactivate and secure system by removing power unit.

	

	2510-01
	Co-Pilots Seat
	D
	1
	0
	May be inoperative provided seat is not occupied, and is blocked and placarded.

(M)(O) The seat will be blocked with tape and placarded “DO NOT OCCUPY”
	

	2510-02
	Crew member Shoulder Harness
	B
	2
	1
	Co-plots shoulder harness may be inoperative or missing provided the affected seat is not required by 14 CFR or used.
	

	2510-03
	Crew Seat Vertical Adjustment
	C
	2
	0
	One or more may be inoperative provided the affected seat is locked in a position acceptable to the flight crew member.

(M) Mechanic will endure that the locking mechanism is fully seated to prevent seat movement.

(O) Pilot will ensure the locked seat position allows for full movement of tail rotor pedals.
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	25. EQUIPMENT/FURNISHINGS

	2510-04
	Fabric Glareshield
	D
	0
	0
	Not Installed.
	

	2510-05
	Sun Shade
	D
	1
	0
	May be inoperative provided it is properly removed and stowed.
	

	2510-06
	Headset Holder
	D
	2
	0
	May be inoperative or missing.
	

	2510-07
	Map Case
	D
	2
	0
	May be inoperative or missing.
	

	2510-08
	Chart Holder
	D

C
	2

2
	0

0
	May be inoperative or missing.

May be inoperative or missing provided:

a)  A personal kneeboard with charge holder function is carried, and
b)  If Night operations are intended, the personal kneeboard has an internal light.
	

	2510-09
	Cockpit Curtain
	D
	0
	0
	Not Installed.
	

	2510-10
(PL-125)
	Printed Supplemental Safety Information
	C
	3
	0
	May be inoperative or missing provided:

a)  No passengers are carried, and
b)  Alternate procedures are established and used.
(O) Pilot shall brief any flight crew regarding alternate normal and emergency procedures to be used. The Pilot briefing must include any appropriate operating restrictions.
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	25. EQUIPMENT/FURNISHINGS

	2520-01
(PL-79)
	Passenger Seat
	D
	4
	0
	May be inoperative provided:

a)  Seat does not block an emergency exit,
b)  Seat does not restrict any passenger from access to the main aircraft isle, and
c)  The affected seat(s) are blocked and placarded “DO NOT OCCUPY”

NOTE 1:  A seat with an inoperative seat belt is considered inoperative.
NOTE 2:  A seat with an inoperative or missing occupant restraint system (seat belt, shoulder harness, etc.), is considered inoperative.
	

	2520-02
	Passenger Seat Belts and/or Shoulder Harnesses
	D


C
	4


4
	0


0
	May be inoperative provided the seat is blocked and placarded.

(M)(O) The seat will be blocked with tape and placarded “DO NOT OCCUPY”
	

	2550-01
	Cargo Net
	D
	-
	0
	May be inoperative or missing provided cargo is secured using alternate means.
	

	2550-02
(PL-100)
	Cargo Restraint Systems
	C
	-
	0
	May be inoperative or missing provided cargo compartment remains empty.
	

	2550-03
	External Cargo Hook
System
	C
	1
	0
	May be inoperable provided the inoperative system is deactivated, secured and placarded.
(M) Ensure cargo arming switch is in the OFF Position.  Install orange dot on suspension system circuit breaker.  No Class B loads allowed.
	

	2550-04
	Cargo Hook Mirror System
	D
	1
	0
	May be inoperable provided the system is deactivated, secured and placarded.

(M) Maintenance shall remove the cargo mirror and placard the cargo mirror adjustment handle. 
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	25. EQUIPMENT/FURNISHINGS

	2550-05
	Fixed Provisions for Bambi Bucket
	D
	1
	0
	May be inoperable provided the system is deactivated, secured and placarded.

(M) Maintenance shall pull and collar system circuit breaker.
	

	2550-06
	External Hoist System
(LH/RH)
	C
	0
	0
	Not installed.
	

	2560-01
	Survival Equipment
	D
	1
	0
	May be inoperative or missing.
	

	2560-02
	Floatation Equipment
	C
	6
	0
	May be unserviceable or missing provided for flights beyond autorotational distance to land;

a) There is a serviceable life preserver for each occupant, and
b) Each occupant must wear a life preserver while aircraft is beyond autorotational distance from the shoreline, 

	

	2560-03
	Helicopter Floatation Devices
	C
	0
	0
	MOVED to Item 3212-01
	

	2560-04
	Litter Adapter
System
	C
	0
	0
	DELETED
	

	2560-05
	Helicopters air Ambulance (HAA) Equipment
	C
	0
	0
	Not installed.
	

	2560-06
	Wire Strike Protection
System
	D
	1
	0
	May be inoperable or missing.
(M) Maintenance shall ensure parts remaining are secured and update aircraft weight and balance.
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	25. EQUIPMENT/FURNISHINGS

	2560-07
	Flare System
	C
	0
	0
	DELETED
	

	2560-08
(PL-73)
	First Aid Kit (FAK) and/or Associated Equipment
	D
	1
	0
	May be missing, incomplete or inoperative.
	

	2562-01
(PL-120)
	Emergency Locator
Transmitter (ELT)
	
	
	
	
	

	
	Survival Type ELT
	D
	0
	0
	Not installed.
	

	
	Fixed ELT
	A
	1
	0
	May be inoperative provided;

a) System is deactivated, and
b) Repairs are made within 90 days.
	
  (M) Remove ELT and placard “ELT not installed” in plain view of flight crew.
	

	
	
	A
	1
	0
	May be missing provided repairs are made within  90 days.

	

	
	
	D
	0
	0
	Not installed. 
	

	
	
	D
	0
	0
	Not installed.
	

	2562-02
	Automatically Deployable Emergency Locator Transmitter (ADELT)
	D
	0
	0
	Not installed.
	

	2562-03
	ELT Remote Switch
	D
	1
	0
	May be inoperative provided ELT transmitter is armed and functional

  (M) Unplug remote switch from ELT, stow and secure.
	

	2562-04
	Sonic Underwater Locator Beacon (ULB)
	D
	0
	0
	Not installed.
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	26. FIRE PROTECTION

	2610-01
	Cargo/Baggage Compartment Smoke Detection System
	C
	1
	0
	May be inoperative provided sound isolation wall is removed.

(M)  Maintenance shall remove isolation wall.
	

	2622-01
(PL-75)
	Portable Fire Extinguisher
	D
	-
	1
	One (1) fire extinguisher must be installed. Any in excess of those required by FAR may be inoperative, or missing provided:

a) Inoperative fire extinguisher is tagged inoperative, removed from the installed location, and placed out of sight so it cannot be mistaken for a functional unit, and

b)  Required distribution is maintained.
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	27. FLIGHT CONTROLS

	2700-01
	Cyclic Stick Lock
	C
	1
	0
	MOVED to Item 6700-01
	

	2700-02
	Co-pilots Cyclic Trim
System
	C
	-
	0
	MOVED to Item 6700-02
	

	2700-03
	Collective Pitch Lock
	C
	1
	0
	MOVED to Item 6700-03
	

	2700-04
	Follow-up Trim System
	C
	-
	0
	MOVED to Item 6700-04
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	28. FUEL

	2810-01
	Long Range Fuel
Tank System
	C
	1
	0
	 May be inoperative provided: 

a) Flight is not predicated upon use of the system, and 
b) Unusable fuel is considered in the weight and balance computations
	

	2822-01
	Main Transfer Pump
	C
	2
	1
	 One pump may be inoperative provided:

a)  Operate IAW BO105 RFM,
b)  Consider unusable fuel quantity in Flight Manual Section 3.2 § 3.
c)  Supply tank fuel level is monitored continuously and operational check prior to departure verifies remainder of fuel system is operational.

 (O)  Conduct a Fuel System Operational Check:
a) Verify operation of low fuel warning light.  Ground run aircraft with transfer pumps off.  Observe low fuel light activates when supply tank indicates approximately 19 gallons of fuel remaining.
b) Verify operation of remaining transfer pump by turning pump on.  Supply tank should refill to 24.5 gallons and warning light should go off.
c) Monitor supply tank during flight.

	

	2822-02
	Supply Pumps
	C
	2
	1
	 On pump may be inoperative provided:

a)   Operate IAW BO105 RFM.
b) Consider unusable fuel quantity in Flight Manual Section 3.2&3..

(O) Verify operation of remaining supply pump by turning pump on.  


	l
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	28. FUEL

	2830-01
	Fuel Dump Valve
	C
	0
	0
	Not installed.


	

	2841-01
	Fuel Contents Gauges
	B
	2
	1
	One fuel gauge may be inoperative provided Fuel quantity for each group is precisely determined.
	

	2841-02
	Fuel Low Quantity Caution Light System
	C
	1
	1
	Must be operative.
	

	2843-01

	Fuel Heater
	D
	0
	0
	Not installed.
	

	
	
	D
	0
	0
	Not installed.
	

	2844-01
	Fuel Flow Monitoring System
	B
	0
	0
	Not installed
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	30. ICE AND RAIN PROTECTION

	3000-01
	Engine Anti-Icing 
System
	C
	2
	0
	May be inoperative provided:

a)  Known and Forecasted outside air temperature above +4.5° C (40° F), and
b)  No visible moisture

	

	3030-01
	Pitot Tube Heat
	B
	1
	0
	May be inoperative provided:

a)  For VFR and
b)  Outside air temperature above +4.5° (40°F), and  
d)  No visible moisture
	






	3030-02
	Co-Pitot Tube Heat
	B
	0
	0
	Copilots pitot heat not installed. Aircraft restricted to single pilot operations. (Does not include training)
	

	3030-03
	Static Port Heat
	C
	0
	0
	Not installed. (Not Required for VFR)
	

	3030-04
	Static Port Heat
	C
	0
	0
	Not installed. (Not Required for VFR)
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	31. INSTRUMENTS

	3100-01
	Electronic flight Instrumentation system (EFS 50)
	C
	0
	0
	Not installed.
	

	3100-02
	Aircraft /Engine
Monitoring systems
	C
	0
	0
	Not installed.
	

	3110-01
	OAT/Free air Temperature Indicator
	C
	1
	0
	May be inoperative provided digital OAT indicator is operational.
	

	3110-02
	Electronic Flight Bag Systems (EFBs)
	C
	0
	0
	Not installed.
	

	3120-01
	Clock 
	C
	1
	0
	Pilot must have watch capable of measuring seconds.
	

	3120-02
	Clock displaying Hours, Minutes and Seconds with sweep second pointer or Digital presentation
	C
	0
	0
	DELETED.
	

	3120-04
	Hour meter
	D
	1
	0
	May be inoperative provided: 

(O) A watch with a stop function is carried in cockpit, and
(O) All flight time with hour meter inoperative will be recorded and entered in the aircraft logbook, and
(M) Adjustments to maintenance time will be recorded in the logbook when the hour meter is repaired.
	

	3120-05
	Elapsed Timer
	C
	1
	0
	DELETED.
	

	3130-01/02
(PL-87)
	Flight Data Recorder (FDR)
	C
	0
	0
	Not installed.
	



	
MARITIME HELICOPTERS                                                       MINIMUM EQUIPMENT LIST

	AIRCRAFT:
BO-105 SERIES
	REV: 2

DATE: 02/15/2017
	PAGE NO.

  32-1

	JASC SYSTEM & TITLE
	1. REPAIR CATEGORY

	SYSTEM & SEQUENCE
NO.
	
COMPONENT DESCRIPTION
	
	2. NUMBER INSTALLED

	
	
	
	
	3. NUMBER REQUIRED FOR DISPATCH

	
	
	
	
	
	4. REMARKS & EXCEPTIONS



	32. LANDING GEAR

	3211-01
	Snow Skids
	D
	1
	0
	May be inoperative provided equipment is secured or both snow skids removed, and landings on soft surface (i.e., bud or snow) 
are not conducted.

	

	3211-02
	Settling Protector
	D
	1
	0
	May be inoperative provided equipment is secured or both settling protectors removed, and landings on soft surface (i.e., mud or snow) are not conducted.
	

	3212-01

	Emergency Flotation
System
	C
	1
	0
	Unless necessary for take-off or landing, for overwater flight,

a) Aircraft must remain within power-off gliding distance to a suitable forced landing area, 

OR

b) For multi-engine operations, aircraft must be operated at a weight, that if the critical engine fails, that will allow it to climb at least 50 feet a minute to an altitude of 1,000 above the surface.

(M) Maintenance shall pull and collar Floatation System Circuit Breaker
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	33. LIGHTS

	3300-01
(PL-127)
	NVG Compatible
Lighting System
	C
	0
	0
	 Not installed.
	

	3310-01
(PL-77)
	Cockpit/Flight Compartment and Instrument Lighting System(s)
	C
	1
	0
	Individual lights may be inoperative provided:

a)	Remaining Lighting System(s) lights are sufficient to clearly illuminate all required instruments, controls, and other devices for which they are provided,
b)	Remaining Lighting System(s) lights are positioned so that direct rays are shielded from flight crewmembers eyes, and
c)	Lighting configuration and intensity is acceptable to the flight crew.

Note 1:  Individual button/switch lights and/or annunciations/indications are excluded from this relief.
Note 2:  Unaided operation (without NVGs) may be permitted with inoperative NVG supplemental lights; cracked or missing filters.
	

	3310-02
	Cockpit Utility Light
	D
	1
	0
	May be inoperative provided two flashlights are available to the pilot flying for Night operations.

	

	3310-03
	Cockpit Dome Light
	C
	1
	0
	May be inoperative.

	

	3320-01
(PL-125)
	Equipment Relief without Passengers
	C
	0
	0
	Not Installed.
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	33. LIGHTS

	3320-02
	“Fasten Seatbelts/No Smoking” Light (Cabin)
	C










D
	-










-
	0










0
	May be inoperative provided a procedure to notify passengers when seat belts must be fastened and smoking is not allowed.

(O) During the passenger safety briefing the passengers will be briefed that the seatbelts will be on for the duration of the flight and the PIC will let them know when they may remove the seatbelts after landing.  Smoking is prohibited at all times.

Provided passengers are not carried.
	

	3320-03
	“Fasten Seatbelts/No Smoking” Light (Cockpit)
	C












D
	-












-
	0












0
	One of more may be inoperative provided a procedure it is verified that the FASTEN SEATBELT AND NO SMOKING SIGN in the cabin is operative, or a procedure is used to notify passenger when the seat belts must be fastened and smoking is not allowed

 (O) During the passenger safety briefing the passengers will be briefed that the seatbelts will be on for the duration of the flight and the PIC will let them know when they may remove the seatbelts after landing.  Smoking is prohibited at all times.
Provided passengers are not carried.
	

	3320-04
	Cabin Lighting System
	D
	1
	0
	May be inoperative for other than Night operation, provided passenger are not carried. 

	

	3330-01
	Utility Light
	D
	1
	0
	May be inoperative provided a flash light is available.

	

	3340-01
	Position Light System
	C
	1
	0
	May be inoperative for day VFR.
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	33. LIGHTS

	3340-02
	Position Light System
IR (IR Flasher)
	C
	1
	0
	May be inoperative for other than Night operation.
	

	3340-03
	Anti-collision light
System
	C
	1
	0
	May be inoperative for day VFR.
	

	3340-04
	Formation Lights 
System
	D
	0
	0
	Not Installed
	

	3340-05
	Pulse Lights
	D
	1
	0
	May be inoperative.
	

	3340-06


	Landing Light / Search and Landing Light System 
	C
	1
	0
	One or more may be inoperative for other than Night operation.

	

	3340-07
	Search and Landing Light (IR Function)
	-
	0
	0
	Not installed
	

	3340-08
	Search Light / Night Sun
	D
	-
	0
	May be inoperative provided system is switched to OFF position.
	

	3340-09
	Tail Flood Light
	D
	0
	0
	Not installed
	

	3340-10
	Strobe Light
	D
	1
	0
	One or more may be inoperative for other than Night provided operations do not require their use.
(see item 3340-03)

	

	3340-11
	Stairway Light
	D
	0
	0
	Not installed
	

	3340-12
	Helicopter Emergency Egress Lighting System (HEELS)
	C
	0
	0
	Not installed
	

	3340-13
	StepLight
	D
	0
	0
	Not installed
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	33. LIGHTS

	3340-14
	Recognition Light 
System
	D
	1
	0
	May be inoperative for other than Night operation.
	

	3340-15
	External Utility Light
	D
	0
	0
	Not Installed.
	

	3340-16
	Supplemental Lighting System
	D
	0
	0
	Not Installed.
	

	3350-01
	Flashlights(s)
	D
	2
	0
	Both may be inoperative for day, one must be operative for night.
	

	3350-02

	Emergency Lighting System
	C
	1
	0
	May be inoperative for day VFR.
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	34. NAVIGATION

	3412-01
	OAT/Free air Temperature Indicator
	D
	1
	0
	May be inoperative provided digital OAT indicator is installed and operational.
	

	3413-01
	Vertical Speed Indicator
	C


B
	2


2
	1


0
	Any in excess of one may be inoperative provided the operative indicator is on the pilots side

One or more may be inoperative for other than Night over routes navigated by reference to the ground.
	

	3414-01
	Airspeed Indicator 
One Pilot Operation

Dual Pilot Operation



	C


D

C

	-


-

-
	1


0

1
	Any in excess of one may be inoperative for other than Night provided operative airspeed indicator is
on the pilot’s side.

Any in excess of two may be inoperative provided the operative airspeed indicators are at each pilot’s station.
Any in excess of one may be inoperative for other than Night provided operative airspeed indicator is
on the pilot’s side.
	

	3416-01
	Sensitive Altimeter
Adjustable for
Barometric Pressure
	C
	1
	1
	Must be operational.
	

	3421-01
	Alternate Static Pressure
	C
	0
	0
	Not installed.
	

	3421-02
	Standby Pitch and Bank Indicator
	C
	0
	0
	Not installed.
	

	3421-03
	Pitch and Bank Indicator
	C
	1
	1
	Must be operational
	

	3422-01
	Direction Indicator

	C
	1
	0
	May be inoperative for other than Night VFR, provided the rate of turn indicator on the Pilot Flying (PF) side is operative.
	

	
	
	C
	-
	0
	Aircraft is restricted to Day VFR flight only.
	

	3423-01
	Magnetic Direction
Indicator.
	C
	1
	0
	 DELETED, Revision 11
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	34. NAVIGATION

	3424-01
	Rate of Turn Indicator
	D



C
	-



-
	0



0
	May be inoperative for other than Night VFR, provided the rate of turn indicator on the Pilot Flying (PF) side is operative.

Aircraft is restricted to Day VFR flight only.
	

	3424-02
	Slip Skid Indicator
	D



C
	-



-
	0



0
	May be inoperative for other than Night VFR, provided the rate of turn indicator on the Pilot Flying (PF) side is operative.

Aircraft is restricted to Day VFR flight only.
	

	3431-01
	Navigation System 
(LOC)
	C
	1
	0
	May be inoperative provided navigation is not predicated on its use.
	

	3432-01
	Navigation Systems 
(ILS)
	C
	1
	0
	May be inoperative provided navigation is not predicated on its use.
	

	3434-01
	Marker Beacon
	C
	1
	0
	May be inoperative provided navigation is not predicated on its use.
	

	3442-01
    
	Weather Radar Thunder- storm Detection System
	C
	0
	0
	Not installed.
	

	3442-02
	Weather Radar System
	C
	0
	0
	 DELETED

	

	3444-01
	Radio Altimeter
	C
	1
	0
	One or more may be inoperative provided:
   a) Autopilot GS-mode is not used,
   b) CAT-A operation is not performed,
c) Night VFR operation is not performed with NVG, and
  d) Operating requirements do not require its use.
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	34. NAVIGATION

	3444-02
(PL-54)
HTAWS
	Class A TAWS Equipment Required
	C
	0
	0
	Not installed
	

	3445-01
(PL-32)
	Traffic Alert and Collision Avoidance System 
(TCAS I)
	B
	0
	0
	Not installed
	

	
	Traffic Alert and
Collision Avoidance
System (TCAS II)

	B
	0
	0
	Not Installed
	

	3445-02
	Traffic Advisory System (TIS/TAS/TCAD)
	D
	0
	0
	Not Installed
	

	3445-03
    
	Outer link CP-2 System
	C
	0
	0
	DELETED
	

	3446-01
	Thunderstorm Detection System
	C
	0
	0
	DELETED
	

	3451-01
(PL-03)
	Distance Measuring Equipment (DME) Systems
	D
	1
	0
	May be inoperative provided navigation is not predicated on its use.
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	34. NAVIGATION (Cont’d)

	3452-01
(PL-76)
	ATC Transponders &
Automatic Altitude
Reporting Systems
	B
	1
	0
	 May be inoperative, provided:
a)  Operations do not require its use,
b)  Prior to flight, approval is obtained from ATC facilities having jurisdiction over the planned route of flight.
	

	
	
	D
	-
	1
	Any in excess of (1) may be inoperative.
	

	
	1)  Elementary and Enhanced Downlink Aircraft Reportable Parameters not required by 14 CFR
	A
	0
	0
	Not installed.
	

	
	2)  ADS-B Squitter
Transmission
	D
	0
	0
	Not installed.
	

	3452-02
(PL-105)
	Automatic Dependent Surveillance-Broadcast (ADS-B) System
	D
	0
	0
	Not installed
	

	3453-01

	LORAN System
	C
	0
	0
	Not installed
	

	3454-01
	VOR System

	C
	1
	0
	May be inoperative provided navigation is not predicated on its use.
	

	3455-01
	ADF System
	C
	0
	0
	Not installed
	

	3457-01
	Global Positioning System (GPS)
(GPS)
	C
	1
	0
	May be inoperative provided navigation is not predicated on its use.
	

	3457-02
	RNAV
	C
	0
	0
	Not installed
	

	3457-03
	XM Weather

	C
	1
	0
	Not installed
	

	3461-01
(PL-98)
	Flight Management
System (FMS)
	C
	0
	0
	Not installed
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	35. OXYGEN

	3510-01
	Oxygen System and Masks (Crew and Passengers)
	D
	0
	0
	Not Installed
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	52. DOORS

	5210-01
	External Door Indicating System
	C
	1
	0
	May be inoperative. 

(O) Pilot will determine thru a visual and pressure applied against door check that doors are closed and latched prior to flight.
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	63. MAIN ROTOR DRIVE

	6310-01
	XMSN Oil TEMP
Caution Light.
	B
	1
	0
	 May be inoperative provided:
 a) Transmission Oil Temperature Indicating System, and	
b)  Transmission Oil Pressure Indicating System are operative.
	

	6510-02
	XMSN Oil PRESS
Warning Light.
	B
	1
	0
	 May be inoperative provided:
 a) Transmission Oil Temperature Indicating System, and	
b)  Transmission Oil Pressure Indicating System are operative.
	

	6320-01
	Intermediate and 90
Degree Gear Boxes Chip Detector System
	C
	3
	0
	May be inoperative if detectors are checked in accordance with manufacturer’s recommendations
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	63. MAIN ROTOR DRIVE

	6321-01
	Rotor Brake System
	C
	1
	0
	 (O) The PIC will conduct a visual inspection to determine the rotor brake pads are not contacting the rotor disk brake and that the main rotor rotates freely by hand.

 (M) Maintenance shall;
a) Safety the handle in the off position to prevent inadvertent use of the rotor brake, 
                                    and
b) Ensure the brake pads are not contacting the rotor brake disk, 
                                    and
c) Perform a visual inspection to ensure that no hydraulic leaks exist,
                                    and
d)   Ensure that the main rotor rotates freely by                                        hand.
	

	[bookmark: _Hlk500252582]6330-01
	Mast Moment Indicating System
	D
	1
	0
	May be inoperative, provided;

  a) Maximum ground sloping for landing is limited to 5°degrees in all directions, and
 b)The RFM limitations for inoperative mast moment indicating system are obeyed.

(M)  May be inoperative for five (5) flights maximum, provided the AMM maintenance procedures are obeyed.

(O)  Pilot shall cross check attitude indicator in order to comply with RFM limitations.
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	65. TAIL ROTOR DRIVE

	6510-01
	XMSN Oil Temperature Indicating System
	
	
	
	DELETED Revision 11
	

	6510-02
	XMSN Oil Temp
Caution Light

	
	
	
	MOVED to Item 6310-01
	

	6510-03
	XMSN Oil Pressure Indicating System
	
	
	
	DELETED Revision 11
	

	6510-04
	XMSN Oil Pressure Warning Light
	
	
	
	MOVED to Item 6310-02
	

	6520-01
	Intermediate and 90° Gear Boxes Chip Detection System
	
	
	
	MOVED to Item 6320-01
	

	6521-01
	Rotor Brake System
	
	
	
	MOVED to Item 6321-01
	

	6530-01
	Mast Moment Indicating System
	
	
	
	MOVED to Item 6330-01
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	67. ROTOR FLIGHT CONTROLS

	6700-01
	Cyclic Stick Lock
	D
	1
	0
	May be inoperative provided cyclic stick is in neutral position during rotor start and run down.
	

	6700-02
	Co-pilots Cyclic Trim
System
	D
	1
	0
	May be inoperative for operations not requiring a co-pilot.
	

	6700-03
	Collective Pitch Lock
	D
	1
	0
	May be inoperative provided collective pitch is in lowest position during rotor start and run down.
	

	6700-04
	Follow-up Trim System
	C
	0
	0
	Not installed.
	





	
MARITIME HELICOPTERS                                                     MINIMUM EQUIPMENT LIST

	AIRCRAFT:
    BO-105 SERIES
	REV: 2

DATE: 02/15/2017
	PAGE NO.

71-1

	JASC SYSTEM & TITLE
	1. REPAIR CATEGORY

	SYSTEM & SEQUENCE
NO.
	
COMPONENT DESCRIPTION
	
	2. NUMBER INSTALLED

	
	
	
	
	3. NUMBER REQUIRED FOR DISPATCH

	
	
	
	
	
	4. REMARKS & EXCEPTIONS



	71. POWERPLANT

	7160-01
	Engine Intake Sand
Filter
	C
	0
	0
	Not installed.
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	77. ENGINE INDICATING

	7700-01
	Automatic Power Sharing and Variable Rotor Speed System (VARTOMS)
	C
	0
	0
	DELETED
	

	7720-01
	Engine Intake Sand
Filter
	C
	0
	0
	MOVED to Item 7160-01
	

	7722-01
	Tachometer, Triple Indicating System (NR) (N2)
	B
	3
	2
	One N2 indicator mat be inoperative provided:

a)  Respective N1 tachometer and engine torque indicator are operative, and
b)  Aircraft shall not depart facility where repairs or replacements can be made, and
c) This engine started first to use NR indicator for the N2.
	

	7722-02
	Dual Torque Indicator
	B
	2
	1
	One indicator needle may be inoperative
provided:

a)  All other engine indicating systems are operating,
b)  Engines are trimmed to matching N1, and
c)  Aircraft shall not depart facility where repairs or replacements can be made.
	

	7723-01
	N2 Trim System
	B
	2
	1
	One trim system may be inoperative
provided;

a)  Pilot verifies respective N2 to be greater than 100% with a torques differential of less than 10% during hover check,
b)  Aircraft shall not depart facility where repairs or replacements can be made.
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	79. ENGINE OIL

	7920-01
	Supplemental Scavenge Oil Filter
	C
	2
	0
	May be inoperative provided it is deactivated and secured

(M)  A maintenance technician will remove the filter from the housing. 

	

	7930-01
	Chip Detector Pulse
Function (Zapper)
	D
	1
	0
	May be inoperative provided RFM emergency procedure for engine chip caution is followed.
	




