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	Cover Page


	Updated to Revision 6 and MKC AEG Cover Page format revised.

	All Pages
	Revised Header to reflect current name of Type Certificate holder and applicable models included in this MMEL.



	Table Of Contents


	Updated to incorporate Revision 6 changes.

	Log Of Revisions


	Updated to incorporate Revision 6 changes.

	Control Pages


	Updated to incorporate Revision 6 changes.

	Highlights Of Change


	Updated to reflect Revision 6 changes.

	Definitions


	Updated to require current Policy Letter (PL)-25 and PL-70 Definitions information for applicable portions of operator’s MEL.



	Preamble
	Updated to require current Preamble information from PL-34, or PL-36 (for Part 91 operations) to be included in operator’s MEL.



	Guidelines (O & M)


	Updated to incorporate Revision 6 changes.

	All ATA Sections


	Revised “FAR” to “14 CFR” in the “SYSTEM ITEM” and “REMARKS” sections of all affected ATA pages.



	ATA 21-10
	Heater Hour Meter relief relocated to ATA 31-4.



	ATA 22
	Chapter title changed from AUTO FLIGHT to AUTOPILOT to reflect current FAA terminology.



	ATA 22-1
	Autopilot relief updated in accordance with (IAW) PL-101.



	ATA 22-3
	Autopilot Disconnect relief added IAW PL-93.



	ATA 23-1
	Communications Systems relief updated IAW PL-95.  HF relief separated and relocated to ATA 23-8, and updated IAW PL-106.



	ATA 23-4
	Passenger Address System relief updated IAW PL-09.



	
	


	ATA 23-5
	Cockpit Voice Recorder relief updated IAW PL-29.



	ATA 23-6
	Boom Microphone relief updated IAW PL-58.



	ATA 23-7
	ELT relief relocated from ATA 25-4, and updated IAW PL-120.



	ATA 23-8
	HF Communications relief relocated from ATA 23-1, and updated IAW 

PL-106.



	ATA 23-9
	Selective Call System (SELCAL) relief added IAW PL-117.



	ATA 25-1
	Repair Category, Number Installed, and Number Required, which were omitted in previous Revision, added for Cockpit Crewmember Shoulder Harness.

 

	ATA 25-2
	Passenger Seat relief updated IAW PL-79.



	ATA 25-4
	ELT relief relocated to ATA 23-7 IAW PL-120.



	ATA 25-5
	Passenger Convenience Items relief converted to Non-Essential Equipment and Furnishings relief IAW PL-116.



	ATA 25-6
	First Aid Kits relief converted to Emergency Medical Equipment relief and updated IAW PL-73.



	ATA 25-7
	Fasten Seat Belt Sign or Placard relief added IAW PL-89.



	ATA 25-8
	Cargo Restraint Systems relief added IAW PL-100.



	ATA 30-7
	Pitot Heat Indicating Systems relief added IAW PL-90.



	ATA 31-3
	Flight Data Recorder System relief updated IAW PL-87.



	ATA 31-4
	Heater Hour Meter relocated from ATA 21-10.



	ATA 33-6
	Cockpit/Flight Deck/Flight Compartment and Instrument Lighting System relief updated IAW PL-77.



	ATA 33-7
	Wing Ice Inspection Light relief updated to current Wing Ice Lights relief.



	ATA 33-9
	Seat Belt and No Smoking Signs relief replaced by Passenger Lighted Information Signs relief IAW PL-123.



	ATA 34-10
	ATC Transponder and Altitude Reporting System relief updated IAW PL-76.


	
	


	ATA 34-13
	Revised Navigation Equipment by separating out and listing major navigation systems independently.

	ATA 34-14
	DME System relief updated IAW PL-03.



	ATA 34-16
	ADF System title spelled out to reflect current FAA terminology.



	ATA 34-17
	RMI System title spelled out to reflect current FAA terminology.



	ATA 34-18
	GPWS relief replaced by Terrain Awareness and Warning System (TAWS) relief IAW PL-54.



	ATA 34-19
	Non-Stabilized Magnetic Compass System relief updated IAW PL-10.



	ATA 34-21
	TCAS II relief updated IAW PL-32.



	ATA 34-22
	TCAS I relief updated IAW PL-32.



	ATA 34-23
	Altitude Alerting System relief added IAW current guidance.



	ATA 34-24
	Flight Management System Navigation Database relief added IAW PL-98.



	ATA 34-25
	Navigation Management System Navigation Database relief added IAW PL-98.



	ATA 34-26
	Standby Attitude Indicator relief added IAW PL-111.



	ATA 34-27
	Windshear Detection, Guidance, and Avoidance System relief added IAW 

PL-67.



	ATA 34-28
	ADS-B relief added IAW PL-105.



	ATA 35-2
	Protective Breathing Equipment relief added IAW PL-43.



	ATA 38
	Chapter added for WATER/WASTE relief items.



	ATA 38-1
	Lavatory Waste System relief added IAW PL-83.



	ATA 46
	Chapter added for INFORMATION SYSTEMS relief items.



	ATA 46-1
	Electronic Flight Bag relief added IAW PL-121.



	
	


The Definitions must be inserted here in each Minimum Equipment List (MEL) from current FAA MMEL Policy Letter 25, entitled “Policy Concerning MMEL Definitions,” and from current FAA MMEL Policy Letter 70, entitled “Definitions Required in MELs”.

The applicable Preamble must be inserted here in each Minimum Equipment List (MEL) from current FAA MMEL Policy Letter 34, entitled “MMEL and MEL PREAMBLE”, or from current FAA Policy Letter 36, entitled “14 CFR Part 91 MEL Approval & Preamble”, for Part 91 MEL approvals.

The FOEB has identified a need for certain procedures to provide an adequate level of safety while providing relief for the following items. These procedures must be established by the operator. The following guidelines are to help establish these required procedures:

	21-1
	(M)

Maintenance procedure to ensure no fuel leak or mechanical/electrical 

fault exists.


	21-3
	(M)

Maintenance procedure to ensure no mechanical or electrical fault exists 

that could cause other damage.


	21-6
	(M)

Maintenance procedure to ensure the Safety Valve is blocked OPEN.

	22-1
	(M)

Maintenance procedure to ensure no electrical or mechanical fault 


exists that will have an adverse affect on any Flight Control function.



	22-2
	(M)

Maintenance procedure to determine that Servos do not cause binding of 

Control Cables.


	23-4-A
	(O)

Operations procedure to ensure PA System is not required by 14 CFR 

and passengers are appropriately briefed.


	23-7-B


	(M)

Maintenance procedure to ensure inoperative System is deactivated.  


Applies to both provisos.



	23-8
	(O)

Operations procedure to ensure SATCOM Voice or Data Link operates

normally, alternate procedures are established and used, and SATCOM 

coverage is available over the intended route of flight. 


	23-9
	(O) Operations procedure to establish and use alternate procedures.  



	23-9-A
	(O)

Operations procedure to establish and use alternate procedures.  



	25-2-A


	(M)

Maintenance procedure to ensure Seat is secured in the FULL 



UPRIGHT position.




	
	


	25-2-B-1


	(M)

Maintenance procedure to ensure Seat is secured in the FULL 



UPRIGHT position if an Armrest is missing.



	25-6-A


	(O)

Operations procedure to ensure AED is resealed in a manner that will


identify it as a Unit that cannot be mistaken for a fully serviceable unit.



	25-6-B


	(O)

Operations procedure to ensure EMK is resealed in a manner that will 

identify it as a Unit that cannot be mistaken for a fully serviceable Unit.


	25-6-C


	(O)

Operations procedure to ensure FAK is resealed in a manner that will 


identify it as a Unit that cannot be mistaken for a fully serviceable Unit.


	25-8


	(M)

Maintenance procedure to ensure acceptable cargo loading limits 



from an approved source are maintained.



	27-1
	(M)

Maintenance procedure to ensure no electrical or mechanical fault exists 

that could affect any flight control function.


	28-1
	(O)

Operations procedure to ensure that fuel on board meets the regulatory 

requirements for the intended flight.  


	28-2
	(O)

Operations procedure to ensure that fuel on board meets the regulatory 

requirements for the intended flight.


	31-2
	(O)

Operations procedure for recording aircraft flight time.

	31-4
	(O)

Operations procedure to record hours of Heater operation.

	32-1
	(O)

Operations procedure to prevent movement of aircraft when stopped or 

parked.



	33-9

	(O)

Operations procedure to ensure PA System operates normally and is 


used to notify passengers when Signs are turned ON or OFF. 


	33-9-A


	(O)

Operations procedure to ensure alternate procedures are established 


and used.



	
	


	34-18-A-1


	(O)

Operations procedure to ensure alternate procedures are established 


and used.



	34-18-A-1-a
	(O)

Operations procedure to ensure alternate procedures are established 


and used.



	34-18-A-1-d


	(O)

Operations procedure to ensure alternate procedures are established 


and used.

(O)

Operations procedure to ensure alternate procedures are established 


and used and Advisory Callouts are not required by 14 CFR.



	34-18-A-1-e
	(O)

Operations procedure to ensure alternate procedures are established 


and used.



	34-18-B-1


	(O)

Operations procedure to ensure alternate procedures are established 


and used.



	34-19


	(O)

Operations procedure to ensure any combination of three Gyro or INS 

(IRU) Stabilized Compass Systems are operative.

(O)

Operations procedure to ensure any combination of two Gyro or INS 


(IRU) Stabilized Compass Systems operate normally, the airplane is 


operated with dual independent navigation capability, and is under 


positive radar control by ATC on the enroute portion of the flight.

(O)

Operations procedure to ensure the flight is entirely within areas of 


magnetic unreliability provided at least two Stabilized Directional Gyro 

Systems are installed, operate normally, and are used in conjunction with 

approved free gyro navigation techniques.



	34-21


	(M)

Maintenance procedure to ensure System is deactivated and 




SECURED.  Applies to both provisos.



	34-21-B


	(O)

Operations procedure to ensure TA Visual Display and Audio Functions 

are operative, TA ONLY Mode is selected by the crew, 
and enroute or 

approach procedures do not require use of the RA Display System.



	34-21-C


	(O)

Operations procedure to ensure RA Visual Display and Audio Functions 

are operative, and enroute or approach procedures do not require use of 

the TA Display System.



	
	


	34-22
	(M)

Maintenance procedure to ensure System is deactivated and 




SECURED.  Applies to both provisos.



	34-23
	(O)

Operations procedure to ensure Autopilot with Altitude Hold is 




operative and enroute operations do not require use of the Altitude 


Alerting System.

(O)

Operations procedure to ensure aircraft is operated with a Second 


in Command and enroute operations do not require use of the 




Altitude Alerting System.


	34-24-A


	(O)  
Operations procedure to ensure current aeronautical charts are used, 


status and suitability of navigation facilities to be used are verified, and 

Approach Navigation Radios are manually tuned and identified.



	34-25-A


	(O)  
Operations procedure to ensure current aeronautical charts are used, 


status and suitability of navigation facilities to be used are verified, and 

Approach Navigation Radios are manually tuned and identified.



	34-27-A-1


	(O)

Operations procedure to ensure alternate procedures are established 


and used.

(O)

Operations procedure to ensure alternate procedures are established 


and used and Windshear Detection and Avoidance System (Predictive) 

operates normally.



	34-27-A-2


	(O)

Operations procedure to ensure alternate procedures are established 


and used.

(O)

Operations procedure to ensure alternate procedures are established 


and used and Windshear Warning and Flight Guidance System 



(Reactive) operates normally.



	34-27-B-1
	(O)

Operations procedure to ensure alternate procedures are established 


and used.



	34-27-B-2


	(O)

Operations procedure to ensure alternate procedures are established 


and used.



	
	


	38-1
	(M)

Maintenance procedure to ensure associated Components are

 

            deactivated or isolated and System Components do not have leaks.


	46-1-A

	(O)  
Operations procedure to ensure alternate procedures are established 


and used.



	46-1-B
	(O)  
Operations procedure to ensure alternate procedures are established 


and used.



	46-1-C
	(O)  
Operations procedure to ensure alternate procedures are established 


and used.



	46-1-D
	(M)  
Maintenance procedure to ensure associated EFB and hardware is 


secured by an alternate means or removed from the aircraft.  

(O)  
Operations procedure to ensure alternate procedures are established 


and used.

(M)  
Maintenance procedure to ensure associated EFB and hardware is 


secured by an alternate means or removed from the aircraft.  



	
	


	21
	AIR CONDITIONING 
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Combustion Heater (Excluding Blower)
	C
	1
	0
	(M)
	

	
	
	
	
	
	
	

	2.
	Automatic Temperature Control System
	C
	1
	0
	
	

	
	
	
	
	
	
	

	3.
	Air Conditioning System
	C
	1
	0
	(M)
	

	
	
	
	
	
	
	

	4.
	Cabin Altitude Controller
	C
	1
	0
	May be inoperative for unpressurized flight.
	

	
	
	
	
	
	
	

	5.
	Cabin Altitude/ Differential Pressure Indicator
	C
	1
	0
	May be inoperative for unpressurized flight.
	

	
	
	
	
	
	
	

	6.
	Safety Valve
	C
	1
	0
	(M) May be inoperative for unpressurized flight provided Safety Valve is blocked OPEN.
	

	
	
	
	
	
	
	

	7.
	Outflow Valve
	C
	1
	0
	May be inoperative for unpressurized flight.
	

	
	
	
	
	
	
	

	8.
	Recirculation Fan
	C
	1
	0
	
	

	
	
	
	
	
	
	

	9.
	Cabin Rate Of Change Indicator
	C
	1
	0
	May be inoperative for unpressurized flight.
	

	
	
	
	
	
	
	

	10.
	Heater Hour Meter
	
	
	
	RELOCATED TO ATA 31-4, REVISION 6.
	|
|
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	AUTOPILOT
	
	
	
	
	|

	
	
	
	
	
	
	

	1.
	Autopilot System 
	C
	-
	0
	(M) May be inoperative provided operations do not require its use.
	|
|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE 1:  For RVSM operations, the 

                Altitude Hold Function must 

    be operative.
	|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE 2:  See AFM Supplement for 


    possible Flap use 




    restrictions.
	|

	
	
	
	
	
	
	

	2.
	Yaw Damper
	C
	1
	0
	(M) May be inoperative provided Yaw Damper is independent of and unrelated to Autopilot operation or the Autopilot is not used.
	

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  See AFM Supplement for 


 possible Yaw Damper vs. 


 Autopilot operating 




 instructions.
	

	
	
	
	
	
	
	

	3.
	Autopilot Disconnect Functions 

(Quick Release Controls)
	C

B


	2

2


	1

0


	One may be inoperative provided: 

a) Autopilot is not used below 1,500 feet AGL, and

b) Approach minimums do not require the use of the Autopilot.

May be inoperative provided Autopilot is not used.
	|

|

|

|

|

|

|
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	COMMUNICATIONS
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Communications System (VHF And UHF) 
	D
	-
	-
	Any in excess of those required by 14 CFR may be inoperative provided it is not powered by any emergency power source and not required for emergency procedures.
	|
|

|

|

|

	
	
	
	
	
	
	

	2.
	Cockpit Speaker
	C
	1
	0
	As required by 14 CFR.
	|

	
	
	
	
	
	
	

	3.
	Audio Amplifier
	C
	1
	0
	As required by 14 CFR.
	|

	
	
	
	
	
	
	

	4.
	Passenger Address System (PA)
	
	
	
	
	|
|

	
	
	
	
	
	
	

	A)
	Passenger Configuration
	C


	1
	0
	(O) May be inoperative provided:

a) PA not required by 14 CFR, and

b) Alternate, normal and emergency procedures, and/or operating restrictions are established and used.

NOTE:  Any station function(s) that

             operate normally may be used.
	|

|

|

|

|

|

|
|

|

	
	
	
	
	
	
	

	B)
	Cargo Configuration
	D


	1


	0


	May be inoperative provided procedures do not require its use.
	|

|

	
	
	
	
	
	
	

	5.
	Cockpit Voice Recorder (CVR)
	
	
	
	
	|

|

	
	
	
	
	
	
	

	A)
	For Air Carrier And Commercial Operators
	
	
	
	
	|

|

	
	
	
	
	
	
	

	1)
	With Flight Data Recorder (FDR) Installed
	A
	1
	0
	May be inoperative provided:

a) Flight Data Recorder (FDR) operates normally, and

b) Repairs are made within three flight days.
	|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|
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	COMMUNICATIONS
	
	
	
	
	

	
	
	
	
	
	
	

	5.
	Cockpit Voice Recorder (CVR) (Continued)
	
	
	
	
	|

|

|

	
	
	
	
	
	
	

	A)
	For Air Carrier And Commercial Operators (Continued)
	
	
	
	
	|

|
|

	
	
	
	
	
	
	

	2)
	Without Flight Data Recorder (FDR) Installed
	A
	1
	0
	May be inoperative provided repairs are made within three flight days.
	|

|

|

	
	
	
	
	
	
	

	B)
	For Operators Other Than Air Carriers And Commercial Operators
	A
	1
	0
	May be inoperative provided repairs are made in accordance with applicable sections of 14 CFR.
	|

|

|

	
	
	
	
	
	
	

	6.
	Boom Microphones 
	
	
	
	
	|

	
	
	
	
	
	
	

	A)
	Cockpit Voice Recorder With Flight Data Recorder Installed
	
	
	
	
	|

|

|

|

	
	
	
	
	
	
	

	1)
	Cockpit Voice Recorder Equipped To Record Boom Microphone Per 14 CFR 135.151(d)
	A
	-
	0
	May be inoperative provided:

a) Flight Data Recorder (FDR) operates normally, and 

b) Repairs are made within three flight days.
	|

|

|

|

|

	
	
	
	
	
	
	

	2) ***
	Cockpit Voice Recorder Not Equipped To Record Boom Microphone 
	D
	-
	0
	Any in excess of those required by 14 CFR may be inoperative.
	|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|
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	COMMUNICATIONS
	
	
	
	
	

	
	
	
	
	
	
	

	6.
	Boom Microphones (Continued)
	
	
	
	
	|

	
	
	
	
	
	
	

	B)
	Cockpit Voice Recorder Without Flight Data Recorder Installed 
	
	
	
	
	|
|

|

|

	
	
	
	
	
	
	

	1)
	Cockpit Voice Recorder Equipped To Record Boom Microphone Per 14 CFR 135.151(d) 
	A
	-
	0
	May be inoperative provided repairs are made within three flight days.
	|
|

|

|

|

	
	
	
	
	
	
	

	2) ***
	Cockpit Voice Recorder Not Equipped To Record Boom Microphones 
	D
	-
	0
	Any in excess of those required by 14 CFR may be inoperative.
	|
|

|

|

	
	
	
	
	
	
	

	7.
	Emergency Locator Transmitter (ELT)
	
	
	
	
	|

|

	
	
	
	
	
	
	

	A)

***
	Survival Type ELTs
	D
	-
	-
	Any in excess of those required by 14 CFR may be inoperative or missing.
	|

|

	
	
	
	
	
	
	

	B)

***
	Fixed ELTs
	A
	-
	0
	(M) May be inoperative provided:

a) System is deactivated, and

b) Repairs are made within 90 days.
	|

|

|

|

	
	
	
	
	
	
	

	
	
	A
	-
	0
	May be missing provided repairs are made within 90 days.
	|

|

	
	
	
	
	
	
	

	
	
	D
	-
	-
	(M) Any in excess of those required by 14 CFR may be inoperative provided system is deactivated.
	|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	-
	Any in excess of those required by 14 CFR may be missing.
	|

|
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	COMMUNICATIONS
	
	
	
	
	

	
	
	
	
	
	
	

	8.
	High Frequency  (HF)

Communication System
	D


	-


	-


	Any in excess of those required by 14 CFR may be inoperative.
	|

|

|

	
	
	
	
	
	
	

	
	
	C
	-
	1
	(O) May be inoperative while conducting operations that require two LRCS provided:

a) SATCOM Voice or Data Link operates normally,

b) Alternate procedures are established and used,

c) SATCOM coverage is available over the intended route of flight, and

d) If INMARSAT Codes are not available while using SATCOM Voice prior coordination with the appropriate ATS facility is required. 
	|

|

|

|

|

|

|

|
|
|
|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  SATCOM is to be used only as 

             a backup to normal HF

             communications unless

             otherwise authorized by the

             appropriate ATS facilities.
	|

|

|

|

|

	
	
	
	
	
	
	

	9.
	Selective Call Systems (SELCAL)
	C
	-
	0
	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	0
	May be inoperative provided procedures do not require its use.
	|

|

	
	
	
	
	
	
	

	A)
	Channels
	C
	-
	0
	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	0
	May be inoperative provided procedures do not require its use.
	|

|

	
	
	
	
	
	
	


	24
	ELECTRICAL
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Alternator Ammeters
	
	
	
	DELETED, REVISION 5.
	

	
	
	
	
	
	
	

	2.
	Battery Ammeter
	
	
	
	DELETED, REVISION 5.
	

	
	
	
	
	
	
	

	3.
	Voltmeter
	
	
	
	DELETED, REVISION 5.
	

	
	
	
	
	
	
	

	4.
	Inverters 

(PA-31P-350 Only)
	B
	2
	1
	One may be inoperative for day VMC.
	

	
	
	
	
	
	
	

	5.
	Alternator Inoperative Warning Lights
	
	
	
	DELETED, REVISION 5.
	

	
	
	
	
	
	
	


	25
	EQUIPMENT/ FURNISHINGS 
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Cockpit Crewmember Shoulder Harness
	C
	2
	1
	Right side may be inoperative provided Seat remains unoccupied.
	|

	
	
	
	
	
	
	

	2.
	Passenger Seat(s) 
	D
	-
	-
	May be inoperative provided:

a) Seat does not block an Emergency Exit,

b) Seat does not restrict any passenger from access to the aircraft aisle, and

c) Affected Seat(s) are blocked and placarded “DO NOT OCCUPY”.
	|
|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE 1:  A Seat with an inoperative 

                Seat Belt is considered 

                inoperative.
	|



	
	
	
	
	
	
	

	
	
	
	
	
	NOTE 2:  Affected Seat(s) may include 

                the Seat(s) behind and/or 

                adjacent Seats.
	|

|

|

	
	
	
	
	
	
	

	A)
	Recline Mechanism 
	D
	-
	-
	(M) May be inoperative and Seat occupied provided Seat is secured in the FULL UPRIGHT position.
	|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	-
	May be inoperative and Seat occupied provided Seat Back is immovable in FULL UPRIGHT position.
	|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|

	
	
	
	
	
	
	


	25
	EQUIPMENT/ FURNISHINGS 
	
	
	
	
	

	
	
	
	
	
	
	

	2.
	Passenger Seat(s) (Continued) 
	
	
	
	
	|
|

	
	
	
	
	
	
	

	B)
	Armrest
	
	
	
	
	|

	
	
	
	
	
	
	

	1)
	Armrest With Recline Mechanism
	D
	-
	-
	(M) May be inoperative or missing and Seat occupied provided:

a) Armrest does not block an Emergency Exit,

b) Armrest does not restrict any passenger from access to the main aircraft aisle, and

c) If Armrest is missing, Seat is secured in the FULL UPRIGHT position.
	|

|

|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	2)
	Armrest Without Recline Mechanism
	D
	-
	-
	May be inoperative or missing and Seat occupied provided:

a) Armrest does not block an Emergency Exit, and

b) Armrest does not restrict any passenger from access to the main aircraft aisle.
	|

|

|

|

|

|

|

	
	
	
	
	
	
	

	3.
	Flotation Equipment
	
	
	
	DELETED, REVISION 5.
	

	
	
	
	
	
	
	

	4.
	Emergency Locator Transmitter (ELT)
	
	
	
	RELOCATED TO ATA 23-7, REVISION 6.
	|
|

	
	
	
	
	
	
	


	25
	EQUIPMENT/ FURNISHINGS 
	
	
	
	
	

	
	
	
	
	
	
	

	5.

***
	Non-Essential Equipment & Furnishings (NEF) 
	
	-
	0
	May be inoperative, damaged, or missing provided that the item(s) is deferred in accordance with the operator’s NEF deferral program.  The NEF program, procedures, and processes are outlined in the operators (insert name) Manual.  (M) and (O) procedures, if required, must be available to the flight crew and included in the operator’s appropriate document.
	|

|

|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	6.
	Emergency Medical Equipment
	
	
	
	
	|

|

	
	
	
	
	
	
	

	A)
	Automatic External Defibrillator (AED) And/Or Associated Equipment
	A
	-
	0
	(O) May be incomplete, missing or inoperative provided: 

a) AED is resealed in a manner that will identify it as a Unit that cannot be mistaken for a fully serviceable Unit, and

b) Repairs or replacements are made within three flight cycles.
	|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	-
	Any in excess of those required by 14 CFR may be incomplete, missing, or inoperative.
	|

|

|

	
	
	
	
	
	
	

	B)
	Emergency Medical Kit (EMK) And/Or Associated Equipment
	A
	-
	0
	(O) May be incomplete, missing or inoperative provided:

a) EMK is resealed in a manner that will identify it as a Unit that cannot be mistaken for a fully serviceable Unit, and

b) Repairs or replacements are made within three flight cycles.
	|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|

	
	
	
	
	
	
	


	25
	EQUIPMENT/ FURNISHINGS 
	
	
	
	
	

	
	
	
	
	
	
	

	6.
	Emergency Medical Equipment 
(Continued)
	
	
	
	
	|

|

	
	
	
	
	
	
	

	B)
	Emergency Medical Kit (EMK) And/Or Associated Equipment (Continued)
	
	
	
	
	|

|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	-
	Any in excess of those required by 14 CFR may be incomplete, missing, or inoperative. 
	|

|

|

	
	
	
	
	
	
	

	C)
	First Aid Kit (FAK) And/Or Associated Equipment
	A
	-
	-
	(O) If more than one is required by 14 CFR, only one of the required First Aid Kits may be incomplete, missing or inoperative provided:

a) FAK is resealed in a manner that will identify it as a Unit that can not be mistaken for a fully serviceable Unit, and 

b) Repairs or replacements are made within three flight cycles.
	|

|

|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	-
	Any in excess of those required by 14 CFR may be incomplete, missing, or inoperative.
	|

|

|

	
	
	
	
	
	
	

	7.
	“Fasten Seat Belt While Seated” Sign Or Placard 
	C
	-
	-
	One or more Signs or Placards may be illegible or missing provided a legible Sign or Placard is visible from each occupied Passenger Seat.
	|

|

|

|

	
	
	
	
	
	
	


	25
	EQUIPMENT/ FURNISHINGS
	
	
	
	
	

	
	
	
	
	
	
	

	8. ***
	Cargo Restraint Systems 
	C
	-
	-
	(M) May be inoperative or missing provided acceptable cargo loading limits from an approved source, i.e., an Approved Cargo Loading Manual, Cargo Handling Manual, or Weight and Balance Document are observed.
	|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	C
	-
	-
	May be inoperative or missing provided Cargo Compartment remains EMPTY.
	|

|
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	FIRE PROTECTION
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Portable Fire Extinguisher 
	D
	-
	-
	Any in excess of those required by 14 CFR may be inoperative or missing provided:

a) The inoperative Fire Extinguisher is tagged INOPERATIVE, removed from the installed location and placed out of sight so it cannot be mistaken for a functional Unit, and 

b) Required distribution is maintained.
	|
|
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	FLIGHT CONTROLS
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Electric Elevator Trim System
	C
	1
	0
	(M) May be inoperative provided:
a) Manual Trim is operative and not affected, and

b) Autopilot operation is unaffected or Autopilot is not used.
	

	
	
	
	
	
	
	

	2.
	Flap Position Indicator
	
	
	
	DELETED, REVISION 5.
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	FUEL 
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Fuel Quantity Gauge (PA-31P)
	C
	4
	3
	(O) One inboard Fuel Gauge may be inoperative provided:
a) A reliable means is established to determine that fuel quantity on board meets the regulatory requirements for the intended flight, and

b) Both Fuel Flow Gauges are operative.
	

	
	
	
	
	
	
	

	2.
	Fuel Quantity Gauge (PA-31P-350)
	C
	2
	1
	(O) One may be inoperative provided:
a) A reliable means is established to determine that fuel quantity on board meets the regulatory requirements for the intended flight, and

b) Both Fuel Flow Gauges are operative.
	

	
	
	
	
	
	
	

	3.
	Fuel Flow Gauges 

(PA-31P-350)
	C
	2
	1
	One may be inoperative provided:
a) All Fuel Quantity Gauges are operative, and

b) Both Fuel Pressure Gauges are operative.
	

	
	
	
	
	
	
	

	4.
	Fuel Totalizer 
(PA-31P-350)
	C
	1
	0
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	ICE & RAIN PROTECTION
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Surface Deicing System 

(Wing, Vertical And Horizontal Stabilizer)
	C
	1
	0
	May be inoperative provided aircraft is not operated in known or forecast icing conditions.
	

	
	
	
	
	
	
	

	2.
	Windshield Deicing System
	C
	1
	0
	May be inoperative provided aircraft is not operated in known or forecast icing conditions.
	

	
	
	
	
	
	
	

	3.
	Pitot Heater
	B
	2
	0
	Left unit must be operative for IFR passenger carrying and for flight in known or forecast icing conditions.  Two heated Pitot Tubes are required for these conditions if a second Airspeed Indicator is installed and operative.
	

	
	
	
	
	
	
	

	4.
	Windshield Wiper
	C
	-
	0
	May be inoperative provided aircraft is not operated in precipitation within 5 nautical miles of the airport of takeoff or intended landing.
	

	
	
	
	
	
	
	

	5.
	Propeller Deicing System
	C
	1
	0
	May be inoperative provided aircraft is not operated in known or forecast icing conditions.
	

	
	
	
	
	
	
	

	6.
	Stall Warning Plate Heater
	C
	1
	0
	May be inoperative provided aircraft is not operated in known or forecast icing conditions.
	

	
	
	
	
	
	
	

	7.
	Pitot Heat Indicating Systems (Not Required By The Certification Or Operating Rules)
	C
	-
	0
	May be inoperative provided:

a) All other Elements of the Pitot Heat System operate normally, and

b) The airplane is not operated into known or forecast icing conditions.
	|

|

|

|

|

|

|

	
	
	
	
	
	
	


	31
	INDICATING/ RECORDING SYSTEMS
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Clock With Sweep Second Hand Or Electric Digital Clock
	C
	1
	0
	May be inoperative for VFR operations.
	

	
	
	
	
	
	
	

	2.
	Flight Hour Recorder 
	C
	1
	0
	(O)
	

	
	
	
	
	
	
	

	3.
	Flight Data Recorder (FDR) System
	C
	-
	-
	Any in excess of those required by 14 CFR may be inoperative.
	|
|

	
	
	
	
	
	
	

	
	
	A
	-
	0
	May be inoperative provided:

a) Cockpit Voice Recorder (CVR) operates normally,

b) Airplane is not dispatched from a designated airport as listed in the operator’s MEL unless:

1. The FDR failure occurs after pushback but prior to takeoff or

2. The FDR repair was attempted but was not successful.

c) In those cases where repair is attempted but not successful, the aircraft may be dispatched on a flight or series of flights until the next designated airport where repair must be accomplished prior to dispatch, and

d) Repairs are made within three flight days.
	|

|

|

|

|

|

|

|

|

|

|

|

|

|

|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|
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	INDICATING/ RECORDING SYSTEMS
	
	
	
	
	

	
	
	
	
	
	
	

	3.
	Flight Data Recorder (FDR) System (Continued)
	
	
	
	
	|

|

|

	
	
	
	
	
	
	

	A)
	For Air Carrier And Commercial Operators
	
	
	
	
	|

|

	
	
	
	
	
	
	

	1)
	FDR Recording Parameters Required By 14 CFR
	A
	-
	-
	May be inoperative provided:

a) Cockpit Voice Recorder (CVR) operates normally, and

b) Repairs are made within 20 calendar days.
	|

|

|

|

|

	
	
	
	
	
	
	

	2)
	FDR Recording Parameters Not Required By 14 CFR
	A
	-
	-
	May be inoperative provided repairs are made prior to completion of the next scheduled maintenance check.
	|

|

|

	
	
	
	
	
	
	

	B)
	Operators Other Than Holders Of Air Carrier Or Commercial Operator Certificates
	C
	-
	1
	Any in excess of those required by 14 CFR may be inoperative.
	|

|

|

|

	
	
	
	
	
	
	

	
	
	A
	-
	0
	May be inoperative provided repairs are made in accordance with applicable sections of 14 CFR.
	|

|

|

	
	
	
	
	
	
	

	4.
	Heater Hour Meter
	C
	1
	0
	(O)
	|
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	LANDING GEAR
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Parking Brake
	C
	1
	0
	(O)
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	LIGHTS
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Position Lights 
	C
	3
	0
	May be inoperative for day operations.
	

	
	
	
	
	
	
	

	2.
	Anti-Collision Light System 
	B
	1
	0
	May be inoperative for day operations.
	

	
	
	
	
	
	
	

	3.
	Landing Lights
	C
	2
	0
	May be inoperative for day operations.
	

	
	
	
	
	
	
	

	4.
	Taxi Light
	C
	1
	0
	
	

	
	
	
	
	
	
	

	5.
	In-Flight Recognition Lights
	C
	2
	0
	
	

	
	
	
	
	
	
	

	6.
	Cockpit/ Flight Deck/ Flight Compartment And Instrument Lighting System 
	C
	-
	-
	Individual Lights may be inoperative provided remaining Lights are:

a) Sufficient to clearly illuminate all required instruments, controls, and other devices for which it is provided,

b) Positioned so that direct rays are shielded from flight crewmembers eyes, and

c) Lighting configuration and intensity is acceptable to the flight crew.
	|



	
	
	
	
	
	
	

	7.
	Wing Ice Lights
	C
	-
	0
	May be inoperative provided aircraft is not operated in known or forecast icing conditions at night.
	|

|

|

	
	
	
	
	
	
	

	
	
	C
	-
	0
	May be inoperative provided:

a) Aircraft is equipped with an approved Ice Detection System, and

b) Ground deicing procedures do not require use of Wing Ice Lights.
	|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|

	
	
	
	
	
	
	


	33
	LIGHTS
	
	
	
	
	

	
	
	
	
	
	
	

	7.
	Wing Ice Lights (Continued)
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	C
	2
	1
	One may be inoperative provided:

a) Left Light is operative for single pilot operations, and

b) Ground deicing procedures do not require use of Wing Ice Lights.
	|

|

|

|

|

|

	
	
	
	
	
	
	

	8.
	Cabin Light System
	C
	-
	-
	May be inoperative provided lighting configuration is acceptable to the flight crew.
	

	
	
	
	
	
	
	

	9.
	Passenger Lighted Information Signs
	C
	-
	-
	(O) May be inoperative and associated Passenger Seat may be occupied provided:

a) PA System operates normally, and

b) PA System is used to notify passengers when associated Sign(s) are placed ON or OFF.
	|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	A)
	For 14 CFR 91 Operations And Operations Not Requiring Use Of PA System 
	C
	-
	-
	(O) May be inoperative provided alternate procedures are established and used to notify Cabin occupants.
	|

|

|

|

|

	
	
	
	
	
	
	

	10.
	Cabin Door Boarding Light
	C
	1
	0
	
	

	
	
	
	
	
	
	

	11.
	Ground Recognition Beacon
	C
	1
	0
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	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Altimeter Adjustable For Barometric Pressure
	B
	2
	1
	May be inoperative on right side.
	

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  Where a Servoed Electric 


 Altimeter is installed, a 



 functioning Pneumatic 



 Altimeter is required.
	

	
	
	
	
	
	
	

	2.
	Airspeed Indicator
	C
	2
	1
	May be inoperative on right side.
	

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  Where a Servoed Electric 


 Airspeed is installed, a 



 functioning Pneumatic 



 Airspeed Indicator is required.
	

	
	
	
	
	
	
	

	3.
	Gyroscopic Pitch And Bank Indicator System
	B
	2
	1
	May be inoperative on right side.
	

	
	
	
	
	
	
	

	4.
	Gyroscopic Directional Indicator System
	B
	2
	1
	May be inoperative on right side.
	

	
	
	
	
	
	
	

	5.
	Gyroscopic Rate Of Turn/Slip Skid Indicator
	B
	2
	0
	May be inoperative on right side, and may be inoperative on left side for day VFR.
	

	
	
	
	
	
	
	

	6.
	Vertical Speed Indicator
	B
	1
	0
	May be inoperative on left side for operations other than IFR passenger carrying.
	

	
	
	
	
	
	
	

	7.
	Flight Director
	C
	1
	0
	
	

	
	
	
	
	
	
	

	8.
	Radar Altimeter
	C
	1
	0
	
	

	
	
	
	
	
	
	

	9.
	Weather Radar/ Thunderstorm Detection Equipment 
	C
	1
	0
	As required by 14 CFR.
	|

	
	
	
	
	
	
	


	34
	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	10.
	ATC Transponders And Automatic Altitude Reporting Systems
	B

D
	-

-
	0

1
	May be inoperative provided:

a) Operations do not require its use, and

b) Prior to flight, approval is obtained from ATC facilities having jurisdiction over the planned route of flight.

Any in excess of those required by 14 CFR may be inoperative.
	|

|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	A)
	Elementary And Enhanced Downlink Aircraft Reportable Parameters Not Required By 14 CFR
	A
	-
	0
	May be inoperative provided:

a) Operations do not require its use, and

b) Repairs are made prior to completion of the next scheduled maintenance check.
	|

|

|

|

|

|

	
	
	
	
	
	
	

	B)
	ADS-B Squitter Transmissions
	A
	-
	0
	May be inoperative provided:

a) Operations do not require its use, and

b) Repairs are made prior to completion of the next scheduled maintenance check.
	|

|

|

|

|

|

	
	
	
	
	
	
	

	11.
	Marker Beacon
	C
	1
	0
	May be inoperative provided approach procedure does not require its use.
	

	
	
	
	
	
	
	

	12.
	Altitude Encoder
	
	
	
	COMBINED WITH ATC TRANSPONDERS, REVISION 5b
	

	
	
	
	
	
	
	

	13.
	Navigation Equipment 
	C
	-
	-
	
	

	
	
	
	
	
	
	

	A)
	VOR/ILS System
	C
	-
	-
	May be inoperative provided:

a)
It is not required by 14 CFR, 


and


b)
Operations don’t require its use.
	|
|

|
|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|
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	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	13.
	Navigation Equipment

(Continued)
	
	
	
	
	|
|

	
	
	
	
	
	
	

	B)
	LORAN, Area Navigation (RNAV)
	C
	-
	-
	May be inoperative provided:


a)
It is not required by 14 CFR, 


and


b)
Operations don’t require its use. 
	|
|

|

|

	
	
	
	
	
	
	

	C)
	Global Positioning System (GPS)
	C
	-
	-
	May be inoperative provided:


a)
It is not required by 14 CFR, 


and 


b)
Operations don’t require its use.
	|

|

|
|

	
	
	
	
	
	
	

	14.
	Distance Measuring Equipment (DME) Systems 
	D
	-
	-
	Any in excess of those required by 14 CFR may be inoperative. 
	|

|

|

	
	
	
	
	
	
	

	15.
	Altitude Alert/Preselect
	C
	1
	0
	
	

	
	
	
	
	
	
	

	16.
	Automatic Direction Finder (ADF)
	C
	1
	0
	As required by 14 CFR.
	|

|

	
	
	
	
	
	
	

	17.
	Radio Magnetic Indicator (RMI)
	C
	1
	0
	
	|

|

	
	
	
	
	
	
	

	18.
	Terrain Awareness And Warning System (TAWS)
	
	
	
	
	|

|

|

	
	
	
	
	
	
	

	A)
	Class B TAWS Equipment (Not Required By 14 CFR)
	
	
	
	
	|

|

|

	
	
	
	
	
	
	

	1)
	Ground Proximity Warning System (GPWS)


	A
	1
	0
	(O) May be inoperative provided:

a) Alternate procedures are established and used, and

b) Repairs are made within two flight days.
	|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|

	
	
	
	
	
	
	


	34
	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	A)
	Class B TAWS Equipment (Not Required By 14 CFR) (Continued) 
	
	
	
	
	|

|

|

|

	
	
	
	
	
	
	

	1)
	Ground Proximity Warning System (GPWS)

(Continued)
	
	
	
	
	|

|

|

|

	
	
	
	
	
	
	

	a)
	Modes 1 & 3
	A
	2
	0
	(O) May be inoperative provided:

a) Alternate procedures are established and used, and 

b) Repairs are made within two flight days.
	|

|

|

|

|

	
	
	
	
	
	
	

	b)
	Test Mode
	A
	1
	0
	May be inoperative provided:

a) GPWS is considered inoperative, and 

b) Repairs are made within two flight days.
	|

|

|

|

|

	
	
	
	
	
	
	

	c)

***
	Modes 2, 4 & 5


	C
	3
	0
	
	|

|

	
	
	
	
	
	
	

	d)
	Advisory Callouts
	B
	-
	0
	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	
	
	C
	-
	0
	(O) May be inoperative provided:

a) Advisory Callouts not required by 14 CFR, and 

b) Alternate procedures are established and used.
	|

|

|

|

|

	
	
	
	
	
	
	

	e)

***
	Windshear Mode (Reactive)
	C
	1
	0
	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|

	
	
	
	
	
	
	


	34
	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	A)
	Class B TAWS Equipment (Not Required by 14 CFR)
(Continued)
	
	
	
	
	|
|

|

|

	
	
	
	
	
	
	

	2)
	Terrain System-Forward Looking Terrain Avoidance (FLTA) And Premature Descent Alert (PDA) Functions
	B
	1
	0
	
	|

|

|

|

|

|

	
	
	
	
	
	
	

	3)

***
	Terrain Displays


	C
	-
	0
	
	|

|

	
	
	
	
	
	
	

	4)

***
	Runway Awareness & Advisory System (RAAS)
	C
	1
	0
	
	|

|

|

	
	
	
	
	
	
	

	B)
	Class C TAWS Equipment
	
	
	
	
	|

|

	
	
	
	
	
	
	

	1)

***


	TAWS/GPWS


	C
	1
	0
	(O) May be inoperative provided alternate procedures are established and used.

NOTE:  Any Mode that operates 

             normally may be used.
	|

|

|

|

|

	
	
	
	
	
	
	

	19.
	Non-Stabilized Magnetic Compass
	B
	1
	0
	(O) May be inoperative provided any combination of three Gyro or INS (IRU) Stabilized Compass Systems are operative.
	|



	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|
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	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	19.
	Non-Stabilized Magnetic Compass (Continued)
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	B
	1
	0
	(O) May be inoperative provided:

a) Any combination of two Gyro or INS (IRU) Stabilized Compass Systems are operative, and

b) Aircraft is operated with dual independent navigation capability and under positive radar control by ATC on the enroute portion of the flight.
	|



	
	
	
	
	
	
	

	
	
	B
	1
	0
	(O) May be inoperative for flights that are entirely within areas of magnetic unreliability provided at least two Stabilized Directional Gyro Systems are installed, operative, and used in conjunction with approved free gyro navigation techniques.
	|



	
	
	
	
	
	
	

	20.
	Flight Profile Advisory System
	C
	1
	0
	
	

	
	
	
	
	
	
	

	21. 
	Traffic Alert And Collision Avoidance System (TCAS II) 
	B
	-
	0
	(M) May be inoperative provided:

a) System is deactivated and SECURED, and

b) Enroute or approach procedures do not require its use.
	|

|

|

|

|

	
	
	
	
	
	
	

	
	
	C
	-
	0
	(M) May be inoperative provided:

a) System is not required by 14 CFR,

b) System is deactivated and SECURED, and

c) Enroute or approach procedures do not require its use.
	|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|
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	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	21. ***
	Traffic Alert And Collision Avoidance System (TCAS II)  (Continued) 
	
	
	
	
	|

|

|

|

	
	
	
	
	
	
	

	A)
	Combined Traffic Alert (TA) And Resolution Advisory (RA) Dual Display System(s)
	C
	2
	1
	One may be inoperative on the non-flying pilot side provided:

a) TA and RA Visual Display is operative on flying pilot side, and

b) TA and RA Audio Functions are operative on flying pilot side.
	|

|

|

|

|

|

|

	
	
	
	
	
	
	

	B)
	Resolution Advisory (RA) Display System(s) 
	C
	2
	1
	May be inoperative on non-flying pilot side.
	|

|

	
	
	
	
	
	
	

	
	
	C
	-
	0
	(O) May be inoperative provided:

a) Traffic Alert (TA) Visual Display and Audio Functions are operative,

b) TA ONLY Mode is selected by the crew, and

c) Enroute or approach procedures do not require its use.
	|

|

|

|

|
|

|

|

|

	
	
	
	
	
	
	

	C)
	Traffic Alert Display System(s)
	C
	-
	0
	(O) May be inoperative provided:

a) RA Visual Display and Audio Functions are operative, and

b) Enroute or approach procedures do not require its use.
	|

|

|

|

|

|

	
	
	
	
	
	
	

	D)
	Audio Functions
	B
	1
	0
	May be inoperative provided enroute or approach procedures do not require use of TCAS.
	|

|

|

	
	
	
	
	
	
	

	E)

***
	Airspace Selection Function
	C
	-
	0
	
	|

|
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	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	22. 
	Traffic Alert And Collision Avoidance System (TCAS I) 
	B
	-
	0
	(M) May be inoperative provided:

a) System is deactivated and SECURED, and

b) Enroute or approach procedures do not require its use.
	|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	C
	-
	0
	(M) May be inoperative provided:

a) Not required by 14 CFR,

b) System is deactivated and SECURED, and

c) Enroute or approach procedures do not require its use.
	|

|

|

|

|

|

|

	
	
	
	
	
	
	

	23.
	Altitude Alerting System 

	A
	-
	0
	(O) May be inoperative provided:

a) Autopilot with Altitude Hold is operative, 

b) Enroute operations do not require its use, and

c) Repairs are made within three flight days.
	|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE: RVSM is affected if Aircraft is 

approved for RVSM operations.
	|

|

	
	
	
	
	
	
	

	
	
	A
	-
	0
	(O) May be inoperative provided:

a) Aircraft is operated with a Second in Command,
b) Enroute operations do not require its use, and

c) Repairs are made within three flight days.
	|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE: RVSM is affected if Aircraft is 

approved for RVSM operations.
	|

|
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	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	24. 
	Flight Management System 
	
	
	
	
	|
|

	
	
	
	
	
	
	

	A)
	Navigation Databases 
	C
	-
	-
	(O) May be out of currency provided:

a) Current aeronautical charts are used to verify navigation fixes prior to dispatch,
b) Procedures are established and used to verify status and suitability of navigation facilities used to define route of flight, and

c) Approach navigation radios are manually tuned and identified. 
	|
|

|

|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	25. 
	Navigation Management System 
	
	
	
	
	|

|

	
	
	
	
	
	
	

	A)
	Navigation Databases 
	C
	-
	-
	(O) May be inoperative provided:

a) Current aeronautical charts are used to verify navigation fixes prior to dispatch,

b) Procedures are established and used to verify status and suitability of navigation facilities used to define route of flight, and

c) Approach navigation radios are manually tuned and identified.
	|

|

|

|

|

|

|

|

|

|

|

	
	
	
	
	
	
	

	26. 
	Standby Attitude Indicator 
	C
	-
	0
	May be inoperative provided not required by 14 CFR.
	|

|

	
	
	
	
	
	
	

	
	
	B
	-
	0
	May be inoperative provided:

a) Operations are conducted in day VMC only, and

b) Operations are not conducted into known or forecast over-the-top conditions.
	|

|

|

|

|

|
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	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	27.
	Windshear Detection, Guidance And Avoidance System
	
	
	
	
	|

|

|

	
	
	
	
	
	
	

	A)
	Installation Required By 14 CFR
	
	
	
	
	|

|

	
	
	
	
	
	
	

	1)

***
	Windshear Warning And Flight Guidance System (Reactive)
	B
	-
	0
	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  Operator’s alternate

             procedures should include
             reviewing windshear

             avoidance and windshear 
             recovery procedure.
	|

|

|

|

|

	
	
	
	
	
	
	

	
	
	C
	-
	0
	(O) May be inoperative provided:

a) Alternate procedures are established and used, and

b) Windshear Detection and Avoidance System (Predictive) operates normally.
	|

|

|

|

|

|

	
	
	
	
	
	
	

	2)

***
	Windshear Detection And Avoidance System (Predictive)
	B
	-
	0
	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  Operator’s alternate 

             procedures should include 

             reviewing windshear 
             avoidance and windshear 
             recovery procedures.
	|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|
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	NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	27.
	Windshear Detection, Guidance And Avoidance System (Continued)
	
	
	
	
	|

|

|

|

	
	
	
	
	
	
	

	A)
	Installation Required By 14 CFR 
(Continued)
	
	
	
	
	|

|

|

	
	
	
	
	
	
	

	2)

***
	Windshear Detection And Avoidance System (Predictive) (Continued)
	
	
	
	
	|

|

|

|

	
	
	
	
	
	
	

	
	
	C
	-
	0
	(O) May be inoperative provided:

a) Alternate procedures are established and used, and

b) Windshear Warning and Flight Guidance System (Reactive) operates normally. 
	|

|

|

|

|

|

	
	
	
	
	
	
	

	B)
	Installation Not Required By 14 CFR
	
	
	
	
	|

|

	
	
	
	
	
	
	

	1)

***
	Windshear Warning And Flight Guidance System (Reactive) 
	C


	-


	0


	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	2)

***
	Windshear Detection And Avoidance System (Predictive)
	C
	-
	0
	(O) May be inoperative provided alternate procedures are established and used. 
	|

|

|

	
	
	
	
	
	
	


	34
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	28. 
	Automatic Dependent Surveillance Broadcast (ADS-B) System 
	D
	-
	0
	May be inoperative provided it is not required by 14 CFR.
	|
|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  If ADS-B is installed in lieu of 
             or as replacement for 14 CFR 
             required equipment, the repair 
             category in the operator’s MEL 
             will be the same as that of the 
             14 CFR required equipment.
	|
|

|

|

|

|

	
	
	
	
	
	
	

	A)
	Link And Display Processor Unit (LDPU) 
	D
	-
	0
	
	|
|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  Cockpit Display Traffic 
             Information (CDTI) display of 
             data from other aircraft 
             systems may be used.
	|
|

|

|

	
	
	
	
	
	
	

	B)
	Cockpit Display And Traffic Information (CDTI) 
	D
	-
	0
	
	|
|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  ADS-B data transmissions 
             may continue.
	|
|

	
	
	
	
	
	
	

	C)
	CDTI Control Panel 
	D
	-
	0
	May be inoperative provided:

a) Flight ID can be set, and

b) Screen Display is acceptable to the flight crew.
	|
|

|

|

	
	
	
	
	
	
	

	D)
	Data Link Transmitter(s) 
	D
	-
	0
	
	|
|

	
	
	
	
	
	
	

	E)
	Data Link Receiver(s) 
	D
	-
	0
	
	|
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	OXYGEN
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Oxygen System (Passenger)
	C
	-
	-
	As required by 14 CFR.
	|

	
	
	
	
	
	
	

	2.
	Protective Breathing Equipment (PBE)
	D
	-
	-
	Any in excess of those required by 14 CFR may be inoperative.
	|

|
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	WATER/WASTE
	
	
	
	
	|

	
	
	
	
	
	
	

	1.

***
	Portable Lavatory System
	C
	-
	0
	(M) May be inoperative provided:

a) Associated Components are deactivated or isolated,

b) System Components are verified not to have leaks, and

c) System is placarded “DO NOT USE”.
	|

|

|

|

|

|

|
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	INFORMATION SYSTEMS
	
	
	
	
	|
|

	
	
	
	
	
	
	

	1.

***
	Electronic Flight Bag Systems (EFBs)
	
	
	
	
	|

|

	
	
	
	
	
	
	

	A)

***
	Class 3 EFBs
	C
	-
	-
	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	NOTE:  Any function, program or 

             document which operates 

             normally may be used.              
	|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	0
	May be inoperative provided procedures do not require its use.
	|

|

	
	
	
	
	
	
	

	B)

***
	Data Connectivity 

(Class 2)
	C
	-
	-
	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	0
	May be inoperative provided procedures do not require its use.
	|

|

	
	
	
	
	
	
	

	C)

***
	Power Connection 

(Class 1 & 2)
	C
	-
	-
	(O) May be inoperative provided alternate procedures are established and used.
	|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	0
	May be inoperative provided procedures do not require its use.
	|

|

	
	
	
	
	
	
	

	D)

***
	Mounting Device 

(Class 2)
	C
	-
	0
	(M)(O) May be inoperative provided:

a) The associated EFB and hardware is secured by an alternate means or removed from the aircraft, and

b) Alternate procedures are established and used.
	|

|

|

|

|

|

|

	
	
	
	
	
	
	

	
	
	
	
	
	(Continued)
	|
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	INFORMATION SYSTEMS
	
	
	
	
	|
|

	
	
	
	
	
	
	

	1.

***
	Electronic Flight Bag Systems (EFBs) (Continued)
	
	
	
	
	|

|

|

	
	
	
	
	
	
	

	D)

***
	Mounting Device 

(Class 2) 
(Continued)
	
	
	
	
	|

|

|

	
	
	
	
	
	
	

	
	
	D
	-
	0
	(M) May be inoperative provided:

a) Associated EFB and hardware is secured by an alternate means or removed from the aircraft, and

b) Procedures do not require its use.
	|

|

|

|

|

|

|
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	DOORS
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Cabin Door Lower Extension Snubber
	C
	1
	0
	May be inoperative provided Door is lowered MANUALLY.
	

	
	
	
	
	
	
	

	2.
	Cabin Door Ajar Warning Light
	C
	1
	0
	May be inoperative provided:
a) A flight crewmember confirms by visual inspection that the Cabin Door is latched prior to each departure,

b) Cabin remains unpressurized, and

c) No Smoking/Fasten Seat Belt Sign remains ON or passengers are orally briefed to remain seated with their Seat Belts FASTENED.
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	PROPELLERS
	
	
	
	
	

	
	
	
	
	
	
	

	1.
	Propeller Synchrophaser
	C
	1
	0
	
	

	
	
	
	
	
	
	



