5/1/13  A/C TT 8037.9  N306MH
Performed: 50, 100, 200, 300 Hr inspections. Replaced all oils and hydraulic fluid.
300Hr Hydraulic filter replacement.
1200 Hr; pilots cyclic stick, T/R long control tube nylatron sleeves, Tailboom inspection.
600 Hr Nicad oil filter bypass check and filter replacement.
730 day ELT battery inspection.
1 month Fire Ext inspection.
180 day float inspection and repack.
36 month float bottle hydro test.
180 day float electrical inflation valve test.
Replaced side crush panel under the pilots side access panel P/N 206-031-120-017S.
Removed mold from beneath baggage compartment.
Adjusted cyclic, collective & Tail Rotor minimum friction.
Adjusted swashplate friction by max torqueing bolts.
Replaced fuel control arm bolt with new P/N NAS6604D8.
Complied with ASB 206L-99-115, 206L-09-158 & AD 2002-25-07, CEB A-73-3075.
Performed M/R & T/R track and balance with RADS system. Installed and removed RADS on T/R and M/R system.
All Work performed in accordance with applicable:  Maritime Helicopters checklists, BHT 206L M.M., CR&O.M, 
Rolls Royce 250 C30P M.M, BHT Corrosion Control Guide &  AC43.13-1B/2B,
Performed ground run and leak check. Operational check flight required
Retorque on T/R short shaft coupling hardware due      8047.9 - 8062.9
This aircraft/engine has been inspected/repaired in accordance with current regulations and is approved for return to service.
Details on file at Maritime Helicopters under WO # 2655
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