	6/27/13  A/C TT 8132.2 N306MH
Performed:  50 lube, 100, Hr Airframe inspection.
150, 300, 600, 2000Hr Engine inspections.
1500 hr freewheeling unit insp.
Performed 100Hr/ 90 day Corrosion Control inspection.
Complied with Engine oil change over to Royco 560 oil
1 month fire Ext inspection.
7 day M/R blade insp
Complied with ASB 206L-09-158 T/B fitting
Complied with CEB A-73-3075 FCU screws
Complied with 1500 hour Bleed Valve insp by installing O/H Bleed Valve
Removed bleed Valve P/N 23073353 S/N FF57427, 
Installed O/H same P/N Bleed Valve S/N FF36235
Complied with 12500 hour Impeller insp by installing serviceable Compressor
Removed Engine Assy and Reinstalled same Assy S/N for 1,2,3,4,wheels retire
Removed Engine Compressor Assy P/N 23033193 S/N CAC91445  
Installed Serviceable Compressor P/N 23033193 S/N CAC91334
Removed Engine Turbine Assy P/N 23035128 S/N CAT98521
Installed O/H Turbine Assy P/N 23035128 S/N CAT97928
1. T/R short shaft coupling re-torque due  between 8142.2 – 8157.2
Performed ground run and leak check. Operational check flight required
Performed Engine “ check run “ procedures.
All work performed in accordance with applicable BHT 206L3 M.M, CR&O, SPM. AC 43.13-2B.
This aircraft/engine has been inspected/repaired in accordance with current regulations and is approved for return to service. Details on file at Maritime Helicopters under WO # 2662

CRS# ENRR619D  ______________________________________

	6/27/13  A/C TT 8132.2 N306MH
Performed:  50 lube, 100, Hr Airframe inspection.
150, 300, 600, 2000Hr Engine inspections.
1500 hr freewheeling unit insp.
Performed 100Hr/ 90 day Corrosion Control inspection.
Complied with Engine oil change over to Royco 560 oil
1 month fire Ext inspection.
7 day M/R blade insp
Complied with ASB 206L-09-158 T/B fitting
Complied with CEB A-73-3075 FCU screws
Complied with 1500 hour Bleed Valve insp by installing O/H Bleed Valve
Removed bleed Valve P/N 23073353 S/N FF57427, 
Installed O/H same P/N Bleed Valve S/N FF36235
Complied with 12500 hour Impeller insp by installing serviceable Compressor
Removed Engine Assy and Reinstalled same Assy S/N for 1,2,3,4,wheels retire
Removed Engine Compressor Assy P/N 23033193 S/N CAC91445  
Installed Serviceable Compressor P/N 23033193 S/N CAC91334
Removed Engine Turbine Assy P/N 23035128 S/N CAT98521
Installed O/H Turbine Assy P/N 23035128 S/N CAT97928
1. T/R short shaft coupling re-torque due  between 8142.2 – 8157.2
Performed ground run and leak check. Operational check flight required
Performed Engine “ check run “ procedures.
All work performed in accordance with applicable BHT 206L3 M.M, CR&O, SPM. AC 43.13-2B.
This aircraft/engine has been inspected/repaired in accordance with current regulations and is approved for return to service. Details on file at Maritime Helicopters under WO # 2662

CRS# ENRR619D  ______________________________________


	6/27/13  A/C TT 8132.2 N306MH
Performed:  50 lube, 100, Hr Airframe inspection.
150, 300, 600, 2000Hr Engine inspections.
1500 hr freewheeling unit insp.
Performed 100Hr/ 90 day Corrosion Control inspection.
Complied with Engine oil change over to Royco 560 oil
1 month fire Ext inspection.
7 day M/R blade insp
Complied with ASB 206L-09-158 T/B fitting
Complied with CEB A-73-3075 FCU screws
Complied with 1500 hour Bleed Valve insp by installing O/H Bleed Valve
Removed bleed Valve P/N 23073353 S/N FF57427, 
Installed O/H same P/N Bleed Valve S/N FF36235
Complied with 12500 hour Impeller insp by installing serviceable Compressor
Removed Engine Assy and Reinstalled same Assy S/N for 1,2,3,4,wheels retire
Removed Engine Compressor Assy P/N 23033193 S/N CAC91445  
Installed Serviceable Compressor P/N 23033193 S/N CAC91334
Removed Engine Turbine Assy P/N 23035128 S/N CAT98521
Installed O/H Turbine Assy P/N 23035128 S/N CAT97928
1. T/R short shaft coupling re-torque due  between 8142.2 – 8157.2
Performed ground run and leak check. Operational check flight required
Performed Engine “ check run “ procedures.
All work performed in accordance with applicable BHT 206L3 M.M, CR&O, SPM. AC 43.13-2B.
This aircraft/engine has been inspected/repaired in accordance with current regulations and is approved for return to service. Details on file at Maritime Helicopters under WO # 2662

CRS# ENRR619D  ______________________________________

	6/27/13  A/C TT 8132.2 N306MH
Performed:  50 lube, 100, Hr Airframe inspection.
150, 300, 600, 2000Hr Engine inspections.
1500 hr freewheeling unit insp.
Performed 100Hr/ 90 day Corrosion Control inspection.
Complied with Engine oil change over to Royco 560 oil
1 month fire Ext inspection.
7 day M/R blade insp
Complied with ASB 206L-09-158 T/B fitting
Complied with CEB A-73-3075 FCU screws
Complied with 1500 hour Bleed Valve insp by installing O/H Bleed Valve
Removed bleed Valve P/N 23073353 S/N FF57427, 
Installed O/H same P/N Bleed Valve S/N FF36235
Complied with 12500 hour Impeller insp by installing serviceable Compressor
Removed Engine Assy and Reinstalled same Assy S/N for 1,2,3,4,wheels retire
Removed Engine Compressor Assy P/N 23033193 S/N CAC91445  
Installed Serviceable Compressor P/N 23033193 S/N CAC91334
Removed Engine Turbine Assy P/N 23035128 S/N CAT98521
Installed O/H Turbine Assy P/N 23035128 S/N CAT97928
1. T/R short shaft coupling re-torque due  between 8142.2 – 8157.2
Performed ground run and leak check. Operational check flight required
Performed Engine “ check run “ procedures.
All work performed in accordance with applicable BHT 206L3 M.M, CR&O, SPM. AC 43.13-2B.
This aircraft/engine has been inspected/repaired in accordance with current regulations and is approved for return to service. Details on file at Maritime Helicopters under WO # 2662

CRS# ENRR619D  ______________________________________




