4/4/13 A/C TT 12821.2

Performed 50/100/200/300hr inspections as per Maritime Helicopters Checklist BHT-206L Series, BHT 206L-3 MM/Rolls Royce 250
C-30P MM instructions and procedures. 
The following maintenance was performed:
1. Removed Retention Straps P/N 206-001-154-107, S/N’s LP56422/LP56406, installed new improved retention straps(calendar life now 36 months)  P/N 206-310-004-103,  S/N’s LPFS0407/LPFS0406.
2. Removed Main Rotor retention strap pin’s P/N 206-011-125-001 S/N’s OP7394/OP8308, installed new pins P/N SAME S/N’s DI37508/DI37679,Removed Main Rotor retention bolts P/N 206-011-260-101 S/N’s DI23450/DI23481, installed new bolts P/N SAME, S/N’s SU7958/SU7750,Performed 1200 Hours of Component Inspection on M/R Hub S/N A-253.
3.  Removed Freewheeling Unit Assembly P/N 206-040-270-009 S/N BMB45936. Installed Overhauled Freewheeling Unit Assembly  P/N 206-040-270-009 S/N BMB45696. Removed Freewheeling Unit Clutch P/N CL42250-1 S/N FD17840. Installed Freewheeling Unit Clutch P/N CL42250-1 S/N FD18256. All work performed reference Able Engineering W/O NM051116VX.
4. Removed and replaced engine compressor assembly due to mandatory 2000 hour inspection requirement.  P/N Removed 23051643 S/N CAC-91334. P/N Installed 23051643 S/N CAC-90716. Reference W/O# 32-09769.
5. C/W engine 2000 hour inspection. Reference W/O# 32-09769. Replaced Combustion Liner Assembly due to cracking. P/N Removed 23066675 S/N TR3-073.  Installed P/N 23066675 S/N 1-97-13. All work performed by Aero Weld reference W/O APG-11213.

Main rotor system balanced with marvel balancer to within manufacturers prescribed limits. Main rotor tracked to within manufacturers prescribed limits. Tail rotor balanced to within .1 IPS. Ground run and leak checks performed for above maintenance performed. All work done in accordance with BHT 206L-3 MM, CR&O, and Rolls Royce 250-C30P MM instructions and procedures.
Flight Check required prior to release for service.

1. Mast Nut Re-Torque 12822.2-12827.2
2. Pillow Block Re-Torque    12823.2-12829.2


Operational check flight required. 
This aircraft/engine has been inspected/repaired in accordance with current regulations and is approved for return to service. Details on file at Maritime Helicopters under WO # 2641.
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