4/26/13  A/C TT 1083.9  N309MH
Performed: 12 month Annual,  50, 100, 200, 300 Hr Airframe inspections. Replaced all oils and hydraulic fluid.
300 Hr Tailboom inspection.
150,  300 Hr Engine inspection.
100, 300 Hr, 12 month Barrier filter clean and inspections. Applied new oil to filter.
600Hr, 6 month M/R blade cleaning inspections. R&R M/R blades to FOM. Cleaned, inspected & Lubed bolts and blade bolts holes.
600 Hr Rotor brake inspection. Installed new o-rings in calipers.
Performed 100Hr/ 90 day Corrosion Control inspection.
300Hr/ 12 month & 24 month Fuel Cell & Aux fuel Cell Cleaning and inspection. Minimum debri found in cells.
1 month, 12 month fire Ext inspection.
12 month: Mast inspection, Elt operational check, Chelton operational checks, 
12 month/ 500Hr emergency float checks. Hydro previously completed 05/12.
24 month: Aircraft reweigh, compass calibration, CEFA filter element replacement, fuel quantity calibration.
27 month pyrotechnic signal device replacement, inspection.
Complied with ASB,s 407-11-94, 407-11-95 pt 2, 407-08-84, 407-10-93, 407-13-99.
Replaced Hydraulic filters. Complied with Compressor wash.
Removed FWU, installed new Eng. G/B fwd and aft seals P/N 23079072. Reinstalled FWU.
Replaced R/S rear cabin door upper A/F mounted upper striker.
R&R M/R Drive shaft to FOM. Replaced ELT horn battery with new battery.
Replaced 4ea bolts with new P/N MS21250H4007 on M/R hub lower cone set.
Replaced 1ea bolt on orange M/R  P/C link upper bolt with new P/N NAS6705AD38.
Adjusted M/R swashplate  friction by max torqueing  adjustment bolts.
Removed high skid landing gear P/N 407-724-101 S/N 5370, installed high skid landing gear with emergency floats P/N
407-724-101 S/N 5272. Installed Bear Paws from removed Landing Gear.
Completed: Paravion, Tanis, Alpine, Dart, Aeronautical Accessories, ICA’s  IAW applicable Manufactures M.M.
Aerospace Filtration Systems M.M.
1. Mast nut re-torque                                                     1084.9 – 1088.9
2. M/R Hub lower cone bolts re-torque                     1084.9 – 1088.9
3. T/R short shaft coupling re-torque                         1093.9 – 1108.9
4. Tension check on expandable M/R blade bolts   1103.9 – 1113.9  
 Performed M/R & T/R track and balance with RADS system. Installed and removed RADS on T/R and M/R system.
Performed ground run and leak check. Operational check flight required.
This aircraft/engine has been inspected/repaired in accordance with current regulations and is approved for return to service. Details on file at Maritime Helicopters under WO # 2637
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