	MARITIME HELICOPTERS
	DHC-6-400 FLIGHT CREWMEMBER rii repairmen TASKs

	
	

	Page No:
	1

	Revision:
	Original

	Issue Date:
	06/01/20

	AIRCRAFT:
	
	R 04 – DHC-6-400

	TYPE:
	
	RII TASK CARD

	TASK:
	
	Propeller Installation



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	RII
REPAIRMENS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R 04.1 GENERAL

	
	
	

	1.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	1.2 Check for entry in the discrepancy section of the log book/Work Order for RII due. At a minimum the log book entry shall contain the following: A description stating that the RII for the maintenance item is due. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	R 04.2 PRIOR TO STARTING TASK

	
	
	

	2.1 Verify any new parts used have correct paperwork.
	
	

	
	
	

	2.2 New mounting bolt must be used when initially installing a new or overhauled propeller.
	
	

	NOTE: Mounting bolts and washers may be reused if not damaged or corroded if propeller is removed between overhaul intervals.
	
	

	2.3 Inspect all calibrated tool’s inspection decal that will be used in the task to confirm it is in current calibration.
	
	

	
	
	

	2.4 Verify that any new P/N used is compatible with aircraft S/N.
	
	

	
	
	

	2.5 Read the Viking and Hartzell MM sections describing the task.
	
	

	
	
	

	2.6 Verify;
	

	
	

	2.6.1 Spinner dome is removed.
	
	

	
	
	

	2.6.2 Sling is properly attached and is rated to 800 lbs to support the weight of the propeller assembly.
	
	

	
	
	

	2.6.3 Propeller is put in feather position.
	
	

	
	
	

	2.6.4 Ensure propeller and engine flanges are clean and free from scoring or burring which could prevent mating.
	
	

	
	
	

	R 04.3  INPROCESS INSPECTIONS

	
	

	3.1 Verify; 
	

	
	

	3.1.1 Propeller is being installed I/A/W Hartzell Owner’s Manual 139 (61-00-39).
	
	

	
	
	

	3.1.2 Hub to engine and spacer O-rings are installed.
	
	

	
	
	


	
	
	RII

REPAIRMENS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	3.1.3 Mounting bolts torqued to correct amount and proper sequence I/A/W Hartzell Torque Table 3-2.
	
	

	
	
	

	3.1.4 Safeties are in place and tight on all mounting bolts.
	
	

	
	
	

	3.1.5 Beta ring is not in contact with any engine component or mounting bolt safety wire.
	
	

	
	
	

	R 04.4 POST TASK INSPECTIONS

	
	
	

	4.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	4.2 Verify;
	
	

	
	
	

	4.2.1 Spinner dome is installed, correctly torqued and has correct clearance.
	
	

	
	
	

	4.2.2 Perform initial run-up to released trapped air from the propeller.
	
	

	
	
	

	4.2.3 POC performs ground idle checks and that it is entered into the aircraft Log Book.
	
	

	
	
	


Upon satisfactory completion of each inspection item, the RII Repairmen shall initial the pertinent space as provided.  All RII Repairmen shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form the RII Repairmen shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  
This form shall be attached to the aircraft log book page.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I certify that I have used this RII card throughout the inspection process and have made an entry into the aircraft log book.
RII Repairmen Signature; ______________________________  

RII REPAIRMEN INSPECTION AUTHORIZATION CARD CERTIFICATE NUMBER; ____________________________

