	MARITIME HELICOPTERS
	DHC-6-400 FLIGHT CREWMEMBER rii repairmen TASKs

	
	

	Page No:
	1

	Revision:
	Original

	Issue Date:
	06/01/20

	AIRCRAFT:
	
	R 05 – DHC-6-400

	TYPE:
	
	RII TASK CARD

	TASK:
	
	Engine/Propeller Control Rigging



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	RII
REPAIRMENS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R 05.1 GENERAL

	
	
	

	1.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	1.2 Check for entry in the discrepancy section of the log book/Work Order for RII due. At a minimum the log book entry shall contain the following: A description stating that the RII for the maintenance item is due. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	R 05.2 PRIOR TO STARTING TASK

	
	
	

	2.1 Verify any new parts used have correct paperwork.
	
	

	
	
	

	2.2 Inspect all calibrated tool’s inspection decal that will be used in the task to confirm it is in current calibration.
	
	

	
	
	

	2.3 Verify that any new P/N used is compatible with aircraft S/N.
	
	

	
	
	

	2.4 Read the Viking MM sections describing the task.
	
	

	
	
	

	R 05.3  INPROCESS INSPECTIONS

	
	

	3.1 Verify; 
	

	
	

	3.1.1 Cable tension and friction checks are correct as applicable.
	
	

	
	
	

	3.1.2 All control hardware is tightened and safetied.
	
	

	
	
	

	3.1.3 Correct torque was used on control tube jam nuts.
	
	

	
	
	

	3.1.4 Control tube rod ends are adjusted so both ends are centered on bellcranks allowing the maximum rotation of the control tube.
	
	

	
	
	

	3.1.5 All locknuts are tightened and torqued.
	
	

	
	
	

	3.1.6 Safeties are in place and tight on all turnbuckles, attachments, stop bolts and all control hardware.
	
	

	
	
	

	3.1.7 Lubrication applied as needed.
	
	

	
	
	


	
	
	RII

REPAIRMENS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	3.1.8 All rigging pins are removed.
	
	

	
	
	

	R 05.4 POST TASK INSPECTIONS

	
	
	

	4.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	4.2 Verify;
	
	

	
	
	

	4.2.1 Smooth operation of levers through the entire range of motion, no binding.
	
	

	
	
	

	4.2.2 Ensure all applicable hardware is secured.
	
	

	
	
	

	4.2.3 All cowlings, access panels are installed and secure.
	
	

	
	
	

	4.2.4 POC performs ground checks, Idle speeds are correct.
	
	

	
	
	

	4.2.5 Engine run performed I/A/W 71-00-00 Power Plant and that it is entered into the aircraft Log Book.
	
	

	
	
	


Upon satisfactory completion of each inspection item, the RII Repairmen shall initial the pertinent space as provided.  All RII Repairmen shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form the RII Repairmen shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  
This form shall be attached to the aircraft log book page.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I certify that I have used this RII card throughout the inspection process and have made an entry into the aircraft log book.
RII Repairmen Signature; ______________________________  

RII REPAIRMEN INSPECTION AUTHORIZATION CARD CERTIFICATE NUMBER; ____________________________

