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206L SERIES CALM VERIFICATION CHECKLIST

[bookmark: _Toc357159201]

6 MONTH AIRCRAFT HISTORICAL RECORDS ACCURACY VERIFICATION CHECK

The Maintenance Department shall be responsible for maintaining accurate historical records of all time controlled items installed on all Maritime Helicopters Inc. aircraft. This includes component serial numbers and total time in hours, cycles, calendar time, take offs, and retirement index numbers (RIN).

In order to maintain accurate serial number accountability, each aircraft is physically checked for corresponding serial numbers using the provided checklist. The records check, including the serial number check must be done post 12 month maintenance to capture all the new components going into service. This check shall be completed every 6 months using the attached checklist. 

The manufactures overhaul, inspection, lube, and retirement intervals shall be reviewed and compared to the latest CALM report to ensure any changes made by the manufacturer have been correctly reflected in CALM.  

The serial number report information is then compared against the latest CALM report and the aircraft historical service records to ensure that the serial numbers and times of all components are in agreement.

This will include:
· Proper entry of the last O/H 
· Proper entry of the last inspection performed
· Verifying component TT, TSO, and TSI are reflected in CALM
· Verifying all AD’s, ASB’s, and TB’s are entered and properly signed off on the component record.
· Verifying install and removal dates and times are entered on the record as applicable.

When any maintenance, overhaul, inspection, airworthiness directive or bulletin compliance is accomplished, an entry shall be made in the aircraft Historical Service Record as necessary.






Inspections


Aircraft N#__________	   Date ___________  
									
	N/A any box if not applicable
	Intervals (Acft TT)
	VARIFICATION ALL AGREE √

	Inspection
	Last C/W
	Due
	CALM
	Hard Card
	Log/WO Entry
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Components


Aircraft N#__________			Date ___________

	N/A any box if not applicable
	Verify with Hard Card and CALM
	VARIFICATION ALL AGREE √

	Component
	Part Number
	S/N
	CALM
	Hard Card
	Log/WO Entry

	Airframe
	
	
	
	
	

	Tailboom Assembly
	
	
	
	
	

	Cargo Hook
	
	
	
	
	

	Forward Crosstube
	
	
	
	
	

	Aft Crosstube
	
	
	
	
	

	Aircraft Battery
	
	
	
	
	

	Hydraulic Servo
	
	
	
	
	

	Hydraulic Servo
	
	
	
	
	

	Hydraulic Servo
	
	
	
	
	

	R/H Cyclic Tube
	
	
	
	
	

	L/H Cyclic Tube
	
	
	
	
	

	Collective Tube
	
	
	
	
	

	M/R Head Assembly
	
	
	
	
	

	Trunnion
	
	
	
	
	

	M/R Grip
	
	
	
	
	

	M/R Grip
	
	
	
	
	

	M/R Blade
	
	
	
	
	

	M/R Blade
	
	
	
	
	

	Mast Assembly
	
	
	
	
	

	Mast Pole
	
	
	
	
	

	Swashplate
	
	
	
	
	

	Transmission
	
	
	
	
	

	Hydraulic Pump
	
	
	
	
	

	Input Driveshaft
	
	
	
	
	

	Freewheeling Unit
	
	
	
	
	

	Rotor Brake Caliper 
	
	
	
	
	

	Rotor Brake Caliper
	
	
	
	
	

	Rotor Brake Disk
	
	
	
	
	

	T/R Hub Assembly
	
	
	
	
	

	T/R Yoke
	
	
	
	
	

	T/R Blade
	
	
	
	
	

	T/R Blade
	
	
	
	
	

	T/R Gearbox
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Components(Cont)




	N/A any box if not applicable
	Verify with Hard Card and CALM
	VARIFICATION ALL AGREE √

	Component
	Part Number
	S/N
	CALM
	Hard Card
	Log/WO Entry

	Engine
	
	
	
	
	

	Compressor
	
	
	
	
	

	Turbine
	
	
	
	
	

	Gearbox
	
	
	
	
	

	Starter/Generator
	
	
	
	
	

	Fuel Nozzle
	
	
	
	
	

	Fuel Pump
	
	
	
	
	

	Fuel Control
	
	
	
	
	

	Governor
	
	
	
	
	

	Bleed Valve
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	If Installed;
	
	
	
	
	

	FLOAT BOTTLE
	
	
	
	
	

	FLOAT BOTTLE VALVE
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