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INSPECTIONS EXCLUDED FROM AAIP 
Since the AAIP inspection program is not intended to prescribe maintenance functions, the following items will be tracked separately in the aircraft status report. 

A. Hand-held Fire Extinguishers
B. Static System and Altitude Reporting System per 14 CFR 91.411.
C. ATC Transponder Test and Inspections per 14 CFR 91.413.
D. Inspect Pitot-Static System per 14 CFR 91.411/413 
E. Main Transmission Oil Change

F. Tail Rotor 90 Degree Gearbox Oil Change
G. Levers of Main and Tail Rotor Servo Actuator lubrication

H. Main Rotor Dampers (4 places)

I. Tail Rotor Gearbox 2400 Hour Inspection – Now Tracked on CALM

J. Engine Fuel Pump 1500 Hour Inspection – Now Tracked on CALM

K. Compressor Bleed Valve 1500 Hour Inspection – Now Tracked on CALM


