Summary of Changes
Global – Reverted back to sectional pagination
Combined A 0007 & E 0007 7-day inspections into one (1) – R 0007
A 0125
5.2 & 6.2 - Removed AD, not applicable to -400 
5.4 & 6.4- Added nicks and cracks, blend nicks/cracks
5.5 & 6.5 - Gas generator part of insp moved to 77 – ENGINE CONTROLS
5.6 & 6.6 - Propeller Synchronizer is not installed on our aircraft. Replaced with shaft seal insp.
7.2 & 8.2 – Added additional inspection items
9.2 & 10.2 – Added additional inspection items
9.4 & 10.4 – Added scavenge pump insp
11.1 & 12.1 – Removed AD, N/A our aircraft
11.4 & 12.4 – Added additional inspection items, Removed AD, N/A our aircraft
11.5 & 12.5 – Added additional items
11.6 & 12.6 – Added additional inspection item
11.7 & 12.7 – Added additional inspection item
13.1 & 14.1 – Removed AD & SB NOTE, N/A our aircraft
15.2 & 16.2 – Added Gas Gen Tach from 5.5 & 5.6, removed Prop Gen
17.3 & 18.3 – Added additional inspection items
19.2 & 20.2 – Modified wording for our configuration

B 0250

B 0250.5 – Removed, no A/C installed
7.1 – Removed, not installed
B 0250.12/13 – 28-FUEL LH & RH removed.  No wing tanks installed. 12.2 & 13.2 already in A 0125
B 0250.24/25 – 61 – PROPELLERS LH & RH removed.  Insp already in lower frequency A 0125
B 0250.19/20 – Added Chip Det inspection to the 72-ENGINE (from P 0100)





