MARITIME HELICOPTERS PRE-WEIGHING CHECK LIST


STATION_____________ DATE______________ A/C NO. N____________ MECH ____________

1. Empty all fuel tanks and drain sumps	
2. Service both engine oil tanks to full	
3. Service hydraulic tanks to normal full	
4. Portable fire extinguishers (2 required)	.
5. Remove all operating items. (List on back of sheet for replacement)	
6. Aircraft clean, exterior and interior	
7. Cargo Nets Installed (Flight Configuration)	
8. First Aid kit, Life Vests and Survival Kit installed	
9. All crew member seats installed	
10. Position flaps up and all controls neutral. Use seat belts to hold yoke	
11. Prop locks and engine inlet covers removed	
12. Aircraft jacked to level condition	
13. Scales properly calibrated, warmed, and zeroed	

AIRCRAFT READY TO BE WEIGHED ____________________ INSP. _________________________
