Ensure the kit is complete.
Verify paperwork for the mounts are for the actual type of camera to be installed. If there is no paper work, incomplete paper work or the wrong paperwork, the camera shall not be installed.
Check installation is complete I/A/W STC.
Check that the proper Flight Manual Supplement is inserted in RFM.
Check for any flight restrictions
Check if any required placards are in place
Ensure there is an updated Weight and Balance inserted into the RFM.

