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	Page No:
	3

	Revision:
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	Issue Date:
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	SECTION:
	
	R 03 – BELL 412 CAMP

	TYPE:
	
	RII TASK CARD

	TASL:
	
	Bell 412 90° Gearbox Install



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	RII
INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R 03.1 GENERAL

	
	
	

	1.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	1.2 Check for entry in the discrepancy section of the log book/Work Order for RII due. At a minimum the log book entry shall contain the following: A description stating that the RII for the maintenance item is due. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	R 03.2 PRIOR TO STARTING TASK

	
	
	

	2.1 Verify any new parts used have correct paperwork.
	
	

	
	
	

	2.2 Verify the maintenance manual is the correct revision number. Check MM revision number against the MHI master publications list.
	
	

	
	
	

	2.3 Check computer tracking system for any item or inspection that could be affected by the maintenance task.
	
	

	
	
	

	2.4 Inspect all calibrated tool’s inspection decal that will be used in the task to confirm it is in current calibration.
	
	

	
	
	

	2.5 Verify that any new P/N used is compatible with aircraft S/N.
	
	

	
	
	

	2.6 Read the MM section describing the task.
	
	

	
	
	

	2.7 Verify;
	

	
	

	2.7.1 POC required for installation of 90° gearbox is entered in aircraft Log Book.
	
	

	
	
	

	2.7.2 Post installation torque check is in logbook.
	
	

	
	
	

	2.7.3 Leak check is entered in log book.
	
	

	
	
	

	2.7.4 Flex couplings are lubricated. (Refer to Paperwork)
	
	

	
	
	

	2.7.5 Grease is not expired. (Refer to Paperwork)
	
	

	
	
	

	2.7.6 Backlash and absence of binding of input quill.
	Refer to MM.
	

	
	
	

	2.7.7 Oil was flushed if GB was preserved.
	
	

	
	
	


	
	
	RII

INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	2.8 Refer to RII task card for installation of Tail Rotor Drive Shaft.
	
	

	
	
	

	R 03.3 INPROCESS INSPECTIONS

	
	

	3.1 Verify;
	

	
	

	3.1.1 Mounting flange is free of sealant.
	
	

	
	
	

	3.1.2 Correct torque procedure is used.
	
	

	
	
	

	3.1.3 Proper torque of bolts.
	
	

	
	
	

	3.1.4 Correct thread length of stud through nut.
	
	

	
	
	

	3.1.5 Gap between shim and input quill is correct.
	
	

	
	
	

	3.1.6 TR pitch change mechanism washer stack up is correct.
	
	

	
	
	

	3.1.7 TR pitch change mechanism torque is correct.
	
	

	
	
	

	3.1.8 TR pitch change mechanism hardware is safety.
	
	

	
	
	

	R 03.4  POST TASK INSEPCTIONS

	
	
	

	4.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	4.2 Verify;
	

	
	

	4.2.1 Gear box is properly serviced.
	
	

	
	
	

	4.2.2 Correct run in procedure was done during the POC.
	
	

	
	
	

	4.2.3 Temp indicators have no indications after POC.
	
	

	
	
	


Upon satisfactory completion of each inspection item, the RII Inspector shall initial the pertinent space as provided.  All RII Inspectors shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form the RII Inspector shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  
This form shall be attached to the aircraft W.O./Log Book. 
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I certify that I have used this RII card throughout the inspection process and have made an entry into the aircraft log book.
RII Inspectors Signature; ______________________________  
RII INSPECTION AUTHORIZATION CARD CERTIFICATE NUMBER; ________________________________


