412 Highlights of Change

Globally – All pages changed to Reissue with a date of 11/15/20 due to large reorganization of manual.

Cover - Reissue

Table of Contents

Pg ii – Removed 2.2 Individual Responsibilities. (Addressed in the CAMP General Manual)
Removed 2.3 Mechanic Qualifications. (Addressed in the CAMP General Manual)
	2.4 Maintenance and Servicing now 2.2
Added 2.8 Airworthiness Check
	Removed 2.12 Contract Maintenance. (Addressed in the CAMP General Manual)
           	Added 2.13 Abbreviations (from old Rev Original Section 7)
Added 2.14 Definitions. (from old Rev Original Section 7)
Removed 4.2.2-4.2.4
Pg iii – Section 6 Now Weight and Balance Control. (Replaced CASS as it’s addressed in CAMP General Manual) 
Section 7 Abbreviations and Definitions incorporated in Section 2 Page ii. Now “Aircraft Log Page”
Section 8 – Now Inspections instead of “Forms”
Added additional ATTACHMENTS
Pg iv – Updated RECORD OF REVISIONS table, removed “Insertion Date” and “Posted by columns. (All MHI manuals now inserted and posted digitally online)
Pg vi – All pages Rev date changed as this manual is a reissue due to multiple additions and global changes. Added xiii, xiv. Removed Abbreviations and Definitions and Forms. Added Weight & Balance Control and Inspections also includes name changes from all noted above.
Pg vii – Removed A0101 -A0103. Now combined in A0120. A0305 moved to viii globally
Pg viii – ENGINE INSPECTION SECTION moved to ix to allow for future additions to AIRFRAME SECTION
Pg ix – Removed B0056, explanation on page. ICA INSPECTION SECTION moved to x
Pg x thru xii – Globally changed
Pg xiii & xiv Added due to Multiple Attachments C Thru F

Preamble

Pg 1-1 – Updated wording under INTRODUCTION to fall in line with a CAMP rather than an AAIP
Pg 2-1 – Removed 2,2 Individual Responsibilities. (Addressed in the CAMP General Manual)
	Removed 2.3 Mechanic Qualifications. (Addressed in the CAMP General Manual)
Replaced 2.4 MAINTENANCE AND SERVICING (now 2.2) with AIRWORTHINESS LIMITATION
2.5 EXCLUSIONS moved to 2.3
2.7 OVERHAUL TIME LIMITS moved to 2.5
	Removed 2.12 Contract Maintenance. (Addressed in the CAMP General Manual)
Pg 2-3 – Added 2.13 ABBREVIATION AND DEFINITIONS moved from Rev 0 7-1
Pg 2-4,5 – New pages. Moved Definitions from Revision 0 Chp 7, pages 7-2 & 3
Pg 3-1 – No changes
Pg 4-2 – Removed 4.2.2
Pg 4-3 – 4.2.3 thru 4.2.3.3 Removed – Covered in new employee training. Now SCHEDULE OF INSPECTIONS
Series A – Airframe Section Table
Pg 4-3 – Removed A0100 – A0103, added A 0120 (contains A0100 thru A0103)
Pg 4-4 – Deleted 4.2.4 Now SERIES B – POWERPLANT SCHEDULE OF INSPECTIONS
Series B – Engine Inspections Table
Pg 4-4 - B0056 Removed. Incorporated into Appx F Airworthiness Daily Inspection 7.16

Series C – Instructions for Continued Airworthiness Table
Pg 4-4 – Changed name of C 0301 to C 0350 to fall in line with AAIP/CAMP designations

Pg 5-1 thru 5-6 – No changes

Pg 6-1 – Replaced Section 6 CASS (Addressed in the CAMP General Manual) with Weight and Balance Control
Pg 7-1 – Abbreviations and Definitions moved (see above) replaced with Aircraft Log page
Pg 8-1 – Changed from FORMS to heading page for the A, B and C Series inspections section.


Airframe Inspections

A 0025 has updates, many items moved to Airworthiness Check, Appx F-1, global changes to pages.
A0100 – Removed. Battery inspections covered in A-0025.4 and on F-4 Daily Airworthiness Check
A0101-A0103 Removed, now combined into A0120 100 hr /120 Day Insp
A0120 – Added to consolidate A0101 – A0103
A0306 - Para 5.1.1 and 5.1.5 from Rev 0 are N/A for our aircraft. We do not have elastomeric rod ends on any flight control rod end. A0306.6 added.
No other changes were made to any remaining Airframe Inspections other than Revision # and Date

Engine Inspections

B0056 – Removed. Incorporated into Appx F Airworthiness Daily Inspection 7.16
No other changes were made to any remaining Engine Inspections other than Revision # and Date
B0100 Para 6.1- not required because we have post SB5398 fuel surge accumulators
B0100 Para 6.2- perform engine deceleration ck not required for our engines. IAW 71-00-00 para O, and SB 5398
B0150- Para 5.6.2 and Para 5.6.4 removed - we have post SB5354 chip detectors (quick disconnect style)
B0156 – Corrected numeration issues on B0156 5 and 6
B0312- Para 5.7.1 note removed and fuel pump gear set and coupling now tracked on CALM because different pumps have different TSN
B0312- Para 5.10 and Para 5.11 note removed. This statement is not required because the inspection is for chip detectors not the entire engine
B0600.6 – Removed - inspection of seam welds is not required on MHI engines. IAW SB5239 effectivity of SB is for PT6T-3 & 3B engines only
B1200RT- Para 5.2.- inspection of seam welds is not required IAW SB5239

ICA Inspections

C 0301 name changed to C 0350
No other changes were made to ICA Inspections other than Revision Name and Date

Appendices
Pg A-1 – Removed R34, was a repeat of R01
Attachment B – Added 300 Hour / 12 Month Fuel Pump Insp – Tracked on CALM against SB5003
Added the following Attachments;
C – Airworthiness Limitations   
D – Lubrication Schedule
E – After Maintenance Checks
F – Airworthiness Check (Daily)




