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REQUIRED INSPECTION ITEM

INSPECTION AUTHORITY EXAMINATION

Select an answer from the choices given that most correctly completes the statement or answers the question. There is no time limit.

1. It is the responsibility of the __________ to keep RII manuals and checklists current at all times.

A. Technical Trainer

B. Chief Inspector

C. Manual Holder

D. Director of Maintenance
Note; there is no such item as a RII manual. 

Question to ask: How would you know if the checklist is current?
2. What is the difference between an SCC and an RII?

A. An SCC is accomplished by pilots only, RII is accomplished by mechanics.

B. An SCC is accomplished for any Bristow aircraft; an RII is for certain items on CAMP maintained aircraft.

C. An SCC is required for aircraft maintained under AAIP but not for aircraft maintained under CAMP.

D. An SCC is accomplished for CAMP maintained aircraft while an RII is accomplished for AAIP maintained aircraft.

3. In what publication does it explain when to do an RII?

A. Repair Station Manual

B. Operations Manual

C. General Maintenance Manual

D. Appendix E of the GMM Bell 412 Continued Airworthiness Maintenance Program
4. A MR pitch link was reconnected during MR blade folding. Whose signature would be required for the approval to return the aircraft to service after maintenance prior to carrying passengers?
A. The mechanic signing the corrective action for unfolding the MR blades.
B. The RII inspector signing the RII for unfolding the MR blade. 

C. Both A. and B.
D. The pilot signing the of the MOC 
Note: the pilot signing the MOC is returning the aircraft to service not approving it for return to service.

Discussion: Does a MOC need to written up for a PC link?
5.
In what publication would you find the FAA accepted procedures referenced during the RII inspection of a tail rotor assembly installation on a bell 412?

A. Bristow Alaska Inc. GMM
B. Bristow Alaska GMM Appendix S supplementary forms manual
C. Bell 412 Maintenance manual

D. Bell 412 component overhaul manual

Note: supplementary forms are not accepted or approved. They are only to be used as a guide.
6.
Two mechanics change a power section on a Bell 412. The senior mechanic is RII rated for the Bell 412. The senior mechanic signs the RII in the log book. What else must be done prior to flight in the RII procedures?
An RII inspection must be performed because the mechanic doing the work cannot perform the RII.
7.
A pilot RII is asked to come and do an inspection on a tail rotor drive shaft hanger bearing repack that was just completed. What must be done prior to signing off the RII.
A. Task card must be started.
B. Mechanic must disassemble coupling to show RII in process inspections.
C. The hanger discrepancy must be signed off
D. All of the above
Note: Task cards are to be used during the entire process, Mechanic must disassemble the hanger to the extent that the RII inspector can see the critical steps, and the discrepancy must be signed off.
8.
Ensuring the following item is a responsibility of the RII inspector.
A. Proper part number was installed
B. All the discrepancies on the log page are signed off
C. Verify the MOC is complied with
D. All of the above
Note: There can be other open discrepancies on the log page as long as they don’t pertain to the RII. It is not the responsibility of the RII to ensure the MOC gets completed. Their responsibility is to ensure it is written up.
9.
An RII is required for which of the following tasks on a Bell 412SP?

A. Windshield replacement.

B. Anti-ice valve replacement.

C. Float installation.

D. Adjustment of the throttle twist grip.

10.
An R.I.I. Inspector, along with ensuring the work is properly done, is also responsible for the entry in the logbook being correct in all details.

A. True

B. False

11.
R.I.I. Inspectors may not inspect their own work.

A. True

B. False

12.
When performing the duties of a mechanic, an mechanic R.I.I. Inspector works for the 135 Chief Inspector. 

A. True

B. False

Note: he is a mechanic working for the DOM
13.
Any mechanic with over two years experience on a type of aircraft may perform the duties of an R.I.I. Inspector.

A. True

B. False 

14.
When the chief inspector signs your R.I.I. Authorization card, Bristow has authorized you to perform R.I.I. inspections on Bell 412.

A. True

B. False

True if you’re a mechanic

False if you are a pilot

Note: the FAA must sign the pilots
15.
When you sign the R.I.I. Authorization card, you show your acceptance of the responsibilities for an R.I.I. Inspector.

A. True

B. False

16.
When would an RII be required to write up a “buy back procedure”?
If an item has to be redone to your satisfaction and you will not be there to see it to completion there must be an entry in the log book for a the Buy Back.
17.
As per the FAR’s what is the minimum qualifications required for a pilot to perform RII?

A. Must be checked out as captain in the type of aircraft performing RII

B. Must be a checked out as a co-pilot in the type of aircraft performing RII

C. Must have a ATP

D. None of the above

Note: Bristow policy is must be a captain in type
18.
Repacking floats requires an R.I.I. Inspection.

A. True 

B. False

19.
When performing the duties of an R.I.I. Inspector at the repair station, the inspector works directly for the 145 Chief Inspector.
A. False
B. True

Note: When the repair station is doing maintenance for an air carrier it must follow the guidelines, use the forms, and get permission from the air carrier. It must also keep a roster of who is authorized at the repair station to do RII inspections on that airframe but the RII inspector is still working for the repair station and not the air carrier. Refer to FAR 145.205(a) and FSIMS 8900.1 Vol 6 sec 15 general and procedures B sections.
Note: pilots cannot perform RII inspections at the repair station.
20.
Who is ultimately responsible to ensure the work done on an aircraft was performed in a way not to jeopardize the safety of the aircraft.
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RII ITEM IDENTIFIER WORKSHEET
Using the aircraft discrepancy on your sample log book page, create a RII task card for that item.
Name__________________________________________________
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