Capabilities List


5.3 Capability List (CL). 

5.3.1 References: 
• Section 145.209(d). 
• Section 145.215. 

5.3.2 CL. A certificated repair station (CRS) with a limited rating may perform maintenance, preventive maintenance, or alterations on an article if it is listed on a current CL acceptable to the FAA or on the repair station’s operations specifications (OpSpecs). If the repair station chooses to use a CL, the RSM must: 
1. Contain procedures for revising the list and notifying the responsible Flight Standards office; 
2. Include how often the responsible Flight Standards office will be notified of revisions; 
3. Contain the procedures for the self-evaluation required under § 145.215(c) for revising the CL; 
4. Describe the methods and frequency of such evaluations; and 
5. Contain the procedures for reporting the results to the appropriate manager for review and action. 

5.3.3 Revising the List. The CL itself may be included as a part of the RSM, but it is suggested that it be made a separate document for ease in revising the list without the need to revise the RSM; however, the procedures for performing the self-evaluation, revising the list, and making those revisions available to the FAA must be included in the manual. 

5.3.4 Self-Evaluation. 

5.3.4.1 The individual performing the self-evaluation required under § 145.215(c) should have the following qualifications: 

1. Experience with performing evaluations (or audits, if that is the method selected by the repair station). 
2. An understanding of the requirements of part 145. 
3. Knowledge of the maintenance requirements for the particular make/model of the article to be added to the list.
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5.3.4.2 The individual must follow the procedures in the RSM for accomplishing a self-evaluation. Checklists, working documents, and forms designed by the repair station to record the self-evaluation should be included in the forms section of the manual system. The self-evaluation should ensure that the repair station has the following: 

1. The appropriate limited rating. 
2. Adequate housing and facilities. 
3. Recommended tools, equipment, and materials, or equivalent, as necessary to perform the maintenance in accordance with part 43. 
4. Current technical data. 
5. Sufficiently trained and qualified personnel. 
6. Completed self-evaluation records on file. 

5.3.5 Record and Report of Self-Evaluation Results. Procedures should be established for conducting the self-evaluation, recording and retaining the self-evaluation, and reporting the results to the appropriate repair station manager for review and action. The procedure used to revise the list should describe the method used to indicate any changes made to the list. Any deficiencies found during the self-evaluation should be corrected before the article can be added to the CL. When the self-evaluation establishes satisfactory results, the article may be placed on the CL. Notification of the revision to the list should be provided to the responsible Flight Standards office in accordance with the procedures required in § 145.209(d)(1). The repair station should retain documentation of the self-evaluation as long as the article is listed on the current CL. If the article was authorized in OpSpecs prior to establishing a CL, or the self-evaluation documents were missing, a baseline assessment should be documented for the current listing. For repair stations located outside the United States, the records of the self-evaluation may be in the national language; however, they must be made available to the FAA in English. 

5.3.6 Person Responsible for Maintaining the CL. The procedures for revising the CL and notifying the responsible Flight Standards office should include who (by title) is responsible for maintaining the CL and communicating any revisions to the office. If the self-evaluation was satisfactory, the CL may be revised. 

5.3.7 Maintaining the CL. CL currency can be shown by a List of Effective Pages (LEP) or equivalent document. The CL must identify each article by make and model or other nomenclature designated by the article’s manufacturer. 

5.3.8 Revising the CL. If the repair station no longer wishes to maintain an article on its CL, the article should be deleted. The repair station must have the necessary tools, equipment, housing, facilities, and trained personnel to maintain articles on the CL at the time the work is performed. The procedures in the manual should describe how to add and delete

5.3.9 Electronic Media. If the CL is maintained on electronic media, the repair station will need to work with the responsible Flight Standards office to ensure compatibility of the media, equipment, and software with that of the office. Revision procedures will need to address how the FAA will be notified of the revision. 

5.3.10 Procedures Guide. The following questions or concerns are offered as a guide and are intended to help initiate the procedures in the manual. They should not be considered all-encompassing. Each facility is unique and therefore may require additional procedures to verify regulatory requirements and the needs of the repair station. 

1. Who (by title) will maintain the CL? 
2. How will the self-evaluation be performed? 
3. Who (by title) will perform the self-evaluation? 
4. How will the self-evaluation be documented? 
5. How will results of the self-evaluation be reported to management and how will management review the addition of capabilities to the list? 
6. How will items be added to and deleted from the list? 
7. How are changes clearly indicated on the document? 
8. If electronic media is used, is the hardware and software compatible with that of the responsible Flight Standards office? 
9. Where and by whom will self-evaluation reports be maintained? 
10. Are the self-evaluations retained by the repair station for as long as an article is listed on the current CL and what is the time period of retention after an article is removed?

























