6-29-13 N 308MH WO # 2664 3175.7 A/F TT
Removed Engine due to metal flakes on chip Detectors .
Removed CAE847697 @ 3175.7 TT 5194 CSN.
Installed Rental CAE848035 @ 1656.1 TT 990.2 TSO 3386 CSN.
Fadec version V5202 installed with rental Eng.
Performed 50hr A/F  lube.
Performed 150, 300 hr Eng Insp
Performed 150 hr fadec Insp.
Perfromed 100hr Barrier filter Insp.
Cleaned, Insp, & lubed barrier filter. 
Complied with ASB 407-11-95 PT 2 T/B 
Complied with 100hr cargo hook Insp.
Operational check flight & Eng. Power check required. 
This aircraft/engine has been inspected/repaired in accordance with current regulations and is approved for return to service. Details on file at Maritime Helicopters under WO # 2664.
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